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Abstract
This contribution proposes specification text changes to the neural-network post filter characteristics SEI message to specify that the post-processing filter associated with the syntax element nnpfc_id is a neural network specified with information in a user data registered by Rec. ITU-T T.35 SEI message syntax structure, as agreed in response to item 2.a.iii in JVET-AB0193 in the JVET meeting on Thursday 20 October 2022 and further considered in the BoG on neural-network post-filter characteristics SEI message on Friday 21 October 2022 (JVET-AB0244).
Introduction
JVET-AB0193 provides a summary of all proposals on NNPF SEI messages, including those included in the VSEI CDAM ballot comments in MPEG input document m60678.
Item 2.a.iii of JVET-AB0193 is as follows:
2.a.iii.	Consider allowing the use of Rec. ITU-T T.35 data as an additional alternative way of identifying processing to be applied for this SEI message, since T.35 data is already supported in the standard and can fulfil a similar purpose. (BC#020)
During the JVET meeting on Thursday October 20 2022, the following was agreed on item 2.a.iii of JVET-AB0193: 
– agreed in principle that this could be useful, requires clarification if this should become a separate mode, and text needs to be developed (S. McCarthy will provide first draft - revisit).
During the BoG on neural-network post-filter characteristics SEI message on Friday 21 October 2022
(JVET-AB0244), action on item 2.a.iii of JVET-AB0193 was further considered as follows:
It was commented that the T.35 syntax structure should be copied into the NNPFC message when the nnpfc_mode_idc indicates signaling via T.35 syntax structure to resolve any ambiguity of which T.35 message has the NN data.
Revisit for the text in JVET.
This contribution proposes specification text changes responsive to the above.
Proposed changes to the specification text
The change marks are relative to JVET-AA2006-v2.
8.28 Neural-network post-filter characteristics SEI message
8.28.1 Neural-network post-filter characteristics SEI message syntax

	nn_post_filter_characteristics( payloadSize ) {
	Descriptor

		nnpfc_id
	ue(v)

		nnpfc_mode_idc
	ue(v)

		nnpfc_purpose_and_formatting_flag
	u(1)

		if( nnpfc_purpose_and_formatting_flag ) {
	

			nnpfc_purpose
	ue(v)

			if( nnpfc_purpose  = =  2  | |  nnpfc_purpose  = =  4 ) 
	

				nnpfc_out_sub_c_flag
	u(1)

			
	

			if( nnpfc_purpose  = =  3  | |  nnpfc_purpose  = =  4 ) {
	

				nnpfc_pic_width_in_luma_samples
	ue(v)

				nnpfc_pic_height_in_luma_samples
	ue(v)

			}
	

		/* input and output formatting */
	

			nnpfc_component_last_flag
	u(1)

			nnpfc_inp_format_flag
	u(1)

			if( nnpfc_inp_format_flag  = =  1 )
	

				nnpfc_inp_tensor_bitdepth_minus8
	ue(v)

			nnpfc_inp_order_idc
	ue(v)

			nnpfc_auxiliary_inp_idc
	ue(v)

			nnpfc_separate_colour_description_present_flag
	u(1)

			if( nnpfc_separate_colour_description_present_flag ) {
	

				nnpfc_colour_primaries
	u(8)

				nnpfc_transfer_characteristics
	u(8)

				nnpfc_matrix_coeffs
	u(8)

			}
	

			nnpfc_out_format_flag
	u(1)

			if( nnpfc_out_format_flag  = =  1 )
	

				nnpfc_out_tensor_bitdepth_minus8
	ue(v)

	[bookmark: _Hlk96087661]		nnpfc_out_order_idc
	ue(v)

			nnpfc_constant_patch_size_flag
	u(1)

			nnpfc_patch_width_minus1
	ue(v)

			nnpfc_patch_height_minus1
	ue(v)

			nnpfc_overlap
	ue(v)

			nnpfc_padding_type
	ue(v)

			if( nnpfc_padding_type  = =  4 ){
	

	[bookmark: _Hlk108745643]			nnpfc_luma_padding_val
	ue(v)

				nnpfc_cb_padding_val
	ue(v)

				nnpfc_cr_padding_val
	ue(v)

			}
	

			nnpfc_complexity_idc
	ue(v)

			if( nnpfc_complexity_idc > 0 )
	

				nnpfc_complexity_element( nnpfc_complexity_idc )
	

	[bookmark: _Hlk106879186]		if( nnpfc_mode_idc  = =  2 1 ) {
	

				while( !byte_aligned( ) )
	

	[bookmark: _Hlk109202531]				nnpfc_reserved_zero_bit
	u(1)

	[bookmark: _Hlk109202492][bookmark: _Hlk106879172]			nnpfc_uri_tag[ i ]
	st(v)

				nnpfc_uri[ i ]
	st(v)

			}
	

		}
	

		/* filter specified or updated by ISO/IEC 15938-17 bitstream */
	

		if( nnpfc_mode_idc  = =  1 0 ) {
	

			while( !byte_aligned( ) )
	

				nnpfc_reserved_zero_bit
	u(1)

			for( i = 0; more_data_in_payload( ); i++ )
	

				nnpfc_payload_byte[ i ]
	b(8)

		}
	

		/* filter specified by user data registered by Rec. ITU-T T.35 SEI message syntax structure */
	

	[bookmark: _Hlk117354098]	else if( nnpfc_mode_idc  = =  2 ) {
	

			while( !byte_aligned( ) )
	

				nnpfc_reserved_zero_bit
	u(1)

	[bookmark: _Hlk114840077]		nnpfc_t35_payload_size_minus1
	ue(v)

			user_data_registered_itu_t_t35(nnpfc_t35_payload_size_minus1+1)
	

		}
	

	}
	



	nnpfc_complexity_element( nnpfc_complexity_idc ) {
	Descriptor

		if( nnpfc_complexity_idc  = =  1 ) {
	

			nnpfc_parameter_type_idc
	u(2)

			if (nnpfc_parameter_type_idc ! = 2) 
	

				nnpfc_log2_parameter_bit_length_minus3
	u(2)

			nnpfc_num_parameters_idc
	u(6)

			nnpfc_num_kmac_operations_idc
	ue(v)

		}
	

	}
	



8.28.2 Neural-network post-filter characteristics SEI message semantics
This SEI message specifies a neural network that may be used as a post-processing filter. The use of specified post-processing filters for specific pictures is indicated with neural-network post-filter activation SEI messages.
Use of this SEI message requires the definition of the following variables:
–	Cropped decoded output picture width and height in units of luma samples, denoted herein by CroppedWidth and CroppedHeight, respectively.
–	Luma sample array CroppedYPic and chroma sample arrays CroppedCbPic and CroppedCrPic, when present, of the cropped decoded output picture for vertical coordinates y and horizontal coordinates x, where the top-left corner of the sample array has coordinates y equal to 0 and x equal to 0.
–	Bit depth BitDepthY for the luma sample array of the cropped decoded output picture.
–	Bit depth BitDepthC for the chroma sample arrays, if any, of the cropped decoded output picture.
–	A chroma format indicator, denoted herein by ChromaFormatIdc, as described in clause ‎7.3.
–	When nnpfc_auxiliary_inp_idc is equal to 1, a quantization strength value StrengthControlVal.
When this SEI message specifies a neural network that may be used as a post-processing filter, the semantics specify the derivation of the luma sample array FilteredYPic[ x ][ y ] and chroma sample arrays FilteredCbPic[ x ][ y ] and FilteredCrPic[ x ][ y ], as indicated by the value of nnpfc_out_order_idc, that contain the output of the post-processing filter.
The variables SubWidthC and SubHeightC are derived from ChromaFormatIdc as specified by Table 2.
nnpfc_id contains an identifying number that may be used to identify a post-processing filter. The value of nnpfc_id shall be in the range of 0 to 232 − 2, inclusive.
Values of nnpfc_id from 256 to 511, inclusive, and from 231 to 232 − 2, inclusive, are reserved for future use by ITU-T | ISO/IEC. Decoders encountering a value of nnpfc_id in the range of 256 to 511, inclusive, or in the range of 231 to 232 − 2, inclusive, shall ignore it.
nnpfc_mode_idc equal to 0 specifies that the post-processing filter associated with the nnpfc_id value is determined by external means not specified in this Specification.
nnpfc_mode_idc equal to 1 0 specifies that the post-processing filter associated with the nnpfc_id value is a neural network represented by the ISO/IEC 15938-17 bitstream contained in this SEI message.
nnpfc_mode_idc equal to 2 1 specifies that the post-processing filter associated with the nnpfc_id value is a neural network identified by a specified tag Uniform Resource Identifier (URI) (nnpfc_uri_tag[ i ]) and neural network information URI (nnpfc_uri[ i ]).
nnpfc_mode_idc equal to 2 specifies that the post-processing filter associated with the nnpfc_id value is a neural network with information specified in a user data registered by Rec. ITU-T T.35 SEI message syntax structure.
[bookmark: OLE_LINK55]The value of nnpfc_mode_idc shall be in the range of 0 to 255, inclusive. Values of nnpfc_mode_idc greater than 2 are reserved for future specification by ITU-T | ISO/IEC and shall not be present in bitstreams conforming to this version of this Specification. Decoders conforming to this version of this Specification shall ignore SEI messages that contain reserved values of nnpfc_mode_idc.
nnpfc_purpose_and_formatting_flag equal to 0 specifies that no syntax elements related to the filter purpose, input formatting, output formatting, and complexity are present. nnpfc_purpose_and_formatting_flag equal to 1 specifies that syntax elements related to the filter purpose, input formatting, output formatting, and complexity are present.
When nnpfc_mode_idc is equal to 1 0, 1, or 2 and the current CLVS does not contain a preceding neural-network post-filter characteristics SEI message, in decoding order, that has the value of nnpfc_id equal to the value of nnpfc_id in this SEI message, nnpfc_purpose_and_formatting_flag shall be equal to 1.
When the current CLVS contains a preceding neural-network post-filter characteristics SEI message, in decoding order, that has the same value of nnpfc_id equal to the value of nnpfc_id in this SEI message, at least one of the following conditions shall apply:
–	This SEI message has nnpfc_mode_idc equal to 0, 1, or 21 and nnpfc_purpose_and_formatting_flag equal to 0 in order to provide a neural network update.
–	This SEI message has the same content as the preceding neural-network post-filter characteristics SEI message.
When this SEI message is the first neural-network post-filter characteristics SEI message, in decoding order, that has a particular nnpfc_id value within the current CLVS, it specifies a base post-processing filter that pertains to the current decoded picture and all subsequent decoded pictures of the current layer, in output order, until the end of the current CLVS. When this SEI message is not the first neural-network post-filter characteristics SEI message, in decoding order, that has a particular nnpfc_id value within the current CLVS, this SEI message pertains to the current decoded picture and all subsequent decoded pictures of the current layer, in output order, until the end of the current CLVS or the next neural-network post-filter characteristics SEI message having that particular nnpfc_id value, in output order, within the current CLVS.
nnpfc_purpose indicates the purpose of post-processing filter as specified in Table 20. The value of nnpfc_purpose shall be in the range of 0 to 232 − 2, inclusive. Values of nnpfc_purpose that do not appear in Table 20 are reserved for future specification by ITU-T | ISO/IEC and shall not be present in bitstreams conforming to this version of this Specification. Decoders conforming to this version of this Specification shall ignore SEI messages that contain reserved values of nnpfc_purpose.
Table 20 – Definition of nnpfc_purpose
	Value
	Interpretation

	0
	Unknown or unspecified

	1
	Visual quality improvement

	2
	Chroma upsampling from the 4:2:0 chroma format to the 4:2:2 or 4:4:4 chroma format, or from the 4:2:2 chroma format to the 4:4:4 chroma format

	3
	Increasing the width or height of the cropped decoded output picture without changing the chroma format

	4
	Increasing the width or height of the cropped decoded output picture and upsampling the chroma format



NOTE 1 – When a reserved value of nnpfc_purpose is taken into use in the future by ITU-T | ISO/IEC, the syntax of this SEI message could be extended with syntax elements whose presence is conditioned by nnpfc_purpose being equal to that value.
[bookmark: _Hlk107944827][bookmark: _Hlk107944435][bookmark: _Hlk107944745]When SubWidthC is equal to 1 and SubHeightC is equal to 1, nnpfc_purpose shall not be equal to 2 or 4.
[bookmark: _Hlk107948000][bookmark: _Hlk107954916][bookmark: _Hlk107947976][bookmark: _Hlk107948217]nnpfc_out_sub_c_flag equal to 1 specifies that outSubWidthC is equal to 1 and outSubHeightC is equal to 1. nnpfc_out_sub_c_flag equal to 0 specifies that outSubWidthC is equal to 2 and outSubHeightC is equal to 1. When nnpfc_out_sub_c_flag is not present, outSubWidthC is inferred to be equal to SubWidthC and outSubHeightC is inferred to be equal to SubHeightC. If SubWidthC is equal to 2 and SubHeightC is equal to 1, nnpfc_out_sub_c_flag shall not be equal to 0.
nnpfc_pic_width_in_luma_samples and nnpfc_pic_height_in_luma_samples specify the width and height, respectively, of the luma sample array of the picture resulting by applying the post-processing filter identified by nnpfc_id to a cropped decoded output picture. When nnpfc_pic_width_in_luma_samples and nnpfc_pic_height_in_luma_samples are not present, they are inferred to be equal to CroppedWidth and CroppedHeight, respectively.
nnpfc_component_last_flag equal to 0 specifies that the second dimension in the input tensor inputTensor to the post-processing filter and the output tensor outputTensor resulting from the post-processing filter is used for the channel. nnpfc_component_last_flag equal to 1 specifies that the last dimension in the input tensor inputTensor to the post-processing filter and the output tensor outputTensor resulting from the post-processing filter is used for the channel.
NOTE 2 – The first dimension in the input tensor and in the output tensor is used for the batch index, which is a practice in some neural network frameworks. While the semantics of this SEI message use batch size equal to 1, it is up to the post-processing implementation to determine the batch size used as input to the neural network inference.
NOTE 3 – A colour component is an example of a channel.
nnpfc_inp_format_flag indicates the method of converting a sample value of the cropped decoded output picture to an input value to the post-processing filter. When nnpfc_inp_format_flag is equal to 0, the input values to the post-processing filter are real numbers and the functions InpY( ) and InpC( ) are specified as follows:
InpY( x ) = x ÷ ( ( 1  <<  BitDepthY ) − 1 )		(76)
InpC( x )= x ÷ ( ( 1  <<  BitDepthC ) − 1 )		(77)
When nnpfc_inp_format_flag is equal to 1, the input values to the post-processing filter are unsigned integer numbers and the functions InpY( ) and InpC( ) are specified as follows:
shiftY = BitDepthY − inpTensorBitDepth
if( inpTensorBitDepth  >=  BitDepthY)
	InpY( x ) = x  <<  ( inpTensorBitDepth − BitDepthY ) 	(78)
else
	InpY( x ) = Clip3(0, ( 1  <<  inpTensorBitDepth ) − 1, ( x + ( 1  <<  ( shiftY − 1 ) ) )  >>  shiftY ) 

shiftC = BitDepthC − inpTensorBitDepth
if( inpTensorBitDepth  >=  BitDepthC )
	InpC( x ) = x  <<  ( inpTensorBitDepth − BitDepthC ) 	(79)
else
	InpC( x ) = Clip3(0, ( 1  <<  inpTensorBitDepth ) − 1, ( x + ( 1  <<  ( shiftC − 1 ) ) )  >>  shiftC )
The variable inpTensorBitDepth is derived from the syntax element nnpfc_inp_tensor_bitdepth_minus8 as specified below.
nnpfc_inp_tensor_bitdepth_minus8 plus 8 specifies the bit depth of luma sample values in the input integer tensor. The value of inpTensorBitDepth is derived as follows:
inpTensorBitDepth = nnpfc_inp_tensor_bitdepth_minus8 + 8	(80)
It is a requirement of bitstream conformance that the value of nnpfc_inp_tensor_bitdepth_minus8 shall be in the range of 0 to 24, inclusive.
nnpfc_auxiliary_inp_idc not equal to 0 specifies auxiliary input data is present in the input tensor of the neural-network post-filter. nnpfc_auxiliary_inp_idc equal to 0 indicates that auxiliary input data is not present in the input tensor. nnpfc_auxiliary_inp_idc equal to 1 specifies that auxiliary input data is derived as specified in Table 23. The value of nnpfc_auxiliary_inp_idc shall be in the range of 0 to 255, inclusive. Values of nnpfc_auxiliary_inp_idc greater than 1 are reserved for future specification by ITU-T | ISO/IEC and shall not be present in bitstreams conforming to this version of this Specification. Decoders conforming to this version of this Specification shall ignore SEI messages that contain reserved values of nnpfc_auxiliary_inp_idc.
nnpfc_separate_colour_description_present_flag equal to 1 indicates that a distinct combination of colour primaries, transfer characteristics, and matrix coefficients for the picture resulting from the post-processing filter is specified in the SEI message syntax structure. nnfpc_separate_colour_description_present_flag equal to 0 indicates that the combination of colour primaries, transfer characteristics, and matrix coefficients for the picture resulting from the post-processing filter is the same as indicated in VUI parameters for the CLVS.
nnpfc_colour_primaries has the same semantics as specified in clause 7.3 for the vui_colour_primaries syntax element, except as follows:
[bookmark: _Hlk107944016]–	nnpfc_colour_primaries specifies the colour primaries of the picture resulting from applying the neural-network post-filter specified in the SEI message, rather than the colour primaries used for the CLVS.
–	When nnpfc_colour_primaries is not present in the neural-network post-filter characteristics SEI message, the value of nnpfc_colour_primaries is inferred to be equal to vui_colour_primaries.
nnpfc_transfer_characteristics has the same semantics as specified in clause 7.3 for the vui_transfer_characteristics syntax element, except as follows:
–	nnpfc_transfer_characteristics specifies the transfer characteristics of the picture resulting from applying the neural-network post-filter specified in the SEI message, rather than the transfer characteristics used for the CLVS.
–	When nnpfc_transfer_characteristics is not present in the neural-network post-filter characteristics SEI message, the value of nnpfc_transfer_characteristics is inferred to be equal to vui_transfer_characteristics.
nnpfc_matrix_coeffs has the same semantics as specified in clause 7.3 for the vui_matrix_coeffs syntax element, except as follows:
[bookmark: _Hlk107943225]–	nnpfc_matrix_coeffs specifies the matrix coefficients of the picture resulting from applying the neural-network post-filter specified in the SEI message, rather than the matrix coefficients used for the CLVS.
–	When nnpfc_matrix_coeffs is not present in the neural-network post-filter characteristics SEI message, the value of nnpfc_matrix_coeffs is inferred to be equal to vui_matrix_coeffs.
–	The values allowed for nnpfc_matrix_coeffs are not constrained by the chroma format of the decoded video pictures that is indicated by the value of ChromaFormatIdc for the semantics of the VUI parameters.
–	When nnpfc_matrix_coeffs is equal to 0, nnpfc_out_order_idc shall not be equal to 1 or 3.
[bookmark: _Hlk99044824]nnpfc_inp_order_idc indicates the method of ordering the sample arrays of a cropped decoded output picture as the input to the post-processing filter. Table 21 contains an informative description of nnpfc_inp_order_idc values. The semantics of nnpfc_inp_order_idc in the range of 0 to 3, inclusive, are specified in Table 23, which specifies a process for deriving the input tensors inputTensor for different values of nnpfc_inp_order_idc and a given vertical sample coordinate cTop and a horizontal sample coordinate cLeft specifying the top-left sample location for the patch of samples included in the input tensors. When the chroma format of the cropped decoded output picture is not 4:2:0, nnpfc_inp_order_idc shall not be equal to 3. The value of nnpfc_inp_order_idc shall be in the range of 0 to 255, inclusive. Values of nnpfc_inp_order_idc greater than 3 are reserved for future specification by ITU-T | ISO/IEC and shall not be present in bitstreams conforming to this version of this Specification. Decoders conforming to this version of this Specification shall ignore SEI messages that contain reserved values of nnpfc_inp_order_idc.
Table 21 – Informative description of nnpfc_inp_order_idc values
	nnpfc_inp_
order_idc
	Description

	0
	If nnpfc_auxiliary_inp_idc is equal to 0, one luma matrix is present in the input tensor, thus the number of channels is 1. Otherwise, nnpfc_auxiliary_inp_idc is not equal to 0 and one luma matrix and one auxiliary input matrix are present, thus the number of channels is 2.

	1
	If nnpfc_auxiliary_inp_idc is equal to 0, two chroma matrices are present in the input tensor, thus the number of channels is 2. Otherwise, nnpfc_auxiliary_inp_idc is not equal to 0 and two chroma matrices and one auxiliary input matrix are present, thus the number of channels is 3.

	2
	If nnpfc_auxiliary_inp_idc is equal to 0, one luma and two chroma matrices are present in the input tensor, thus the number of channels is 3. Otherwise, nnpfc_auxiliary_inp_idc is not equal to 0 and one luma matrix, two chroma matrices and one auxiliary input matrix are present, thus the number of channels is 4.

	3
	If nnpfc_auxiliary_inp_idc is equal to 0, four luma matrices and two chroma matrices are present in the input tensor, thus the number of channels is 6. Otherwise, nnpfc_auxiliary_inp_idc is not equal to 0 and four luma matrices, two chroma matrices, and one auxiliary input matrix are present in the input tensor, thus the number of channels is 7. The luma channels are derived in an interleaved manner as illustrated in Figure 12. This nnpfc_inp_order_idc can only be used when the chroma format is 4:2:0.

	4..255
	Reserved



[image: ]
[bookmark: _Ref278067287][bookmark: _Toc55408388]Figure 12 – Illustration of luma data channels of nnpfc_inp_order_idc equal to 3 (informative)
A patch is a rectangular array of samples from a component (e.g., a luma or chroma component) of a picture.
nnpfc_constant_patch_size_flag equal to 0 specifies that the post-processing filter accepts any patch size that is a positive integer multiple of the patch size indicated by nnpfc_patch_width_minus1 and nnpfc_patch_height_minus1 as input. When nnpfc_constant_patch_size_flag is equal to 0 the patch size width shall be less than or equal to CroppedWidth. When nnpfc_constant_patch_size_flag is equal to 0 the patch size height shall be less than or equal to CroppedHeight. nnpfc_constant_patch_size_flag equal to 1 specifies that the post-processing filter accepts exactly the patch size indicated by nnpfc_patch_width_minus1 and nnpfc_patch_height_minus1 as input.
nnpfc_patch_width_minus1 + 1, when nnpfc_constant_patch_size_flag equal to 1, specifies the horizontal sample counts of the patch size required for the input to the post-processing filter. When nnpfc_constant_patch_size_flag is equal to 0, any positive integer multiple of ( nnpfc_patch_width_minus1 + 1 ) may be used as the horizontal sample counts of the patch size used for the input to the post-processing filter. The value of nnpfc_patch_width_minus1 shall be in the range of 0 to Min( 32766, CroppedWidth − 1 ), inclusive.
nnpfc_patch_height_minus1 + 1, when nnpfc_constant_patch_size_flag equal to 1, specifies the vertical sample counts of the patch size required for the input to the post-processing filter. When nnpfc_constant_patch_size_flag is equal to 0, any positive integer multiple of ( nnpfc_patch_height_minus1 + 1 ) may be used as the vertical sample counts of the patch size used for the input to the post-processing filter. The value of nnpfc_patch_height_minus1 shall be in the range of 0 to Min( 32766, CroppedHeight − 1 ), inclusive.
nnpfc_overlap specifies the overlapping horizontal and vertical sample counts of adjacent input tensors of the post-processing filter. The value of nnpfc_overlap shall be in the range of 0 to 16383, inclusive.
The variables inpPatchWidth, inpPatchHeight, outPatchWidth, outPatchHeight, horCScaling, verCScaling, outPatchCWidth, outPatchCHeight, and overlapSize are derived as follows:
inpPatchWidth = nnpfc_patch_width_minus1 + 1
inpPatchHeight = nnpfc_patch_height_minus1 + 1
outPatchWidth = ( nnpfc_pic_width_in_luma_samples * inpPatchWidth ) / CroppedWidth
outPatchHeight = ( nnpfc_pic_height_in_luma_samples * inpPatchHeight ) / CroppedHeight
horCScaling = SubWidthC / outSubWidthC
verCScaling = SubHeightC / outSubHeightC							(81)
outPatchCWidth = outPatchWidth * horCScaling
outPatchCHeight = outPatchHeight * verCScaling
overlapSize = nnpfc_overlap
It is a requirement of bitstream conformance that outPatchWidth * CroppedWidth shall be equal to nnpfc_pic_width_in_luma_samples * inpPatchWidth and outPatchHeight * CroppedHeight shall be equal to nnpfc_pic_height_in_luma_samples * inpPatchHeight.
nnpfc_padding_type specifies the process of padding when referencing sample locations outside the boundaries of the cropped decoded output picture as described in Table 22. The value of nnpfc_padding_type shall be in the range of 0 to 15, inclusive.
Table 22 – Informative description of nnpfc_padding_type values
	nnpfc_padding_type
	Description

	0
	zero padding

	1
	replication padding

	2
	reflection padding

	3
	[bookmark: _Hlk107412882]wrap-around padding

	4
	fixed padding 

	5..15
	Reserved



nnpfc_luma_padding_val specifies the luma value to be used for padding when nnpfc_padding_type is equal to 4.
nnpfc_cb_padding_val specifies the Cb value to be used for padding when nnpfc_padding_type is equal to 4.
nnpfc_cr_padding_val specifies the Cr value to be used for padding when nnpfc_padding_type is equal to 4.
The function InpSampleVal( y, x, picHeight, picWidth, croppedPic ) with inputs being a vertical sample location y, a horizontal sample location x, a picture height picHeight, a picture width picWidth, and sample array croppedPic returns the value of sampleVal derived as follows:
[bookmark: _Hlk108736881][bookmark: _Hlk107486710][bookmark: _Hlk108736940][bookmark: _Hlk108736928]if( nnpfc_padding_type  = =  0 )
	if( y < 0  | |  x < 0  | |  y >= picHeight  | |  x  >=  picWidth )
		sampleVal = 0
	else
		sampleVal = croppedPic[ x ][ y ]		(82)
else if( nnpfc_padding_type  = =  1 )
	sampleVal = croppedPic[ Clip3( 0, picWidth − 1, x ) ][ Clip3( 0, picHeight − 1, y ) ]
else if( nnpfc_padding_type  = =  2 ) 
	sampleVal = croppedPic[ Reflect( picWidth − 1, x ) ][ Reflect( picHeight − 1, y ) ]
else if( nnpfc_padding_type  = =  3 ) 
	if( y >= 0  &&  y < picHeight )
		sampleVal = croppedPic[ Wrap( picWidth − 1, x ) ][ y ] 
else if( nnpfc_padding_type  = =  4 ) 
	if( y < 0  | |  x < 0  | |  y >= picHeight  | |  x  >=  picWidth )
		sampleVal[ 0 ]  = nnpfc_luma_padding_val			sampleVal[ 1 ]  = nnpfc_cb_padding_val
		sampleVal[ 2 ] = nnpfc_cr_padding_val
	else
		sampleVal = croppedPic[ x ][ y ]

Table 23 – Process for deriving the input tensors inputTensor for a given vertical sample coordinate cTop and a horizontal sample coordinate cLeft specifying the top-left sample location for the patch of samples included in the input tensors
	nnpfc_inp_
order_idc
	Process DeriveInputTensors( ) for deriving input tensors

	0
	for( yP = −overlapSize; yP < inpPatchHeight + overlapSize; yP++)
	for( xP = −overlapSize; xP < inpPatchWidth + overlapSize; xP++ ) {
		inpVal = InpY( InpSampleVal( cTop + yP, cLeft + xP, CroppedHeight,
				CroppedWidth, CroppedYPic ) )
		if( nnpfc_component_last_flag  = =  0 )
			inputTensor[ 0 ][ 0 ][ yP + overlapSize ][ xP + overlapSize ] = inpVal
		else
			inputTensor[ 0 ][ yP + overlapSize ][ xP + overlapSize ][ 0 ] = inpVal
		if( nnpfc_auxiliary_inp_idc  = =  1 ) 
			if( nnpfc_component_last_flag  = =  0 )
				inputTensor[ 0 ][ 1 ][ yP + overlapSize ][ xP + overlapSize ] = 2( StrengthControlVal − 42 ) / 6 
			else
				inputTensor[ 0 ][ yP + overlapSize ][ xP + overlapSize ][ 1 ] = 2( StrengthControlVal − 42 ) / 6
	}

	1
	for( yP = −overlapSize; yP < inpPatchHeight + overlapSize; yP++)
	for( xP = −overlapSize; xP < inpPatchWidth + overlapSize; xP++ ) {
		inpCbVal = InpC( InpSampleVal( cTop + yP, cLeft + xP, CroppedHeight / SubHeightC,
				CroppedWidth / SubWidthC, CroppedCbPic ) )
		inpCrVal = InpC( InpSampleVal( cTop + yP, cLeft + xP, CroppedHeight / SubHeightC,
				CroppedWidth / SubWidthC, CroppedCrPic ) )
		if( nnpfc_component_last_flag  = =  0 ) {
			inputTensor[ 0 ][ 0 ][ yP + overlapSize ][ xP + overlapSize ] = inpCbVal
			inputTensor[ 0 ][ 1 ][ yP + overlapSize ][ xP + overlapSize ] = inpCrVal
		} else {
			inputTensor[ 0 ][ yP + overlapSize ][ xP + overlapSize ][ 0 ] = inpCbVal
			inputTensor[ 0 ][ yP + overlapSize ][ xP + overlapSize ][ 1 ] = inpCrVal
		}
		if(nnpfc_auxiliary_inp_idc  = =  1)
			if( nnpfc_component_last_flag  = =  0 )
				inputTensor[ 0 ][ 2 ][ yP + overlapSize ][ xP + overlapSize ] = 2( StrengthControlVal − 42 ) / 6
			else
				inputTensor[ 0 ][ yP + overlapSize ][ xP + overlapSize ][ 2 ] = 2( StrengthControlVal − 42 ) / 6
	}

	2
	for( yP = −overlapSize; yP < inpPatchHeight + overlapSize; yP++)
	for( xP = −overlapSize; xP < inpPatchWidth + overlapSize; xP++ ) {
		yY = cTop + yP
		xY = cLeft + xP
		yC = yY / SubHeightC
		xC = xY / SubWidthC	
		inpYVal = InpY( InpSampleVal( yY, xY, CroppedHeight,
				CroppedWidth, CroppedYPic ) )
		inpCbVal = InpC( InpSampleVal( yC, xC, CroppedHeight / SubHeightC,
				CroppedWidth / SubWidthC, CroppedCbPic ) )
		inpCrVal = InpC( InpSampleVal( yC, xC, CroppedHeight / SubHeightC,
				CroppedWidth / SubWidthC, CroppedCrPic ) )
		if( nnpfc_component_last_flag  = =  0 ) {
			inputTensor[ 0 ][ 0 ][ yP + overlapSize ][ xP + overlapSize ] = inpYVal
			inputTensor[ 0 ][ 1 ][ yP + overlapSize ][ xP + overlapSize ] = inpCbVal
			inputTensor[ 0 ][ 2 ][ yP + overlapSize ][ xP + overlapSize ] = inpCrVal
		} else {
			inputTensor[ 0 ][ yP + overlapSize ][ xP + overlapSize ][ 0 ] = inpYVal
			inputTensor[ 0 ][ yP + overlapSize ][ xP + overlapSize ][ 1 ] = inpCbVal
			inputTensor[ 0 ][ yP + overlapSize ][ xP + overlapSize ][ 2 ] = inpCrVal
		}
		if(nnpfc_auxiliary_inp_idc  = =  1)
			if( nnpfc_component_last_flag  = =  0 )
				inputTensor[ 0 ][ 3 ][ yP + overlapSize ][ xP + overlapSize ] = 2( StrengthControlVal − 42 ) / 6
			else
				inputTensor[ 0 ][ yP + overlapSize ][ xP + overlapSize ][ 3 ] = 2( StrengthControlVal − 42 ) / 6
	}

	3
	for( yP = −overlapSize; yP < inpPatchHeight + overlapSize; yP++)
	for( xP = −overlapSize; xP < inpPatchWidth + overlapSize; xP++ ) {
		yTL = cTop + yP * 2
		xTL = cLeft + xP * 2
		yBR = yTL + 1
		xBR = xTL + 1
		yC = cTop / 2 + yP
		xC = cLeft / 2 + xP
		inpTLVal = InpY( InpSampleVal( yTL, xTL, CroppedHeight,
				CroppedWidth, CroppedYPic ) )
		inpTRVal = InpY( InpSampleVal( yTL, xBR, CroppedHeight,
				CroppedWidth, CroppedYPic ) )
		inpBLVal = InpY( InpSampleVal( yBR, xTL, CroppedHeight,
				CroppedWidth, CroppedYPic ) )
		inpBRVal = InpY( InpSampleVal( yBR, xBR, CroppedHeight,
				CroppedWidth, CroppedYPic ) )
		inpCbVal = InpC( InpSampleVal( yC, xC, CroppedHeight / 2,
				CroppedWidth / 2, CroppedCbPic ) )
		inpCrVal = InpC( InpSampleVal( yC, xC, CroppedHeight / 2,
				CroppedWidth / 2, CroppedCrPic ) )
		if( nnpfc_component_last_flag  = =  0 ) {
			inputTensor[ 0 ][ 0 ][ yP + overlapSize ][ xP + overlapSize ] = inpTLVal
			inputTensor[ 0 ][ 1 ][ yP + overlapSize ][ xP + overlapSize ] = inpTRVal
			inputTensor[ 0 ][ 2 ][ yP + overlapSize ][ xP + overlapSize ] = inpBLVal
			inputTensor[ 0 ][ 3 ][ yP + overlapSize ][ xP + overlapSize ] = inpBRVal
			inputTensor[ 0 ][ 4 ][ yP + overlapSize ][ xP + overlapSize ] = inpCbVal
			inputTensor[ 0 ][ 5 ][ yP + overlapSize ][ xP + overlapSize ] = inpCrVal
			inputTensor[ 0 ][ 6 ][ yP + overlapSize ][ xP + overlapSize ] = 2( StrengthControlVal − 42 ) / 6
		} else {
			inputTensor[ 0 ][ yP + overlapSize ][ xP + overlapSize ][ 0 ] = inpTLVal
			inputTensor[ 0 ][ yP + overlapSize ][ xP + overlapSize ][ 1 ] = inpTRVal
			inputTensor[ 0 ][ yP + overlapSize ][ xP + overlapSize ][ 2 ] = inpBLVal
			inputTensor[ 0 ][ yP + overlapSize ][ xP + overlapSize ][ 3 ] = inpBRVal
			inputTensor[ 0 ][ yP + overlapSize ][ xP + overlapSize ][ 4 ] = inpCbVal
			inputTensor[ 0 ][ yP + overlapSize ][ xP + overlapSize ][ 5 ] = inpCrVal		}
		if(nnpfc_auxiliary_inp_idc  = =  1) 
			if( nnpfc_component_last_flag  = =  0 )
				inputTensor[ 0 ][ 6 ][ yP + overlapSize ][ xP + overlapSize ] = 2( StrengthControlVal − 42 ) / 6
			else
				inputTensor[ 0 ][ yP + overlapSize ][ xP + overlapSize ][ 6 ] = 2( StrengthControlVal − 42 ) / 6
	}
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[bookmark: _Hlk104544193]nnpfc_complexity_idc greater than 0 specifies that one or more syntax elements that indicate the complexity of the post-processing filter associated with the nnpfc_id may be present. nnpfc_complexity_idc equal to 0 specifies that no syntax elements that indicate the complexity of the post-processing filter associated with the nnpfc_id are present. The value nnpfc_complexity_idc shall be in the range of 0 to 255, inclusive. Values of nnpfc_complexity_idc greater than 1 are reserved for future specification by ITU-T | ISO/IEC and shall not be present in bitstreams conforming to this version of this Specification. Decoders conforming to this version of this Specification shall ignore SEI messages that contain reserved values of nnpfc_complexity_idc.
nnpfc_out_format_flag equal to 0 indicates that the sample values output by the post-processing filter are real numbers and the functions OutY( ) and OutC( ) for converting luma sample values and chroma sample values, respectively, output by the post-processing, to integer values at bit depths BitDepthY and BitDepthC, respectively, are specified as follows:
OutY( x ) = Clip3( 0, ( 1  <<  BitDepthY ) − 1, Round( x * ( ( 1  <<  BitDepthY ) − 1 ) ) )	(83)
OutC( x )= Clip3( 0, ( 1  <<  BitDepthC ) − 1, Round( x * ( ( 1  <<  BitDepthC ) − 1 ) ) )	(84)
[bookmark: _Hlk101599236]nnpfc_out_format_flag equal to 1 indicates that the sample values output by the post-processing filter are unsigned integer numbers and the functions OutY( ) and OutC( ) are specified as follows:
shiftY = outTensorBitDepth − BitDepthY
if( shiftY > 0 )
	OutY( x ) = Clip3( 0, ( 1  <<  BitDepthY ) − 1, ( x + ( 1  <<  ( shiftY − 1 ) ) )  >>  shiftY ) ) 	(85)
else
	OutY( x ) = x  <<  ( BitDepthY − outTensorBitDepth ) 
shiftC = outTensorBitDepth − BitDepthC
if( shiftC > 0 )
	OutC( x )= Clip3( 0, ( 1  <<  BitDepthC ) − 1, ( x + ( 1  <<  ( shiftC − 1 ) ) )  >>  shiftC ) 	(86)
else
	OutC( x ) = x  <<  ( BitDepthC − outTensorBitDepth )
The variable outTensorBitDepth is derived from the syntax element nnpfc_out_tensor_bitdepth_minus8 as described below.
[bookmark: _Hlk101599286]nnpfc_out_tensor_bitdepth_minus8 plus 8 specifies the bit depth of sample values in the output integer tensor. The value of outTensorBitDepth is derived as follows:
outTensorBitDepth = nnpfc_out_tensor_bitdepth_minus8 + 8	(87)
It is a requirement of bitstream conformance that the value of nnpfc_out_tensor_bitdepth_minus8 shall be in the range of 0 to 24, inclusive.
nnpfc_out_order_idc indicates the output order of samples resulting from the post-processing filter. Table 24 contains an informative description of nnpfc_out_order_idc values. The semantics of nnpfc_out_order_idc in the range of 0 to 3, inclusive, are specified in Table 25, which specifies a process for deriving sample values in the filtered output sample arrays FilteredYPic, FilteredCbPic, and FilteredCrPic from the output tensors outputTensor for different values of nnpfc_out_order_idc and a given vertical sample coordinate cTop and a horizontal sample coordinate cLeft specifying the top-left sample location for the patch of samples included in the input tensors. When nnpfc_purpose is equal to 2 or 4, nnpfc_out_order_idc shall not be equal to 3. The value of nnpfc_out_order_idc shall be in the range of 0 to 255, inclusive. Values of nnpfc_out_order_idc greater than 3 are reserved for future specification by ITU-T | ISO/IEC and shall not be present in bitstreams conforming to this version of this Specification. Decoders conforming to this version of this Specification shall ignore SEI messages that contain reserved values of nnpfc_out_order_idc.
Table 24 – Informative description of nnpfc_out_order_idc values
	nnpfc_out_
order_idc
	Description

	0
	Only the luma matrix is present in the output tensor, thus the number of channels is 1.

	1
	Only the chroma matrices are present in the output tensor, thus the number of channels is 2.

	2
	The luma and chroma matrices are present in the output tensor, thus the number of channels is 3.

	3
	Four luma matrices and two chroma matrices are present in the output tensor, thus the number of channels is 6. This nnpfc_out_order_idc can only be used when the chroma format is 4:2:0.
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Table 25 – Process for deriving sample values in the filtered output sample arrays FilteredYPic, FilteredCbPic, and FilteredCrPic from the output tensors outputTensor for a given vertical sample coordinate cTop and a horizontal sample coordinate cLeft specifying the top-left sample location for the patch of samples included in the input tensors
	nnpfc_out_
order_idc
	Process StoreOutputTensors( ) for deriving sample values in the filtered picture from the output tensors

	0
	for( yP = 0; yP < outPatchHeight; yP++)
	for( xP = 0; xP < outPatchWidth; xP++ ) {
		yY = cTop * outPatchHeight / inpPatchHeight + yP
		xY = cLeft * outPatchWidth / inpPatchWidth + xP
		if ( yY < nnpfc_pic_height_in_luma_samples  &&  xY < nnpfc_pic_width_in_luma_samples )
			if( nnpfc_component_last_flag  = =  0 )
				FilteredYPic[ xY ][yY ] = OutY( outputTensor[ 0 ][ 0 ][ yP ][ xP ] )
			else
				FilteredYPic[ xY ][ yY ] = OutY( outputTensor[ 0 ][ yP ][ xP ][ 0 ] )
	}

	1
	for( yP = 0; yP < outPatchCHeight; yP++)
	for( xP = 0; xP < outPatchCWidth; xP++ ) {
		xSrc = cLeft * horCScaling + xP
		ySrc = cTop * verCScaling + yP
		if ( ySrc < nnpfc_pic_height_in_luma_samples / outSubHeightC  &&
				xSrc < nnpfc_pic_width_in_luma_samples / outSubWidthC )
			if( nnpfc_component_last_flag  = =  0 ) {
				FilteredCbPic[ xSrc ][ ySrc ] = OutC( outputTensor[ 0 ][ 0 ][ yP ][ xP ] )
				FilteredCrPic[ xSrc ][ ySrc ] = OutC( outputTensor[ 0 ][ 1 ][ yP ][ xP ] )
			} else {
				FilteredCbPic[ xSrc ][ ySrc ] = OutC( outputTensor[ 0 ][ yP ][ xP ][ 0 ] )
				FilteredCrPic[ xSrc ][ ySrc ] = OutC( outputTensor[ 0 ][ yP ][ xP ][ 1 ] )
			}
	}

	2
	for( yP = 0; yP < outPatchHeight; yP++)
	for( xP = 0; xP < outPatchWidth; xP++ ) {
		yY = cTop * outPatchHeight / inpPatchHeight + yP
		xY = cLeft * outPatchWidth / inpPatchWidth + xP
		yC = yY / outSubHeightC 
		xC = xY / outSubWidthC 
		yPc = ( yP / outSubHeightC ) * outSubHeightC
		xPc = ( xP / outSubWidthC ) * outSubWidthC
		if ( yY < nnpfc_pic_height_in_luma_samples && xY < nnpfc_pic_width_in_luma_samples)
			if( nnpfc_component_last_flag  = =  0 ) {
				FilteredYPic[ xY ][ yY ] = OutY( outputTensor[ 0 ][ 0 ][ yP ][ xP ] )
				FilteredCbPic[ xC ][ yC ] = OutC( outputTensor[ 0 ][ 1 ][ yPc ][ xPc ] )
				FilteredCrPic[ xC ][ yC ] = OutC( outputTensor[ 0 ][ 2 ][ yPc ][ xPc ] )
			} else {
				FilteredYPic[ xY ][ yY ] = OutY( outputTensor[ 0 ][ yP ][ xP ][ 0 ] )
				FilteredCbPic[ xC ][ yC ] = OutC( outputTensor[ 0 ][ yPc ][ xPc ][ 1 ] )
				FilteredCrPic[ xC ][ yC ] = OutC( outputTensor[ 0 ][ yPc ][ xPc ][ 2 ] )
			}
	}

	3
	for( yP = 0; yP < outPatchHeight; yP++ )
	for( xP = 0; xP < outPatchWidth; xP++ ) {
		ySrc = cTop / 2 * outPatchHeight / inpPatchHeight + yP
		xSrc = cLeft / 2 * outPatchWidth / inpPatchWidth + xP
		if ( ySrc < nnpfc_pic_height_in_luma_samples / 2  &&
				xSrc < nnpfc_pic_width_in_luma_samples / 2 )
			if( nnpfc_component_last_flag  = =  0 ) {
				FilteredYPic[ xSrc * 2 ][ ySrc * 2 ] = OutY( outputTensor[ 0 ][ 0 ][ yP ][ xP ] )
				FilteredYPic[ xSrc * 2 + 1 ][ ySrc * 2 ] = OutY( outputTensor[ 0 ][ 1 ][ yP ][ xP ] )
				FilteredYPic[ xSrc * 2 ][ ySrc * 2 + 1 ] = OutY( outputTensor[ 0 ][ 2 ][ yP ][ xP ] )
				FilteredYPic[ xSrc * 2 + 1][ ySrc * 2 + 1 ] = OutY( outputTensor[ 0 ][ 3 ][ yP ][ xP ] )
				FilteredCbPic[ xSrc ][ ySrc ] = OutC( outputTensor[ 0 ][ 4 ][ yP ][ xP ] )
				FilteredCrPic[ xSrc ][ ySrc ] = OutC( outputTensor[ 0 ][ 5 ][ yP ][ xP ] )
			} else {
				FilteredYPic[ xSrc * 2 ][ ySrc * 2 ] = OutY( outputTensor[ 0 ][ yP ][ xP ][ 0 ] )
				FilteredYPic[ xSrc * 2 + 1 ][ ySrc * 2 ] = OutY( outputTensor[ 0 ][ yP ][ xP ][ 1 ] )
				FilteredYPic[ xSrc * 2 ][ ySrc * 2 + 1 ] = OutY( outputTensor[ 0 ][ yP ][ xP ][ 2 ] )
				FilteredYPic[ xSrc * 2 + 1][ ySrc * 2 + 1 ] = OutY( outputTensor[ 0 ][ yP ][ xP ][ 3 ] )
				FilteredCbPic[ xSrc ][ ySrc ] = OutC( outputTensor[ 0 ][ yP ][ xP ][ 4 ] )
				FilteredCrPic[ xSrc ][ ySrc ] = OutC( outputTensor[ 0 ][ yP ][ xP ][ 5 ] )
			}
	}
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A base post-processing filter for a cropped decoded output picture picA is the filter that is identified by the first neural-network post-filter characteristics SEI message, in decoding order, that has a particular nnpfc_id value within a CLVS.
If there is another neural-network post-filter characteristics SEI message that has the same nnpfc_id value, has nnpfc_mode_idc equal to 0, 1, or 21, has different content than the neural-network post-filter characteristics SEI message that defines the base post-processing filter, and pertains to the picture picA, the base post-processing filter is updated by decoding the ISO/IEC 15938-17 bitstream in that neural-network post-filter characteristics SEI message to obtain a post-processing filter PostProcessingFilter( ). Otherwise, the post-processing processing filter PostProcessingFilter( ) is assigned to be the same as the base post-processing filter.
The following process is used to filter the cropped decoded output picture with the post-processing filter PostProcessingFilter( ) to generate the filtered picture, which contains Y, Cb, and Cr sample arrays FilteredYPic, FilteredCbPic, and FilteredCrPic, respectively, as indicated by nnpfc_out_order_idc.
if( nnpfc_inp_order_idc  = =  0 )
	for( cTop = 0; cTop < CroppedHeight; cTop  +=  inpPatchHeight )
		for( cLeft = 0; cLeft < CroppedWidth; cLeft  +=  inpPatchWidth ) {
			DeriveInputTensors( )
			outputTensor = PostProcessingFilter( inputTensor )
			StoreOutputTensors( )
		}
else if( nnpfc_inp_order_idc  = =  1 )
	for( cTop = 0; cTop < CroppedHeight / SubHeightC; cTop  +=  inpPatchHeight )
		for( cLeft = 0; cLeft < CroppedWidth / SubWidthC; cLeft  +=  inpPatchWidth ) {
			DeriveInputTensors( )
			outputTensor = PostProcessingFilter( inputTensor )
			StoreOutputTensors( )
		}
else if( nnpfc_inp_order_idc  = =  2 )
	for( cTop = 0; cTop < CroppedHeight; cTop  +=  inpPatchHeight)	(88)
		for( cLeft = 0; cLeft < CroppedWidth; cLeft  +=  inpPatchWidth) {
			DeriveInputTensors( )
			outputTensor = PostProcessingFilter( inputTensor )
			StoreOutputTensors( )
		}
else if( nnpfc_inp_order_idc  = =  3 )
	for( cTop = 0; cTop < CroppedHeight; cTop  +=  inpPatchHeight * 2 )
		for( cLeft = 0; cLeft < CroppedWidth; cLeft  +=  inpPatchWidth * 2 ) {
			DeriveInputTensors( )
			outputTensor = PostProcessingFilter( inputTensor )
			StoreOutputTensors( )
		}
nnpfc_reserved_zero_bit shall be equal to 0.
[bookmark: _Hlk106879970][bookmark: _Hlk106880694][bookmark: _Hlk106879941][bookmark: _Hlk101545149]nnpfc_uri_tag[ i ] contains a NULL-terminated UTF-8 character string specifying a tag URI. The UTF-8 character string shall contain a URI, with syntax and semantics as specified in IETF RFC 4151, uniquely identifying the format and associated information about the neural network used as the post-processing filter specified by nnrpf_uri[ i ] values.
[bookmark: _Hlk106880017]NOTE 4 – nnrpf_uri_tag[ i ] elements represent a 'tag' URI, which enables uniquely identifying the format of neural network data specified by nnrpf_uri[ i ] values without needing a central registration authority.
[bookmark: _Hlk106880426][bookmark: _Hlk106880589][bookmark: _Hlk106880490]nnpfc_uri[ i ] shall contain a NULL-terminated UTF-8 character string, as specified in ISO/IEC 10646. The UTF-8 character string shall contain a URI, with syntax and semantics as specified in IETF Internet Standard 66, identifying the neural network information (e.g. data representation) used as the post-processing filter.
nnpfc_t35_payload_size_minus1 plus 1 specifies the number of bytes in the user_data_registered_itu_t_t35( ) syntax structure  that immediately follows.
nnpfc_payload_byte[ i ] contains the i-th byte of a bitstream conforming to ISO/IEC 15938-17. The byte sequence nnpfc_payload_byte[ i ] for all present values of i shall be a complete bitstream that conforms to ISO/IEC 15938-17.
[bookmark: _Hlk102086328]nnpfc_parameter_type_idc equal to 0 indicates that the neural network uses only integer parameters. nnpfc_parameter_type_flag equal to 1 indicates that the neural network may use floating point or integer parameters. nnpfc_parameter_type_idc equal to 2 indicates that the neural network uses only binary parameters. nnpfc_parameter_type_idc equal to 3 is reserved for future specification by ITU-T | ISO/IEC and shall not be present in bitstreams conforming to this version of this Specification. Decoders conforming to this version of this Specification shall ignore SEI messages that contain reserved value of nnpfc_parameter_type_idc.
[bookmark: _Hlk102086340]nnpfc_log2_parameter_bit_length_minus3 equal to 0, 1, 2, and 3 indicates that the neural network does not use parameters of bit length greater than 8, 16, 32, and 64, respectively. When nnpfc_parameter_type_idc is present and nnpfc_log2_parameter_bit_length_minus3 is not present the neural network does not use parameters of bit length greater than 1.
nnpfc_num_parameters_idc indicates the maximum number of neural network parameters for the post processing filter in units of a power of 2048. nnpfc_num_parameters_idc equal to 0 indicates that the maximum number of neural network parameters is not specified. The value nnpfc_num_parameters_idc shall be in the range of 0 to 52, inclusive. Values of nnpfc_num_parameters_idc greater than 52 are reserved for future specification by ITU-T | ISO/IEC and shall not be present in bitstreams conforming to this version of this Specification. Decoders conforming to this version of this Specification shall ignore SEI messages that contain reserved values of nnpfc_num_parameters_idc.
If the value of nnpfc_num_parameters_idc is greater than zero, the variable maxNumParameters is derived as follows:
	maxNumParameters = ( 2048  <<  nnpfc_num_parameters_idc ) − 1	(89)
It is a requirement of bitstream conformance that the number of neural network parameters of the post-processing filter shall be less than or equal to maxNumParameters.
nnpfc_num_kmac_operations_idc greater than 0 specifies that the maximum number of multiply-accumulate operations per sample of the post-processing filter is less than or equal to nnpfc_num_kmac_operations_idc * 1000. nnpfc_num_kmac_operations_idc equal to 0 specifies that the maximum number of multiply-accumulate operations of the network is not specified. The value of nnpfc_num_kmac_operations_idc shall be in the range of 0 to 232 − 1, inclusive.
Patent rights declaration(s)
Dolby Laboratories, Inc. may have current or pending patent rights relating to the technology described in this contribution and, conditioned on reciprocity, is prepared to grant licenses under reasonable and non-discriminatory terms as necessary for implementation of the resulting ITU-T Recommendation | ISO/IEC International Standard (per box 2 of the ITU-T/ITU-R/ISO/IEC patent statement and licensing declaration form).
Sharp Labs of America, Inc., may have current or pending patent rights relating to the technology described in this contribution and, conditioned on reciprocity, is prepared to grant licenses under reasonable and non-discriminatory terms as necessary for implementation of the resulting ITU-T Recommendation | ISO/IEC International Standard (per box 2 of the ITU-T/ITU-R/ISO/IEC patent statement and licensing declaration form).
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