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Summary
The ITU-T/ISO/IEC Joint Video Experts Team (JVET) is a group of video coding experts from the ITU-T Study Group 16 Visual Coding Experts Group (VCEG) and ISO/IEC JTC 1/‌SC 29/‌WG 5. The parent bodies of the JVET are ITU-T WP3/16 and ISO/IEC JTC 1/‌SC 29. JVET is chaired by Jens-Rainer Ohm (contact information in the list of authors)
It is further noted that the unabbreviated name of JVET was formerly known as “Joint Video Exploration Team”, but the parent bodies modified it when entering the phase of formal development of the Versatile Video Coding (VVC) and Versatile Supplemental Enhancement Information Messages for Coded Video Bitstreams (VSEI) standards. Furthermore, starting from the twentieth meeting, work items which had originally been conducted by the Joint Collaborative Team on Video Coding (JCT-VC) during 2010-2020 were continued to be conducted in JVET as a single joint team, as negotiated by the parent bodies. The same is the case for other joint teams whose work had previously been continued by JCT-VC, namely the Joint Video Team (JVT, 2001-2009), and the Joint Collaborative Team on 3D Video Coding Extension Development (JCT-3V, 2012-2016).
This document introduces IT systems and resources maintained by JVET for effective progression of its work. This includes communication practices, software, conformance testing suites, and test materials.
Communication practices
All documents of JVET can be found at https://jvet-experts.org/. It was is noted that the previous site http://phenix.int-evry.fr/jvet/ (containing documents of JVET meetings 1-20) is still accessible, but was converted to read-only. Likewise, documents of the other joint teams are accessible under http://phenix.int-evry.fr/jct/, http://phenix.int-evry.fr/jct3v/, and https://www.itu.int/wftp3/av-arch/jvt-site/.
All these sites are openly accessible. However, if you want to submit a contribution to the next JVET meeting, it is necessary to register as a user (this may take some time, as there is a process of authorization involved). Once you are a registered user, you can register and subsequently upload your contribution. A template document is available at the site https://www.itu.int/wftp3/av-arch/jvet-site/ in the folder of the respective meeting. As an example, for the 28th 30th meeting, this would be https://www.itu.int/wftp3/av-arch/jvet-site/20222023_1004_ABAD_MainzAntalya/JVET-ABXXXXADXXXX.docx. It is mandatory using this template and following the instructions given in that document. Please further note that after uploading, the document will not immediately be available to other experts. It first needs to be approved by the chair. The chair will contact you via email if some problem was found with your uploaded document, in which case he would reject the uploaded version to prevent its public availability. You may also ask the chair yourself to reject an uploaded version in case you find an error afterwards.
JVET email lists are managed through the site https://lists.rwth-aachen.de/postorius/lists/jvet.lists.rwth-aachen.de/, and to send email to the reflector, the email address is jvet@lists.rwth-aachen.de. Only members of the reflector can send email to the list. However, membership of the reflector is not limited to qualified JVET participants.
It is emphasized that reflector subscriptions and email sent to the reflector must use real names when subscribing and sending messages, and subscribers must respond to inquiries regarding the nature of their interest in the work. All discussions (including those on AVC, HEVC, VVC, CICP, etc.) shall be conducted on the JVET reflector rather than any of the old reflectors (including JVT, JCT-VC, and JCT-3V) which are retained for archiving purposes. Archives can be found after logging in to the site mentioned in the previous paragraph for the JVET list, and on the corresponding sites https://lists.rwth-aachen.de/postorius/lists/jct-vc.lists.rwth-aachen.de/ for the JCT-VC list, https://lists.rwth-aachen.de/postorius/lists/jct-3v.lists.rwth-aachen.de/ for the JCT-3V list, and https://lists.rwth-aachen.de/postorius/lists/jvt-experts.lists.rwth-aachen.de/ for the JVT list.
When JVET related meeting activities or events are conducted online, (usually via Zoom teleconference meeting), the following rules have been established:
· Use the “hand-raising” function to enter yourself in the queue to speak (unless otherwise instructed by the session chair). If you are dialed in by phone, request your queue position verbally. The online queue will be interleaved with the room queue, though it may not always be guaranteed that the sequence perfectly follows the sequence by which hand raising occurred.
· Stay muted unless you have something to say. People are muted by default when they join and need to unmute themselves to speak. The chair may mute anyone who is disrupting the proceedings (e.g. by forgetting they have a live microphone while chatting with their family or by causing bad noise or echo).
· Identify who you are and your affiliation when you begin speaking. The same applies for speakers in the room to let online participants know who is speaking.
· Use your full name and company/organization and country affiliation in your joining information, since the participation list of Zoom would also be used to compile the online part of attendance records.
· Turn on the chat window and watch for chair communication and side commentary there as well as by audio.
· Generally, do not use video for the teleconferencing calls in order to avoid overloading people’s internet connections; enable only voice and screen sharing.
· Extensive use of screen sharing is encouraged, to enable participants to view the presented material and the meeting notes. At times, multiple sources of screen sharing may be enabled, so it may be necessary for participants to understand that this is happening and to understand how to select which one they want to watch.
[bookmark: _Hlk120812387]It is an established practice that during every JVET meeting that the notes recorded during the sessions are made available and usually updated on a daily basis. The latest version of the notes can be found at the site https://www.itu.int/wftp3/av-arch/jvet-site/ in the folder of the respective meeting. As an example, for the 28th 30th meeting, this would be https://www.itu.int/wftp3/av-arch/jvet-site/2022_10_AB_Mainz/ https://www.itu.int/wftp3/av-arch/jvet-site/2023_04_AD_Antalya/. The latest version of the notes would be document JVET-ABAD_notes_d*.docx, where * stands for the highest number or capital letter. Meeting notes use Microsoft Word’s changemark mode, such that it is straightforward to determine which aspects were discussed on which day of the meeting.
From the side of the ISO/IEC JTC 1/‌SC 29 parent body, JVET is also known as WG WG 5. For those who are registered members of WG WG 5, the following web sites are also relevant, which are password protected (password to be obtained via official ISO channels):
· https://dms.mpeg.expert/ is a site containing WG WG 5 input and output documents (with input documents being copies of the corresponding JVET documents), as well as those of other MPEG working groups.
· https://sd.iso.org/ is a site from which you retrieve WG WG 5 output documents, manage organizational tasks related to your committee membership, register for meetings, etc.

[bookmark: _Ref123670844]Software
Reference and exploration software is developed using the git distributed version control system. Software repositories are hosted on a GitLab server, which is located at https://vcgit.hhi.fraunhofer.de
The registration and development workflow isare documented at:
https://vcgit.hhi.fraunhofer.de/jvet/VVCSoftware_VTM/wikis/VVC-Software-Development-Workflow
Although the development process is described in the context of the VTM software, it can be applied to all other software projects hosted on the GitLab server as well.
The following reference software packages are being developed:
· VTM (VVC): https://vcgit.hhi.fraunhofer.de/jvet/VVCSoftware_VTM
· HM (HEVC): https://vcgit.hhi.fraunhofer.de/jvet/HM
· SHM (SHVC): https://vcgit.hhi.fraunhofer.de/jvet/SHM
· HTM (3D-HEVC, MV-HEVC): https://vcgit.hhi.fraunhofer.de/jvet/HTM
· JM (AVC): https://vcgit.hhi.fraunhofer.de/jvet/JM
· JSVM (SVC): https://vcgit.hhi.fraunhofer.de/jvet/jsvm
· JMVC (MVC): https://vcgit.hhi.fraunhofer.de/jvet/jmvc
· 3DV-ATM reference software (3D-AVC): https://vcgit.hhi.fraunhofer.de/jvet/3dv-atm
The following packages are developed for use in combination with reference software:
· 360Lib (for HEVC and VVC): https://vcgit.hhi.fraunhofer.de/jvet/360lib
· HDRTools: https://gitlab.com/standards/HDRTools
The following exploration software packages are developed:
· ECM: https://vcgit.hhi.fraunhofer.de/ecm/ECM
· NNVC: https://vcgit.hhi.fraunhofer.de/jvet-ahg-nnvc/VVCSoftware_VTM
· SADL library for NNVC: https://vcgit.hhi.fraunhofer.de/jvet-ahg-nnvc/sadl
Read access to all listed git repositories is public. For contributing to the software, users must register for an account and ask the software coordinators to convert it to an “internal” account. After conversion, the target repository can be forked into the personal project space and “merge requests” can be used to contribute software changes.
Reference software is aligned with the associated video coding standard. Technical changes to the decoder need to be proposed to the appropriate standard. Algorithmic changes to the encoder, that have influence on coding performance shall also be proposed to a JVET meeting. Software shall be provided by proponents for all adopted technical proposals within one meeting cycle. Smaller optimizations, bug fixes and cleanups don’t need to be proposed and inclusion into the software will be decided by the appointed software coordinators. The software coordinators review all merge requests and decide whether the code is ready to be merged according to the software development guidelines.Software development guidelines can be found in the following documents:
· JVET-N1003 Guidelines for VVC reference software development [K. Sühring]
· JCTVC-H1001 HEVC software guidelines [K. Sühring, D. Flynn, F. Bossen (software coordinators)]
It is noted that the software implementation packages developed by JVET or the former joint groups come with a software copyright license header based on the BSD license with a preceding sentence declaring that other contributor or third party rights, including patent rights, are not granted by the license. This has been recorded in N 10791 of the 89th meeting of ISO/IEC JTC 1/‌SC 29/‌WG 11, and has been agreed upon by both parent bodies of JVET. Both ITU and ISO/IEC will be identified in the <OWNER> and <ORGANIZATION> tags in the header. It is further noted that software packages or parts thereof might have been publishes or may be published by ITU-T and ISO/IEC as example implementations of a video coding standards, and for use as the basis of products to promote adoption of such technology.
Conformance test data
The procedure to exchange the bitstream (ftp site, bitstream files, etc.) is specified in Sec 2 “Procedure” of JVET-R2008. The ftp and http sites for downloading bitstreams are
· VVC:
	ftp://ftp3.itu.int/jvet-site/bitstream_exchange/VVC 
	https://www.itu.int/wftp3/av-arch/jvet-site/bitstream_exchange/VVC/
· VVC operation range extensions:
	ftp://ftp3.itu.int/jvet-site/bitstream_exchange/VVCv2 
	https://www.itu.int/wftp3/av-arch/jvet-site/bitstream_exchange/VVCv2

The ftp site for uploading bitstream file is as follows.
	ftp://ftp3.itu.int/jvet-site/dropbox/
	(user id: avguest, passwd: Avguest201007)
If using FileZilla, the following configuration is suggested: 

[image: ]
In the Filezilla Edit  Settings  Connection menu, it may also be necessary to set the minimum TLS level to 1.0.
Ed. note: This should be made more complete regarding conformance bitstreams of HEVC at least
Bug tracking
Three different bug tracking system are currently used:
· Mantis bug tracker for the JM (AVC) reference software
· Trac bug tracker for HEVC and VVC related specification text, reference software and conformance specification
· GitLab integrated bug trackers for all other software projects including exploration work
Registration is required for reporting bugs. Each of these tracking systems uses separate accounts. All Trac instances share the same accounts, but registration is only available at the HEVC bug tracker at https://hevc.hhi.fraunhofer.de/trac/hevc
The appropriate bug tracker for software projects can be found going to the software repository listed in section 3 and following the link titled “issues” or “custom issue tracker” in the left side menu.
Specification issues can be reported to the following trackers”
· for VVC at https://jvet.hhi.fraunhofer.de/trac/vvc
· for HEVC at https://hevc.hhi.fraunhofer.de/trac/hevc
· for MV-HEVC and 3D-HEVC at https://hevc.hhi.fraunhofer.de/trac/3d-hevc
· for SHVC at https://hevc.hhi.fraunhofer.de/trac/shvc
Conformance issues can be reported
· for VVC at https://jvet.hhi.fraunhofer.de/trac/vvc

Test sequence materials
The test sequences used by JVET (and previous joint groups such as JCT-VC, JCT-3V, and JVT) for CTC, as well as test sequences used for other purposes (e.g., calls for proposals or core experiments), are available on ftp://jvet@ftp.ient.rwth-aachen.de (accredited members of JVET may contact the JVET chair for login information). A mirror of this site is provided at  with the same login ID but a different password.
Due to copyright restrictions, the JVET database of test sequences is only available for purposes of developing video compression standards of ITU-T and ISO/IEC.

0. Test materials available for JVET
The list of test sequences available for CTC are as follows. Due to copyright restrictions, the JVET database of test sequences is only available to accredited members of JVET (i.e., members of ISO/IEC MPEG and ITU-T VCEG). Test sequences are made available only to qualified JVET participants. Qualified participants may contact the JVET chairs for login information. Specific license information is provided with each test sequence.
0. VVC CTC sequences for SDR video
Test sequences are available on ftp://jvet@ftp.ient.rwth-aachen.de and ftp://jvet@ftp.hhi.fraunhofer.de in the “ctc/sdr” folder.

	Class
	Sequence name
	Frame count
	Frame rate
	Bit depth

	A1
	Tango2
	294
	60
	10

	A1
	FoodMarket4
	300
	60
	10

	A1
	Campfire
	300
	30
	10

	A2
	CatRobot
	300
	60
	10

	A2
	DaylightRoad2
	300
	60
	10

	A2
	ParkRunning3
	300
	50
	10

	B
	MarketPlace
	600
	60
	10

	B
	RitualDance
	600
	60
	10

	B
	Cactus
	500
	50
	8

	B
	BasketballDrive
	500
	50
	8

	B
	BQTerrace
	600
	60
	8

	C
	RaceHorses
	300
	30
	8

	C
	BQMall
	600
	60
	8

	C
	PartyScene
	500
	50
	8

	C
	BasketballDrill
	500
	50
	8

	D
	RaceHorses
	300
	30
	8

	D
	BQSquare
	600
	60
	8

	D
	BlowingBubbles
	500
	50
	8

	D
	BasketballPass
	500
	50
	8

	E
	FourPeople
	600
	60
	8

	E
	Johnny
	600
	60
	8

	E
	KristenAndSara
	600
	60
	8

	F
	ArenaOfValor
	600
	60
	8

	F
	BasketballDrillText
	500
	50
	8

	F
	SlideEditing
	300
	30
	8

	F
	SlideShow
	500
	20
	8



0. VVC CTC sequences for HDR video
Test sequences are available on ftp://jvet@ftp.ient.rwth-aachen.de/ctc/hdr/. Test sequences are made available only to qualified JVET participants. Qualified participants may contact the JVET chairs for login information. Specific license information is provided with each test sequence.

	Class
	Sequence name
	Frame count
	Frame rate
	Bit depth
	Transfer function

	H1
	BalloonFestival 
	240
	24 fps
	10
	PQ

	H1
	Cosmos1_TreeTrunk
	240
	24 fps
	10
	PQ

	H1
	EBU_Hurdles
	500
	50 fps
	10
	PQ

	H1
	EBU_Starting
	500
	50 fps
	10
	PQ

	H1
	Market
	400
	50 fps
	10
	PQ

	H1
	ShowGirl
	339
	25 fps
	10
	PQ

	H1
	SunRise
	200
	25 fps
	10
	PQ


Note: The test sequences from the EBU (i.e. with the string ‘EBU’ included in the test sequence name) are password protected.  The password can be obtained by contacting the EBU using the form located at:
https://tech.ebu.ch/EBU_SVT_Public_Test_Sequences

Note: The capture frame rate of the EBU_Hurdles and EBU_Starting sequences was 100fps. However, these sequences are treated as 50fps sequences for the evaluation processes defined in this document.

	Class
	Sequence name
	Frame count
	Frame rate
	Bit depth
	Transfer function

	H2
	DayStreet2
	300
	60 fps
	10
	HLG

	H2
	FlyingBirds3
	300
	60 fps
	10
	HLG

	H2
	PeopleInShoppingCenter2
	300
	60 fps
	10
	HLG

	H2
	SunsetBeach3
	300
	60 fps
	10
	HLG



0. VVC CTC sequences for 360° video
Test sequences are available on ftp://jvet@ftp.ient.rwth-aachen.de/testsequences/testset360 and ftp://jvet@ftp.hhi.fraunhofer.de/testsequences/testset360

	Class
	Sequence name
	Width
	Height
	Frame count
	Frame rate
	Bit depth

	S1
	SkateboardInLot
	8192
	4096
	300
	30 fps
	10

	S1
	ChairLift
	8192
	4096
	300
	30 fps
	10

	S1
	KiteFlite
	8192
	4096
	300
	30 fps
	8

	S1
	Harbor
	8192
	4096
	300
	30 fps
	8

	S1
	Trolley
	8192
	4096
	300
	30 fps
	8

	S1
	GasLamp
	8192
	4096
	300
	30 fps
	8

	S2
	Balboa
	6144
	3072
	600
	60 fps
	8

	S2
	Broadway
	6144
	3072
	600
	60 fps
	8

	S2
	Landing2
	6144
	3072
	300
	30 fps
	8

	S2
	BranCastle2
	6144
	3072
	300
	30 fps
	8



0. HEVC v.1 CTC sequences
Test sequences are available on ftp://hevc@mpeg.tnt.uni-hannover.de/testsequences/ 

	Class
	Sequence name
	Width x Height
	Frame count
	Frame rate
	Bit depth

	A
	Traffic
	2560x1600
	150
	30 fps
	8

	A
	PeopleOnStreet
	2560x1600
	150
	30 fps
	8

	A
	Nebuta
	2560x1600
	300
	60 fps
	10

	A
	SteamLocomotive
	2560x1600
	300
	60 fps
	10

	B
	Kimono
	1920x1080
	240
	24 fps
	8

	B
	ParkScene
	1920x1080
	240
	24 fps
	8

	B
	Cactus
	1920x1080
	500
	50 fps
	8

	B
	BQTerrace
	1920x1080
	600
	60 fps
	8

	B
	BasketballDrive
	1920x1080
	500
	50 fps
	8

	C
	RaceHorses
	832x480
	300
	30 fps
	8

	C
	BQMall
	832x480
	600
	60 fps
	8

	C
	PartyScene
	832x480
	500
	50 fps
	8

	C
	BasketballDrill
	832x480
	500
	50 fps
	8

	D
	RaceHorses
	416x240
	300
	30 fps
	8

	D
	BQSquare
	416x240
	600
	60 fps
	8

	D
	BlowingBubbles
	416x240
	500
	50 fps
	8

	D
	BasketballPass
	416x240
	500
	50 fps
	8

	E
	FourPeople
	1280x720
	600
	60 fps
	8

	E
	Johnny
	1280x720
	600
	60 fps
	8

	E
	KristenAndSara
	1280x720
	600
	60 fps
	8

	F
	BaskeballDrillText
	832x480
	500
	50 fps
	8

	F
	ChinaSpeed
	1024x768
	500
	30 fps
	8

	F
	SlideEditing
	1280x720
	300
	30 fps
	8

	F
	SlideShow
	1280x720
	500
	20 fps
	8


0. HEVC v.1 verification test sequences
The following test sequences that were used in the verification test reported in JCTVC-Q1011 have only been available from the content owners on a case-by-case basis. Information is hereby solicited regarding how to obtain them and whether or not they can be made available in our test sequence database.

	Class
	Sequence name
	Width x Height
	Frame count
	Frame rate
	Bit depth

	UHD
	BT709Birthday
	3840x2160
	500
	50 fps
	8

	UHD
	Book
	3840x2160
	500
	50 fps
	8

	UHD
	Manage
	3840x2160
	600
	60 fps
	8

	UHD
	HomelessSleeping
	3840x2160
	600
	60 fps
	8

	UHD
	Traffic
	4096x2048
	300
	30 fps
	8

	1080p
	JohnnyLobby
	1920x1080
	600
	60 fps
	8

	1080p
	Calendar
	1920x1080
	500
	50 fps
	8

	1080p
	SVT15
	1920x1080
	500
	50 fps
	8

	1080p
	sedofCropped
	1920x1080
	600
	60 fps
	8

	1080p
	UnderBoat1
	1920x1080
	300
	30 fps
	8

	720p
	ThreePeople
	1280x720
	600
	60 fps
	8

	720p
	BT709Parakeets
	1280x720
	500
	50 fps
	8

	720p
	QuarterBackSneak1
	1280x720
	300
	30 fps
	8

	720p
	SVT01a
	1280x720
	500
	50 fps
	8

	720p
	SVT04a
	1280x720
	500
	50 fps
	8

	480p
	Cubicle
	832x480
	300
	30 fps
	8

	480p
	Anemone
	832x480
	300
	30 fps
	8

	480p
	BT709BirthdayFlash
	832x480
	500
	50 fps
	8

	480p
	Ducks
	832x480
	600
	60 fps
	8

	480p
	WheelAndCalendar
	832x480
	500
	50 fps
	8



0. HEVC Range Extensions CTC sequences
Test sequences are available on ftp://hevc@mpeg.tnt.uni-hannover.de/testsequences/FrExt-candidate-sequences/ 

	Sequence name
	Width x Height
	Frame count
	Frame rate
	Bit depth

	Traffic
	2560x1600
	150
	30 fps
	12

	Traffic
	2560x1600
	150
	30 fps
	10

	Kimono
	1920x1080
	240
	24 fps
	10

	EBULupoCandlelight (down conv.)
	1920x1080
	500
	50 fps
	10

	EBURainFruits (down conv.)
	1920x1080
	500*
	50 fps
	10

	EBUHorse
	1920x1080
	500
	50 fps
	10

	EBUGraphics
	1920x1080
	500
	50 fps
	10

	EBUWaterRocksClose
	1920x1080
	500
	50 fps
	10

	EBUKidsSoccer
	1920x1080
	500
	50 fps
	10

	VenueVu
	1920x1080
	300
	30 fps
	8

	VenueVu
	1920x1080
	300
	30 fps
	10

	DucksAndLegs
	1920x1080
	300
	30 fps
	10

	BirdsInCage
	1920x1080
	600
	60 fps
	10

	OldTownCross
	1920x1080
	500
	50 fps
	10

	CrowdRun
	1920x1080
	500
	50 fps
	10

	Seeking
	1920x1080
	500
	50 fps
	10

	ParkScene
	1920x1080
	240
	24 fps
	10


A number of the new sequences were kindly provided by the EBU. 
Note that test sequences from the EBU (i.e. with the string ‘EBU’ included in the test sequence name) are password protected.  The password can be obtained by contacting the EBU using the form located at:
https://tech.ebu.ch/EBU_SVT_Public_Test_Sequences

0. [bookmark: _Ref377730219]High bit-depth coding test sequences


	Class
	Test sequence filename
	Encoded frame count
	Input bit-depth
	MSB extended bit-depth

	
	
	AI
	LD
	
	

	SVT
16 bit from 10 bit source
(intermediate processing)
	OldTownCross_1920x1080_50_16bit_444.rgb
OldTownCross_RGB_16bit.cfg
	50
	50
	16
	0

	
	CrowdRun_1920x1080_50_16bit_444.rgb
CrowdRun_RGB_16bit.cfg
	50
	50
	16
	0

	
	DucksTakeOff_1920x1080_50_16bit_444.rgb
DucksTakeOff_RGB_16bit.cfg
	50
	-
	16
	0

	
	InToTree_1920x1080_50_16bit_444.rgb
InToTree_RGB_16bit.cfg
	50
	[bookmark: _Ref374030714]-
	16
	0

	
	ParkJoy_1920x1080_50_16bit_444.rgb
ParkJoy_RGB_16bit.cfg
	50
	-
	16
	0

	IBDI 4:4:4
	Traffic_2560x1600_30_12bit_444_crop.rgb
Traffic_RGB_12bit.cfg
	60
	60
	12
	0

	16 bit HDR
	FruitStall_1920x1080_24_16bit_444.rgb
FruitStall_RGB_16bit.cfg
	120
	120
	16
	0

	16 bit from 16 bit HDR source
	Bubbles_4096x2160_24_16bit_444.rgb
Bubbles_RGB_16bit.cfg
	60
	-
	16
	0

	16 bit HDR 4:0:0 Medical
	AX_Head_1240x960_16bit_400.yuv
Head_400_16bit.cfg
	250
	250
	16
	0

	IBDI 4:0:0
	CT_ Cardiac_512x512_12bit_400.yuv
Cardiac_400_12bit.cfg
	250
	250
	12
	0

	
	CT_ LongrunShort_512x512_12bit_400.yuv
LongRunShort_400_12bit.cfg
	500
	500
	12
	0

	Synthesised RGB HDR
	EBURainFruits_1920x1080_50_10bit_444.rgb
EBURainFruits_RGB_10bit+2MSB.cfg
EBURainFruits_RGB_10bit+4MSB.cfg
EBURainFruits_RGB_10bit+6MSB.cfg
	50
	50
	10
	12,14,16

	
	Kimono1_1920x1080_24_10bit_444.rgb
Kimono_RGB_10bit+2MSB.cfg
Kimono_RGB_10bit+4MSB.cfg
Kimono_RGB_10bit+6MSB.cfg
	60
	-
	10
	12,14,16


For test sequences in the “16 bit HDR 4:0:0 Medical” and “IBDI 4:0:0” classes, the frame rate is set to 50, even though the test sequences do not have an inherent frame rate.

0. HEVC screen content sequences
Test sequences are available on ftp://ftp.ient.rwth-aachen.de/ctc/hevc-scc/. Some of the sequences are located in the N0294_Gaming and TongJiYUVRevision_02-24-2013, among other subdirectories. The last two tables shown below contain sequences used for the common conditions for screen content coding tests, as specified in JCTVC-U1015.

	JCT-VC number
	sequence name
	frames

	L0301
	sc_map_1280x720_60_8bit
	600

	
	sc_programming_1280x720_60_8bit
	600

	
	sc_wordEditing_1280x720_60_8bit
	600

	
	
	

	L0317
	sc_cad_waveform_1920x1080_20_8bit_200_r1
	200

	
	sc_cg_twist_tunnel_1280x720_30_8bit_300_r1
	300

	
	sc_pcb_layout_1920x1080_20_8bit_200_r1
	200

	
	sc_ppt_doc_xls_1920x1080_20_8bit_200_r1
	200

	
	sc_video_conferencing_doc_sharing_1280x720_30_8bit_300_r1
	300

	
	sc_web_browsing_1280x720_30_8bit_300_r1
	300

	
	
	

	M0431
	sc_doc_1280x720_10_8bit_500
	500

	
	sc_SlideShow_1280x720_20_8bit_500
	500

	
	sc_Web_1280x720_10_8bit_500
	500

	
	
	

	N0294
	sc_robot_1280x720_30_8bit_300
	300

	
	sc_viking_1280x720_30_8bit_300
	300

	
	
	

	O0222
	Basketball_Screen_2560x1440_60p_8b
	623

	
	BigBuck_1920x1080_60p_8b
	404

	
	KimonoError1_2560x1440_60p_8b
	1006

	
	KimonoError2_2560x1440_60p_8b
	516

	
	KristenAndSaraScreen_1920x1080_60p_8b
	604

	
	MissionControlClip1_2560x1440_60p_8b
	601

	
	MissionControlClip2_2560x1440_60p_8b
	600

	
	MissionControlClip3_1920x1080_60p_8b
	603

	
	
	

	O0256
	sc_console_1920x1080_60_8bit
	600

	
	sc_desktop_1920x1080_60_8bit
	600

	
	sc_flyingGraphics_1920x1080_60_8bit
	600

	
	sc_realtimeData_1920x1080_60_8bit
	600

	
	sc_socialNetworkMap_1920x1080_60_8bit
	601

	
	sc_videoTesting_1920x1080_60_8bit
	601

	
	
	

	O0268
	sc_cg2twist_tunnel_1280x720_30_8bit
	300

	
	
	

	JVET-C0044
	BitstreamAnalyzer_1920x1080_30_8bit
	300

	
	ChineseDocumentEditing_1920x1080_30_8bit
	300

	
	CircuitLayoutPresentation_1920x1080_30_8bit
	300

	
	ClearTypeSpreadsheet_1920x1080_30_8bit
	300

	
	EnglishDocumentEditing_1920x1080_30_8bit
	300

	
	
	

	Others
	sc_VenueVu_1920x1080_30_8bit1
	300



1The YCbCr and RGB VenueVue sequences can be found with the Range Extensions sequences on the FTP site.

	Resolution
	Sequence name
	Category
	fps
	Frames to be encoded

	1920x1080
	sc_flyingGraphics_1920x1080_60_8bit*
sc_desktop_1920x1080_60_8bit
sc_console_1920x1080_60_8bit
ChineseEditing_1920x1080_60_8bit
MissionControlClip3_1920x1080_60p_8b444
EBURainFruits_1920x1080_50_10bit**
Kimono1_1920x1080_24_10bit***
	TGM
TGM
TGM
TGM
M
CC
CC
	60
60
60
60
60
50
24
	0-299*
0-599
0-599
0-599
0-599
0-249**
0-119***

	1280x720
	sc_web_browsing_1280x720_30_8bit
sc_map_1280x720_60_8bit
sc_programming_1280x720_60_8bit
sc_SlideShow_1280x720_20_8bit
sc_robot_1280x720_30_8bit
	TGM
TGM
TGM
TGM
A
	30
60
60
20
30
	0-299
0-599
0-599
0-499
0-299

	2560x1440
	Basketball_Screen_2560x1440_60p_8b444
MissionControlClip2_2560x1440_60p_8444
	M
M
	60
60
	322-621
120-419

	*Note that only the first 300 frames of this sequence are used.
**Note that only the first 250 frames of this 10-bit sequence are used, and InternalBitDepth is set to 8.
***Note that only the first 120 frames of this 10-bit sequence are used, and InternalBitDepth is set to 8
TGM: Text and graphics with motion; M: mixed content; A: animation; CC: camera-captured content




	Resolution
	Sequence name
	Category
	fps
	Frames to be encoded

	1920x1080
	sc_flyingGraphics_1920x1080_60_8bit_420*
sc_desktop_1920x1080_60_8bit_420
sc_console_1920x1080_60_8bit_420
ChineseEditing_1920x1080_60_8bit_420
MissionControlClip3_1920x1080_60p_8b420
	4:2:0 TGM
4:2:0 TGM
4:2:0 TGM
4:2:0 TGM
4:2:0 M
	60
60
60
60
60
	0-299*
0-599
0-599
0-599
0-599

	1280x720
	sc_web_browsing_1280x720_30_8bit_420_r1
sc_map_1280x720_60_8bit_420
sc_programming_1280x720_60_8bit_420
SlideShow_1280x720_20
sc_robot_1280x720_30_8bit_420
	4:2:0 TGM
4:2:0 TGM
4:2: 0TGM
4:2:0 TGM
4:2:0 A
	30
60
60
20
30
	0-299
0-599
0-599
0-499
0-299

	2560x1440
	Basketball_Screen_2560x1440_60p_8b420
MissionControlClip2_2560x1440_60p_8420
	4:2:0 M
4:2:0 M
	60
60
	322-621
120-419

	1024x768
	ChinaSpeed_1024x768_30
	4:2:0 A
	30
	0-499

	*Note that only the first 300 frames of this sequence are used.
TGM: Text and graphics with motion; M: mixed content; A: animation; CC: camera-captured content


0. HEVC HDR sequences
HDR test sequences to be used for HDR-related experiments are listed in document “Common Test Conditions for HDR/WCG video coding experiments”, JCTVC-Z1020. Some of the sequences are available on ftp://jvet@ftp.ient.rwth-aachen.de in directory “/testsequences/testset_hdr” (accredited members of JCT-VC may contact the JCT-VC chairs for login information). 
Some of the sequences mentioned in JCTVC-Z1020 are only available upon request to the content owner, as described in Annex B of JCTVC-Z1020.
The following sequences are available:
	Resolution  
	gamut 
	TF
	Sequence name
	fps
	Frames

	1920x1080
	BT.709
	Linear
	FireEater2Clip4000r1_1920x1080p_25_hf_709_ct2020_444_xxx.exr 
	25
	0-199

	1920x1080
	BT.709
	Linear
	Market3Clip4000r2_1920x1080p_50_hf_709_ct2020_444_xxx.exr
	50
	0-399

	1920x1080
	BT.709
	Linear
	BalloonFestival_1920x1080p_24_hf_709_ct2020_444_xxx.exr
	24
	0-239

	1920x1080
	BT.709
	Linear
	EBU_04_Hurdles_1920x1080p_25_hf_709_ct2020_444_xxx.exr
	100
	0-499

	1920x1080
	BT.709
	Linear
	EBU_06_Starting_1920x1080p_25_hf_709_ct2020_444_xxx.exr
	100
	0-499

	1920x1080
	BT.709
	Linear
	Sunrise_1920x1080p_25_hf_709_ct2020_444_xxx.exr
	25
	0-199



These sequences are provided in EXR format, Y'CbCr 10-bit 4:2:0 with BT.2100 PQ transfer function and BT.2020 color primaries, and a Y'CbCr 10-bit 4:2:0 SDR with BT.709 color primaries version is also available for each content.
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