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Abstract
This contribution summarizes the crosschecking results of JVET-AG0158 EE2-4.3: Adaptive precision for luma ALF coefficients. It is reported that the results matched what provided by the proponent.
Introduction
In JVET-AG0158 EE2-4.3, the number of bits used to represent the fractional part of a luma ALF coefficient can vary from 5 to 8 adaptively. This document reports the cross check results of it.
Results
The EE2-4.3 tests are implemented based on the ECM-11.0[1] reference software. The simulation was conducted under the ECM CTC[2].
Table 1. EE2-4.3 vs ECM-11.0
	
	All Intra Main 10 

	
	Over ECM-11.0

	
	Y
	U
	V
	EncT
	DecT
	EncVmPeak
	DecVmPeak

	Class A1
	-0.01%
	0.00%
	0.00%
	100.4%
	100.9%
	100.1%
	100.0%

	Class A2
	#VALUE!
	#VALUE!
	#VALUE!
	#DIV/0!
	#DIV/0!
	#DIV/0!
	#DIV/0!

	Class B
	-0.03%
	0.00%
	0.00%
	99.8%
	99.9%
	100.1%
	100.0%

	Class C
	-0.07%
	0.00%
	0.00%
	99.8%
	99.5%
	99.9%
	100.0%

	Class E
	-0.05%
	0.00%
	0.00%
	99.8%
	99.5%
	100.2%
	100.0%

	Overall 
	#VALUE!
	#VALUE!
	#VALUE!
	#DIV/0!
	#DIV/0!
	#DIV/0!
	#DIV/0!

	Class D
	-0.07%
	0.02%
	0.02%
	97.5%
	98.9%
	100.1%
	100.0%

	Class F
	-0.06%
	0.03%
	0.03%
	101.1%
	100.6%
	100.2%
	100.0%

	Class TGM
	#VALUE!
	#VALUE!
	#VALUE!
	#DIV/0!
	#DIV/0!
	#DIV/0!
	#DIV/0!

	
	
	
	
	
	
	
	

	
	Random Access Main 10

	
	Over ECM-11.0

	
	Y
	U
	V
	EncT
	DecT
	EncVmPeak
	DecVmPeak

	Class A1
	#VALUE!
	#VALUE!
	#VALUE!
	#DIV/0!
	#DIV/0!
	#DIV/0!
	#DIV/0!

	Class A2
	#VALUE!
	#VALUE!
	#VALUE!
	#DIV/0!
	#DIV/0!
	#DIV/0!
	#DIV/0!

	Class B
	-0.08%
	-0.02%
	-0.10%
	99.7%
	101.0%
	99.5%
	100.0%

	Class C
	-0.12%
	-0.09%
	-0.01%
	98.3%
	100.6%
	98.9%
	100.1%

	Class E
	　
	
	　
	　
	
	　
	　

	Overall
	#VALUE!
	#VALUE!
	#VALUE!
	#DIV/0!
	#DIV/0!
	#DIV/0!
	#DIV/0!

	Class D
	-0.13%
	0.13%
	-0.01%
	92.5%
	99.5%
	99.9%
	100.0%

	Class F
	#VALUE!
	#VALUE!
	#VALUE!
	#DIV/0!
	#DIV/0!
	#DIV/0!
	#DIV/0!

	Class TGM
	#VALUE!
	#VALUE!
	#VALUE!
	#DIV/0!
	#DIV/0!
	#DIV/0!
	#DIV/0!



Conclusion
The crosschecker’s results can match proponent’s results. 
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