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Abstract
This contribution proposes a new SEI message for conveying Region-dependent film grain characteristics. It is a unified proposal based on contributions JVET-AG0140, JVET-AG0215 and JVET-AG0101. The proposal describes a region-dependent film grain characteristics SEI message, that includes the existing FGC SEI message syntax, notably independent intensity intervals with model parameters for each interval and adds elements to describe a list of picture regions, and associate each region with a set of intervals. 
If agreeable by the group, it is proposed to document this proposed solution in the TuC so that proponents can use it for running experiments as requested during the 1st presentation of the different contributions.
The proponents will provide a software implementation of the proposed SEI.
Introduction
Following the review of contributions JVET-AG0140, JVET-AG0215 and JVET-AG0101 on Region-dependent film grain characteristics SEI message, it was recommended to unify the SEI message. This proposal provides the syntax and semantics of a proposed unified solution that will serve as reference for developping a software implementation of the proposed functionality as requested by the group. 
Proposal
It is proposed to create a new region-dependent film grain characteristics SEI message, that reuses the same syntax (and semantics) as the FGC SEI message to list all intervals needed for the whole picture.
Two modes are supported, a rectangular regions adaptation mode, and an alpha channel adaptation mode.
When rectangular regions adaptation mode is enabled, the SEI message lists picture regions (rectangular areas, for example A, B and C in Figure 1) and associate sets of intervals with each region. Several regions can use the same set of intervals (e.g. B and C), and some intervals can be reused in different sets (in Figure 2, a few intervals are used by A, B, and C).
[image: ]
[bookmark: _Ref155865575]Figure 1 – Video with regions A, B and C (e.g. different sources with different grain)
[image: ]
[bookmark: _Ref155865776]Figure 2 – Associating sets of intervals with regions

When rectangular regions adaptation mode is disabled, film grain is generated for the full picture as done with the FGS SEI. In this later case, alpha channel map can be used to modulate the generated film grain when alpha channel adaptation mode is enabled. 
Syntax and semantics
Film grain regions characteristics syntax
[Editor’s notes: 
· the Grey highlighted text is a replicate of the FGC SEI message as defined in 8.5 of VSEI, with prefix “fg” replaced by “fgr”
· the Blue-highlighted text is specific to the use of the alpha map as an alternate approach of the region-based option]

	film_grain_regions_characteristics( payloadSize ) {
	Descriptor

		fgr_cancel_flag
	u(1)

		if( !fgr_cancel_flag ) {
	

			fgr_model_id
	u(2)

			fgr_separate_colour_description_present_flag
	u(1)

			if( fgr_separate_colour_description_present_flag ) {
	

				fgr_bit_depth_luma_minus8
	u(3)

				fgr_bit_depth_chroma_minus8
	u(3)

				fgr_full_range_flag
	u(1)

				fgr_colour_primaries
	u(8)

				fgr_transfer_characteristics
	u(8)

				fgr_matrix_coeffs
	u(8)

			}
	

			fgr_blending_mode_id
	u(2)

			fgr_log2_scale_factor
	u(4)

			for( c = 0; c < 3; c++ )
	

				fgr_comp_model_present_flag[ c ]
	u(1)

			for( c = 0; c < 3; c++ )
	

				if( fgr_comp_model_present_flag[ c ] ) {
	

					fgr_num_intensity_intervals_minus1[ c ]
	u(8)

					fgr_num_model_values_minus1[ c ]
	u(3)

					for( i = 0; i  <=  fgr_num_intensity_intervals_minus1[ c ]; i++ ) {
	

						fgr_intensity_interval_lower_bound[ c ][ i ]
	u(8)

						fgr_intensity_interval_upper_bound[ c ][ i ]
	u(8)

						for( j = 0; j  <=  fgr_num_model_values_minus1[ c ]; j++ )
	

							fgr_comp_model_value[ c ][ i ][ j ]
	se(v)

					}
	

				}
	

			fgr_region_information_present_flag
	u(1)

			if( fgr_region_information_present_flag ) {
	

				fgr_region_based_adaptation_flag
	u(1)

				if( fgr_region_based_adaptation_flag ) {
	

					fgr_active_regions_number_minus1
	u(8)

					for( i = 0; i <= fgr_active_regions_number_minus1; i++ ) {
	

						fgr_region_top[ i ]
	u(16)

						fgr_region_left[ i ]
	u(16)

						fgr_region_width[ i ]
	u(16)

						fgr_region_height[ i ]
	u(16)

			fgr_film_grain_enabled_flag[ i ]
	u(1)

					if  ( fgr_film_grain_enabled_flag[ i ] ) {
	

					for( c = 0; c < 3; c++ )
	

						if ( fgr_comp_model_present_flag[ c ] ) {
	

							fgr_region_interval_min[ i ][ c ]
	u(8)

							fgr_region_interval_max[ i ][ c ]
	u(8)

						}
	

						}
	

					}
	

				}
	

				else
	

					fgr_alpha_channel_adaptation_flag
	u(1)

			}
	

			fgr _persistence_flag
	u(1)

		}
	

	}
	


Film grain regions characteristics semantics 
This SEI message provides the decoder with a parameterized model for a film grain synthesis process. The film grain synthesis process should be applied to the decoded pictures prior to their display.
Compared to the FGC SEI message defined in 8.5, this SEI message also provides the decoder with parameters defining how to apply locally the film grain synthesis.
Use of this SEI message requires the definition of the following variables:
–	A picture width and picture height in units of luma samples, denoted herein by PicWidthInLumaSamples and PicHeightInLumaSamples, respectively.
–	When the syntax element rdf_separate_colour_description_present_flag of the film grain regions characteristics SEI message is equal to 0, the following additional variables:
–	A chroma format indicator, denoted herein by ChromaFormatIdc, as described in clause 7.3.
–	A bit depth for the samples of the luma component, denoted herein by BitDepthY, and when ChromaFormatIdc is not equal to 0, a bit depth for the samples of the two associated chroma components, denoted herein by BitDepthC.
The film grain models specified in the film grain regions characteristics SEI message are expressed for application to decoded pictures that have 4:4:4 colour format with luma and chroma bit depths corresponding to the luma and chroma bit depths of the film grain model and use the same colour representation domain as the identified film grain model. When the colour format of the decoded video is not 4:4:4 or the decoded video uses a different luma or chroma bit depth from that of the film grain model or uses a different colour representation domain from that of the identified film grain model, an unspecified conversion process is expected to be applied to convert the decoded pictures to the form that is expressed for application of the film grain model.
NOTE 4 – Because the use of a specific method is not required for performing the film grain generation function used by the display process, a decoder could, if desired, down-convert the model information for chroma in order to simulate film grain for other chroma formats (4:2:0 or 4:2:2) rather than up-converting the decoded video (using a method not specified in this Specification) before performing film grain generation.
[Editor’s notes: 
· the Grey highlighted text is a replicate of the FGC SEI message as defined in 8.5 of VSEI, with prefix “fg” replaced by “fgr”
· the Blue-highlighted text is specific to the use of the alpha map as an alternate approach of the region-based option]
fgr_cancel_flag equal to 1 indicates that the SEI message cancels the persistence of any previous film grain regions characteristics SEI message in output order that applies to the current layer. fgr_cancel_flag equal to 0 indicates that film grain regions characteristics follows.
fgr_model_id identifies the film grain simulation model as specified in Table 5. The value of fgr_model_id shall be in the range of 0 to 1, inclusive. The values of 2 and 3 for fgr_model_id are reserved for future use by ITU‑T | ISO/IEC and shall not be present in bitstreams conforming to this version of this Specification. Decoders shall ignore film grain regions characteristics SEI messages with fgr_model_id equal to 2 or 3.
[bookmark: _Ref21912787][bookmark: _Ref81401429][bookmark: _Toc37056126][bookmark: _Ref81401413][bookmark: _Toc246350773][bookmark: _Toc259024422][bookmark: _Toc415476515][bookmark: _Toc501130643][bookmark: _Toc503770651][bookmark: _Toc143862520]Table 5 – fgr_model_id values

	Value
	Description

	0
	Frequency filtering

	1
	Auto-regression


fgr_separate_colour_description_present_flag equal to 1 indicates that a distinct combination of luma bit depth, chroma bit depth, video full range flag, colour primaries, transfer characteristics, and matrix coefficients for the film grain characteristics specified in the SEI message is present in the film grain extension SEI message syntax. fgr_separate_colour_description_present_flag equal to 0 indicates that the combination of luma bit depth, chroma bit depth, video full range flag, colour primaries, transfer characteristics, and matrix coefficients for the film grain characteristics specified in the SEI message are the same as indicated in VUI parameters for the CLVS.
NOTE 5 – When fgr_separate_colour_description_present_flag is equal to 1, any of the luma bit depth, chroma bit depth, video full range flag, colour primaries, transfer characteristics, and matrix coefficients specified for the film grain characteristics specified in the SEI message could differ from that for the pictures in the CLVS.
When VUI parameters are not present for the CLVS or the value of vui_colour_description_present_flag is equal to 0, and equivalent information to that conveyed when vui_colour_description_present_flag is equal to 1 is not conveyed by external means, fgr_separate_colour_description_present_flag shall be equal to 1.
The input image Î, which may be the decoded picture or converted from the decoded picture, used in the equations in this clause is in the same colour representation domain as the simulated film grain signal. Therefore, when any of these parameters does differ from that for the pictures in CLVS, the input image Î used in the equations in this clause would be in a different colour representation domain than that for the pictures in the CLVS. For example, when the value of fgr_bit_depth_luma_minus8 + 8 is greater than BitDepthY (i.e., the bit depth of the luma component of the pictures in the CLVS), the bit depth of the input image Î used in the equations in this clause is also greater than BitDepthY. In such a case, the input image Î would be generated by converting the actual decoded picture to be in the same colour representation domain as the simulated film grain signal. The process for converting an actual decoded picture to the 4:4:4 colour format with same colour representation domain as the simulated film grain signal is not specified in this Specification.
fgr_bit_depth_luma_minus8 plus 8 specifies the bit depth used for the luma component of the film grain characteristics specified in the SEI message. When fgr_bit_depth_luma_minus8 is not present in the film grain extension SEI message, the value of fgr_bit_depth_luma_minus8 is inferred to be equal to BitDepthY − 8.
The value of fgBitDepth[ 0 ] is derived as follows:
fgBitDepth[ 0 ] = fgr_bit_depth_luma_minus8 + 8		(19)
fgr_bit_depth_chroma_minus8 plus 8 specifies the bit depth used for the Cb and Cr components of the film grain characteristics specified in the SEI message. When fgr_bit_depth_chroma_minus8 is not present in the film grain extension SEI message, the value of fgr_bit_depth_chroma_minus8 is inferred to be equal to BitDepthC − 8.
The value of fgBitDepth[ c ] for c = 1 and 2 is derived as follows:
fgBitDepth[ c ] = fgr_bit_depth_chroma_minus8 + 8, with c = 1, 2	(20)
fgr_full_range_flag has the same semantics as specified in clause 7.3 for the vui_full_range_flag syntax element, except as follows:
–	fgr_full_range_flag specifies the video full range flag of the film grain characteristics specified in the SEI message, rather than the video full range flag used for the CLVS.
–	When fgr_full_range_flag is not present in the film grain extension SEI message, the value of fgr_full_range_flag is inferred to be equal to vui_full_range_flag.
fgr_colour_primaries has the same semantics as specified in clause 7.3 for the vui_colour_primaries syntax element, except as follows:
–	fgr_colour_primaries specifies the colour primaries of the film grain characteristics specified in the SEI message, rather than the colour primaries used for the CLVS.
–	When fgr_colour_primaries is not present in the film grain extension SEI message, the value of fgr_colour_primaries is inferred to be equal to vui_colour_primaries.
fgr_transfer_characteristics has the same semantics as specified in clause 7.3 for the vui_transfer_characteristics syntax element, except as follows:
–	fgr_transfer_characteristics specifies the transfer characteristics of the film grain characteristics specified in the SEI message, rather than the transfer characteristics used for the CLVS.
–	When fgr_transfer_characteristics is not present in the film grain extension SEI message, the value of fgr_transfer_characteristics is inferred to be equal to vui_transfer_characteristics.
fgr_matrix_coeffs has the same semantics as specified in clause 7.3 for the vui_matrix_coeffs syntax element, except as follows:
–	fgr_matrix_coeffs specifies the matrix coefficients of the film grain characteristics specified in the SEI message, rather than the matrix coefficients used for the CLVS.
–	When fgr_matrix_coeffs is not present in the film grain extension SEI message, the value of fgr_matrix_coeffs is inferred to be equal to vui_matrix_coeffs.
–	The values allowed for fgr_matrix_coeffs are not constrained by the chroma format of the decoded video pictures that is indicated by the value of ChromaFormatIdc for the semantics of the VUI parameters.
fgr_blending_mode_id identifies the blending mode used to blend the simulated film grain with the input images as specified in Table 6. fgr_blending_mode_id shall be in the range of 0 to 1, inclusive. The values of 2 and 3 for fgr_blending_mode_id are reserved for future use by ITU‑T | ISO/IEC and shall not be present in bitstreams conforming to this version of this Specification. Decoders shall ignore film grain characteristic SEI messages with fgr_blending_mode_id equal to 2 or 3.
[bookmark: _Ref21912961][bookmark: _Ref81401515][bookmark: _Toc246350774][bookmark: _Toc259024423][bookmark: _Toc415476516][bookmark: _Toc501130644][bookmark: _Toc503770652][bookmark: _Toc143862521]Table 6 – fgr_blending_mode_id values

	Value
	Description

	0
	Additive

	1
	Multiplicative



Depending on the value of fgr_blending_mode_id, the blending mode is specified as follows:
–	If fgr_blending_mode_id is equal to 0, the blending mode is additive as specified by:
Igrain[ c ][ x ][ y ] = Clip3( 0, ( 1  <<  fgBitDepth[ c ] ) − 1, Î[ c ][ x ][ y ] + G[ c ][ x ][ y ] )	(21)
–	Otherwise (fgr_blending_mode_id is equal to 1), the blending mode is multiplicative as specified by:
Igrain[ c ][ x ][ y ] = Clip3( 0, ( 1  <<  fgBitDepth[ c ] ) − 1, Î[ c ][ x ][ y ] +	(22)
			Round( ( Î[ c ][ x ][ y ] * G[ c ][ x ][ y ] ) ÷ ( ( 1  <<  fgBitDepth[ c ] ) − 1 ) ) )
where Î[ c ][ x ][ y ] represents the sample value at coordinates x, y of the colour component c of the input image Î, G[ c ][ x ][ y ] is the simulated film grain value at the same position and colour component, and fgBitDepth[ c ] is the number of bits used for each sample in a fixed-length unsigned binary representation of the arrays Igrain[ c ][ x ][ y ], Î[ c ][ x ][ y ], and G[ c ][ x ][ y ], where c = 0..2, x = 0..PicWidthInLumaSamples − 1, and y = 0..PicHeightInLumaSamples − 1.
fgr_log2_scale_factor specifies a scale factor used in the film grain characterization equations.
fgr_comp_model_present_flag[ c ] equal to 0 indicates that film grain is not modelled on the c-th colour component, where c equal to 0 refers to the luma component, c equal to 1 refers to the Cb component, and c equal to 2 refers to the Cr component. fgr_comp_model_present_flag[ c ] equal to 1 indicates that syntax elements specifying modelling of film grain on colour component c are present in the SEI message.
When fgr_separate_colour_description_present_flag is equal to 0 and ChromaFormatIdc is equal to 0, the value of fgr_comp_model_present_flag[ 1 ] and fgr_comp_model_present_flag[ 2 ] shall be equal to 0.
fgr_num_intensity_intervals_minus1[ c ] plus 1 specifies the number of intensity intervals for which a specific set of model values has been estimated.
NOTE 6 – The intensity intervals could overlap in order to simulate multi-generational film grain.
fgr_num_model_values_minus1[ c ] plus 1 specifies the number of model values present for each intensity interval in which the film grain has been modelled. The value of fgr_num_model_values_minus1[ c ] shall be in the range of 0 to 5, inclusive.
fgr_intensity_interval_lower_bound[ c ][ i ] specifies the lower bound of the i-th intensity interval for which the set of model values applies.
fgr_intensity_interval_upper_bound[ c ][ i ] specifies the upper bound of the i-th intensity interval for which the set of model values applies.
The variable intensityIntervalIdx[ c ][ x ][ y ][ j ] represents the j-th index to the list of intensity intervals selected for the sample value Î[ c ][ x ][ y ] for c = 0..2, x = 0..PicWidthInLumaSamples − 1, y = 0..PicHeightInLumaSamples − 1, and j = 0..numApplicableIntensityIntervals[ c ][ x ][ y ] − 1, where numApplicableIntensityIntervals[ c ][ x ][ y ] is derived below.
Depending on the value of fgr_model_id, the selection of the one or more intensity intervals for the sample value Î[ c ][ x ][ y ] is specified as follows:
–	The variable numApplicableIntensityIntervals[ c ][ x ][ y ] is initially set equal to 0.
–	If fgr_model_id is equal to 0, the following applies:
· The top-left sample location ( xB, yB ) of the current 8x8 block b that contains the sample value Î[ c ][ x ][ y ] is derived as ( xB, yB ) = ( x / 8, y / 8 ).
· The average value bavg of the current 8x8 block b is derived as follows:
sum8x8 = 0
for( i = 0; i < 8; i++ )
	for( j = 0; j < 8; j++ )
		sum8x8  +=  Î[ c ][ xB * 8 + i ][yB * 8 + j ]	(23)
bavg = Clip3( 0, 255, ( sum8x8 + ( 1  <<  ( fgBitDepth[ c ] − 3 ) ) )  >>  ( fgBitDepth[ c ] − 2 ) )
· The value of intensityIntervalIdx[ c ][ x ][ y ][ j ] is derived as follows:
for( i = 0, j = 0; i  <=  fgr_num_intensity_intervals_minus1[ c ]; i++ )
	if( bavg  >=  fgr_intensity_interval_lower_bound[ c ][ i ]  &&
			bavg  <=  fgr_intensity_interval_upper_bound[ c ][ i ] ) {
		intensityIntervalIdx[ c ][ x ][ y ][ j ] = i		(24)
		j++
	}
numApplicableIntensityIntervals[ c ][ x ][ y ] = j
–	Otherwise (fgr_model_id is equal to 1), the value of intensityIntervalIdx[ c ][ x ][ y ][ j ] is derived as follows:
I8[ c ][ x ][ y ] = ( fgBitDepth[ c ]  = =  8 ) ? ( Î[ c ][ x ][ y ] :
		Clip3( 0, 255, ( Î[ c ][ x ][ y ] + ( 1  <<  ( fgBitDepth[ c ] − 9 ) ) )  >>  ( fgBitDepth[ c ] − 8 ) )
for( i = 0, j = 0; i  <=  fgr_num_intensity_intervals_minus1[ c ]; i++ )
	if( I8[ c ][ x ][ y ]  >=  fgr_intensity_interval_lower_bound[ c ][ i ]  &&	(25)
			I8[ c ][ x ][ y ]  <=  fgr_intensity_interval_upper_bound[ c ][ i ] ) {
		intensityIntervalIdx[ c ][ x ][ y ][ j ] = i
		j++
	}
numApplicableIntensityIntervals[ c ][ x ][ y ] = j
Samples that do not fall into any of the defined intervals (i.e., those samples for which the value of numApplicableIntensityIntervals[ c ][ x ][ y ] is equal to 0) are not modified by the grain generation function. Samples that fall into more than one interval (i.e., those samples for which the value of numApplicableIntensityIntervals[ c ][ x ][ y ] is greater than 1) will originate multi-generation grain. Multi-generation grain results from adding the grain computed independently for each of the applicable intensity intervals.
In the equations in the remainder of this clause, the variable sj in each instance of the list fgr_comp_model_value[ c ][ sj ] is the value of intensityIntervalIdx[ c ][ x ][ y ][ j ] derived for the sample value Î[ c ][ x ][ y ].
fgr_comp_model_value[ c ][ i ][ j ] specifies the j-th model value for the colour component c and the i-th intensity interval. The set of model values has different meaning depending on the value of fgr_model_id.
The value of fgr_comp_model_value[ c ][ i ][ j ] is constrained as follows, and could be additionally constrained as specified elsewhere in this clause:
–	If fgr_model_id is equal to 0, fgr_comp_model_value[ c ][ i ][ j ] shall be in the range of 0 to 2fgBitDepth[ c ] − 1, inclusive.
–	Otherwise (fgr_model_id is equal to 1), fgr_comp_model_value[ c ][ i ][ j ] shall be in the range of −2( fgBitDepth[ c ] − 1 ) to 2( fgBitDepth[ c ] − 1 ) − 1, inclusive.
Depending on the value of fgr_model_id, the synthesis of the film grain is modelled as follows:
–	If fgr_model_id is equal to 0, a frequency filtering model enables simulating the original film grain for c = 0..2, x = 0..PicWidthInLumaSamples − 1, and y = 0..PicHeightInLumaSamples − 1 as specified by:
[bookmark: Equation34]G[ c ][ x ][ y ] = ( fgr_comp_model_value[ c ][ sj ][ 0 ] * Q[ c ][ x ][ y ] + fgr_comp_model_value[ c ][ sj ][ 5 ] *
		G[ c − 1 ][ x ][ y ] )  >>  fgr_log2_scale_factor	(26)
	where Q[ c ] is a two-dimensional random process generated by filtering 16x16 blocks gaussRv with random-valued elements gaussRvij generated with a normalized Gaussian distribution (independent and identically distributed Gaussian random variable samples with zero mean and unity variance) and where the value of an element G[ c − 1 ][ x ][ y ] used in the right-hand side of the equation is inferred to be equal to 0 when c − 1 is less than 0.
NOTE 7 – A normalized Gaussian random variable can be generated from two independent, uniformly distributed random values over the interval from 0 to 1 (and not equal to 0), denoted as uRv0 and uRv1, using the Box-Muller transformation specified by:
gaussRvi,j = Sqrt( −2 * Ln( uRv0 ) ) * Cos( 2 * π * uRv1 )	(27)
where  is Archimedes' constant 3.141 592 653 589 793....
	The band-pass filtering of blocks gaussRv can be performed in the discrete cosine transform (DCT) domain as follows:
for( y = 0; y < 16; y++ )
	for( x = 0; x < 16; x++ )
		if( ( x < fgr_comp_model_value[ c ][ sj ][ 3 ]  &&  y < fgr_comp_model_value[ c ][ sj ][ 4 ] )  | |	(28)
				x > fgr_comp_model_value[ c ][ sj ][ 1 ]  | |  y > fgr_comp_model_value[ c ][ sj ][ 2 ] )
			gaussRv[ x ][ y ] = 0
filteredRv = IDCT16x16( gaussRv )
	where IDCT16x16( z ) refers to a unitary inverse discrete cosine transformation (IDCT) operating on a 16x16 matrix argument z as specified by:
IDCT16x16( z ) = r * z * rT		(29)
	where the superscript T indicates a matrix transposition and r is the 16x16 matrix with elements rij specified by:
		(30)
	where  is Archimedes' constant 3.141 592 653 589 793....
	Q[ c ] is formed by the frequency-filtered blocks filteredRv.
NOTE 8 – Coded model values are based on blocks of size 16x16, but a decoder implementation could use other block sizes. For example, decoders implementing the IDCT on 8x8 blocks could down-convert by a factor of two the set of coded model values fgr_comp_model_value[ c ][ sj ][ i ] for i equal to 1..4.
NOTE 9 – To reduce the degree of visible blocks that result from mosaicking the frequency-filtered blocks filteredRv, decoders could apply a low-pass filter to the boundaries between frequency-filtered blocks.
–	Otherwise (fgr_model_id is equal to 1), an auto-regression model enables simulating the original film grain for c = 0..2, x = 0..PicWidthInLumaSamples − 1, and y = 0..PicHeightInLumaSamples − 1 as specified by:
[bookmark: Equation39]G[ c ][ x ][ y ] = ( fgr_comp_model_value[ c ][ sj ][ 0 ] * n[ c ][ x][ y ] +
		fgr_comp_model_value[ c ][ sj ][ 1 ] * ( G[ c ][ x − 1 ][ y ] +
		( ( fgr_comp_model_value[ c ][ sj ][ 4 ] * G[ c ][ x ][ y − 1 ] )  >>
		fgr_log2_scale_factor ) ) + fgr_comp_model_value[ c ][ sj ][ 3 ] *
		( ( fgr_comp_model_value[ c ][ sj ][ 4 ] * ( G[ c ][ x − 1 ][ y − 1 ] + G[ c ][ x + 1 ][ y − 1 ] ) )  >>	(31)
		fgr_log2_scale_factor ) +
		fgr_comp_model_value[ c ][ sj ][ 5 ] * ( G[ c ][ x − 2 ][ y ] +
		( ( fgr_comp_model_value[ c ][ sj ][ 4 ] * fgr_comp_model_value[ c ][ sj ][ 4 ] * G[ c ][ x ][ y − 2 ] )  >>
		( 2 * fgr_log2_scale_factor ) ) ) +
		fgr_	comp_model_value[ c ][ sj ][ 2 ] * G[ c − 1 ][ x ][ y ] )  >>  fgr_log2_scale_factor
	where n[ c ][ x ][ y ] is a random value with normalized Gaussian distribution (independent and identically distributed Gaussian random variable samples with zero mean and unity variance for each value of c, x, and y) and where the value of an element G[ c ][ x ][ y ] used in the right-hand side of the equation is inferred to be equal to 0 when any of the following conditions are true:
–	c is less than 0,
–	x is less than 0,
–	y is less than 0.
fgr_comp_model_value[ c ][ i ][ 0 ] provides the first model value for the model as specified by fgr_model_id. fgr_comp_model_value[ c ][ i ][ 0 ] corresponds to the standard deviation of the Gaussian noise term in the generation functions specified in Equations 26 through 31.
fgr_comp_model_value[ c ][ i ][ 1 ] provides the second model value for the model as specified by fgr_model_id. When fgr_model_id is equal to 0, fgr_comp_model_value[ c ][ i ][ 1 ] shall be greater than or equal to 0 and less than 16.
When not present in the film grain extension SEI message, fgr_comp_model_value[ c ][ i ][ 1 ] is inferred as follows:
–	If fgr_model_id is equal to 0, fgr_comp_model_value[ c ][ i ][ 1 ] is inferred to be equal to 8.
–	Otherwise (fgr_model_id is equal to 1), fgr_comp_model_value[ c ][ i ][ 1 ] is inferred to be equal to 0.
fgr_comp_model_value[ c ][ i ][ 1 ] is interpreted as follows:
–	If fgr_model_id is equal to 0, fgr_comp_model_value[ c ][ i ][ 1 ] indicates the horizontal high cut frequency to be used to filter the DCT of a block of 16x16 random values.
–	Otherwise (fgr_model_id is equal to 1), fgr_comp_model_value[ c ][ i ][ 1 ] indicates the first order spatial correlation for neighbouring samples ( x − 1, y ) and ( x, y − 1 ).
fgr_comp_model_value[ c ][ i ][ 2 ] provides the third model value for the model as specified by fgr_model_id. When fgr_model_id is equal to 0, fgr_comp_model_value[ c ][ i ][ 2 ] shall be greater than or equal to 0 and less than 16.
When not present in the film grain extension SEI message, fgr_comp_model_value[ c ][ i ][ 2 ] is inferred as follows:
–	If fgr_model_id is equal to 0, fgr_comp_model_value[ c ][ i ][ 2 ] is inferred to be equal to fgr_comp_model_value[ c ][ i ][ 1 ]
–	Otherwise (fgr_model_id is equal to 1), fgr_comp_model_value[ c ][ i ][ 2 ] is inferred to be equal to 0.
fgr_comp_model_value[ c ][ i ][ 2 ] is interpreted as follows:
–	If fgr_model_id is equal to 0, fgr_comp_model_value[ c ][ i ][ 2 ] indicates the vertical high cut frequency to be used to filter the DCT of a block of 16x16 random values.
–	Otherwise (fgr_model_id is equal to 1), fgr_comp_model_value[ c ][ i ][ 2 ] indicates the colour correlation between consecutive colour components.
fgr_comp_model_value[ c ][ i ][ 3 ] provides the fourth model value for the model as specified by fgr_model_id. When fgr_model_id is equal to 0, fgr_comp_model_value[ c ][ i ][ 3 ] shall be greater than or equal to 0 and less than or equal to fgr_comp_model_value[ c ][ i ][ 1 ].
When not present in the film grain extension SEI message, fgr_comp_model_value[ c ][ i ][ 3 ] is inferred to be equal to 0.
fgr_comp_model_value[ c ][ i ][ 3 ] is interpreted as follows:
–	If fgr_model_id is equal to 0, fgr_comp_model_value[ c ][ i ][ 3 ] indicates the horizontal low cut frequency to be used to filter the DCT of a block of 16x16 random values.
–	Otherwise (fgr_model_id is equal to 1), fgr_comp_model_value[ c ][ i ][ 3 ] indicates the first order spatial correlation for neighbouring samples ( x − 1, y − 1 ) and ( x + 1, y − 1 ).
fgr_comp_model_value[ c ][ i ][ 4 ] provides the fifth model value for the model as specified by fgr_model_id. When fgr_model_id is equal to 0, fgr_comp_model_value[ c ][ i ][ 4 ] shall be greater than or equal to 0 and less than or equal to fgr_comp_model_value[ c ][ i ][ 2 ].
When not present in the film grain extension SEI message, fgr_comp_model_value[ c ][ i ][ 4 ] is inferred to be equal to fgr_model_id.
fgr_comp_model_value[ c ][ i ][ 4 ] is interpreted as follows:
–	If fgr_model_id is equal to 0, fgr_comp_model_value[ c ][ i ][ 4 ] indicates the vertical low cut frequency to be used to filter the DCT of a block of 16x16 random values.
–	Otherwise (fgr_model_id is equal to 1), fgr_comp_model_value[ c ][ i ][ 4 ] indicates the aspect ratio of the modelled grain.
fgr_comp_model_value[ c ][ i ][ 5 ] provides the sixth model value for the model as specified by fge_model_id.
When not present in the film grain extension SEI message, fge_comp_model_value[ c ][ i ][ 5 ] is inferred to be equal to 0.
fgr_comp_model_value[ c ][ i ][ 5 ] is interpreted as follows:
–	If fgr_model_id is equal to 0, fgr_comp_model_value[ c ][ i ][ 5 ] indicates the colour correlation between consecutive colour components.
–	Otherwise (fgr_model_id is equal to 1), fgr_comp_model_value[ c ][ i ][ 5 ] indicates the second order spatial correlation for neighbouring samples ( x, y − 2 ) and ( x − 2, y ).
fgr_region_based_adaptation_flag equal to 1 indicates that the spatial adaption of the film grain is defined per each region of the present SEI message and described by a rectangle.
fgr_active_regions_number indicates the number of regions for which the film grain adaptation is specified. fgr_active_regions_number shall be in the range of 0 to 255, inclusive.
fgr_region_top[ i ], fgr_region_left[ i ], fgr_region_width[ i ], and fgr_region_height[ i ] specify the coordinates of the top-left corner and the width and height, respectively, of the bounding box of the i-th region in the picture.
The value of fgr_region_left[ i ] shall be in the range of 0 to PicWidthInLumaSamples − 1, inclusive.
The value of fgr_region_top[ i ] shall be in the range of 0 to PicHeightInLumaSamples  − 1, inclusive.
The value of fgr_region_width[ i ] shall be in the range of 0 to PicWidthInLumaSamples  − fgr_region_left [ i ], inclusive.
The value of fgr_region_height[ i ] shall be in the range of 0 to PicHeightInLumaSamples  − fgr_region_top[ i ], inclusive.
fgr_film_grain_enabled_flag[ i ] equal to 1 indicates that the film grain characteristics using region intervals are applied on the i-th region. fge_film_grain_enabled_flag[ i ] equals to 0 indicates that no film grain synthesis is applied to the i-th region of the current picture.
fgr_region_interval_min[ i ][ c ] and fgr_region_interval_max[ i ][ c ] specify the range of interval indexes for color component c that are applicable to the i-th region. fgr_region_interval_min[ i ][ c ] shall be in the range of 0 to fg_num_intensity_intervals_minus1[ c ], inclusive, and fgr_region_interval_max[ i ][ c ] shall be in the range of fgr_region_interval_min[ i ][ c ] to fg_num_intensity_intervals_minus1[ c ], inclusive.
NOTE – Overlapping regions are processed in the increasing order of region index i, which means that a sample belonging to the region with index i=N with min and max film grain intervals indexes equal to x and y, respectively, and also belonging to region with index i=M (with M>N) with min and max film grain intervals indexes equal to x’ and y’, respectively, is processed with film grain characteristics defined with min and max film grain intervals indexes equal to x’ and y’.
fgr_alpha_channel_adaptation_flag equal to 1 indicates that the decoded alpha planes coded in auxiliary pictures of type AUX_ALPHA are applied to the simulated film grain values defined in the present SEI message prior to be applied are associated primary picture.
When an AU contains an SDI SEI message with sdi_aux_id[ i ] equal to 1 for at least one value of i, the SDI SEI message shall precede the FRGC SEI message in decoding order.
When an access unit contains an auxiliary picture picA in a layer, with nuh_layer_id equal to nuhLayerIdA, that is indicated as an alpha auxiliary layer by an SDI SEI message, the alpha channel sample values of picA persist in output order until one or more of the following conditions are true:
–	The next picture, in output order, with nuh_layer_id equal to nuhLayerIdA is output.
–	A CLVS containing the auxiliary picture picA ends.
–	The bitstream ends.
–	A CLVS of any associated primary layer of the auxiliary picture layer with nuh_layer_id equal to nuhLayerIdA ends.
If the current PU contains an SDI SEI message with sdi_aux_id[ i ] equal to 1 for at least one value of i, the simulated film grain values are weighted by the auxiliary data as follow:
–	If fgr_blending_mode_id is equal to 0, the blending mode is additive as specified by:
Igrain[ c ][ x ][ y ] = Clip3( 0, ( 1  <<  fgBitDepth[ c ] ) − 1, Î[ c ][ x ][ y ] + G[ c ][ x ][ y ]* Iaux[ c ][ x ][ y ])
–	Otherwise (fgr_blending_mode_id is equal to 1), the blending mode is multiplicative as specified by:
Igrain[ c ][ x ][ y ] = Clip3( 0, ( 1  <<  fgBitDepth[ c ] ) − 1, Î[ c ][ x ][ y ] +
			Round( ( Î[ c ][ x ][ y ] * G[ c ][ x ][ y ]* Iaux[ c ][ x ][ y ]) ) ÷ ( ( 1  <<  fgBitDepth[ c ] ) − 1 ) ) )
where Î[ c ][ x ][ y ] represents the sample value at coordinates x, y of the colour component c of the input image Î, G[ c ][ x ][ y ] is the simulated film grain value at the same position and colour component, and fgBitDepth[ c ], is the number of bits used for each sample in a fixed-length unsigned binary representation of the arrays Igrain[ c ][ x ][ y ], Î[ c ][ x ][ y ], and G[ c ][ x ][ y ], where c = 0..2, x = 0..PicWidthInLumaSamples − 1, and y = 0..PicHeightInLumaSamples – 1, and where Iaux[ c ][ x ][ y ] represents the sample value at coordinates x, y of the colour component c of the decoded auxiliary picture.
fgr_persistence_flag specifies the persistence of the film grain regions characteristics SEI message for the current layer.
fgr_persistence_flag equal to 0 specifies that the film grain regions characteristics SEI message applies to the current decoded picture only.
fgr_persistence_flag equal to 1 specifies that the film grain regions characteristics SEI message applies to the current decoded picture and persists for all subsequent pictures of the current layer in output order until one or more of the following conditions are true:
–	A new CLVS of the current layer begins.
–	The bitstream ends.
–	A picture in the current layer in an AU associated with a film grain regions characteristics SEI message is output that follows the current picture in output order.
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