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Abstract
This contribution report the crosscheck results of JVET-AH0117 (AHG12: Modification of chroma QP mapping table for ECM). The proposed method is tested based on ECM-12.0. Partial results indicate the BD-rate matches that in JVET-AH0117.
Simulation results
[bookmark: _Ref92718326]Table 1: Coding performance of ECM-12.0 with proposed configuration in JVET-AH0117 compared to VTM-11.0ecm12.0
	
	All Intra Main 10 

	
	Over 

	
	Y
	U
	V
	EncT
	DecT
	EncVmPeak
	DecVmPeak

	Class A1
	-12.73%
	-13.44%
	-24.20%
	
	
	
	

	Class A2
	-19.58%
	-21.41%
	-25.80%
	
	
	
	

	Class B
	-12.94%
	-19.29%
	-17.16%
	
	
	
	

	Class C
	-13.07%
	-9.64%
	-10.66%
	
	
	
	

	Class E
	-16.60%
	-19.31%
	-16.49%
	
	
	
	

	Overall 
	-14.65%
	-16.53%
	-18.22%
	
	
	
	

	Class D
	-11.07%
	-6.65%
	-7.16%
	
	
	
	

	Class F
	-28.49%
	-31.67%
	-31.91%
	
	
	
	

	Class TGM
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	Random Access Main 10

	
	Over 

	
	Y
	U
	V
	EncT
	DecT
	EncVmPeak
	DecVmPeak

	Class A1
	
	
	
	
	
	
	

	Class A2
	
	
	
	
	
	
	

	Class B
	
	
	
	
	
	
	

	Class C
	-24.49%
	-18.79%
	-19.20%
	
	
	
	

	Class E
	　
	
	　
	
	
	
	

	Overall
	
	
	
	
	
	
	

	Class D
	-25.24%
	-20.45%
	-20.80%
	
	
	
	

	Class F
	
	
	
	
	
	
	

	Class TGM
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	Low delay B Main 10 

	
	Over 

	
	Y
	U
	V
	EncT
	DecT
	EncVmPeak
	DecVmPeak

	Class A1
	　
	　
	　
	　
	　
	　
	　

	Class A2
	　
	
	　
	　
	
	　
	　

	Class B
	
	
	
	
	
	
	

	Class C
	
	
	
	
	
	
	

	Class E
	-18.15%
	-18.28%
	-16.24%
	
	
	
	

	Overall
	
	
	
	
	
	
	

	Class D
	-22.92%
	-19.07%
	-17.91%
	
	
	
	

	Class F
	
	
	
	
	
	
	

	Class TGM
	
	
	
	
	
	
	



Table 2: Coding performance of ECM-12.0 with proposed configuration in JVET-AH0117 compared to ECM-12.0

	
	All Intra Main 10 

	
	Over 

	
	Y
	U
	V
	EncT
	DecT
	EncVmPeak
	DecVmPeak

	Class A1
	-1.39%
	14.57%
	10.43%
	
	
	
	

	Class A2
	-2.16%
	14.27%
	13.17%
	
	
	
	

	Class B
	-0.87%
	13.92%
	14.03%
	
	
	
	

	Class C
	-1.01%
	10.89%
	11.01%
	
	
	
	

	Class E
	-0.72%
	11.08%
	11.09%
	
	
	
	

	Overall 
	-1.18%
	12.94%
	12.12%
	
	
	
	

	Class D
	-1.02%
	10.74%
	10.80%
	
	
	
	

	Class F
	-0.97%
	8.79%
	8.61%
	
	
	
	

	Class TGM
	[bookmark: _GoBack]
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	Random Access Main 10

	
	Over 

	
	Y
	U
	V
	EncT
	DecT
	EncVmPeak
	DecVmPeak

	Class A1
	
	
	
	
	
	
	

	Class A2
	
	
	
	
	
	
	

	Class B
	
	
	
	
	
	
	

	Class C
	-0.91%
	12.49%
	12.61%
	
	
	
	

	Class E
	　
	
	　
	
	
	
	

	Overall
	
	
	
	
	
	
	

	Class D
	-0.78%
	10.96%
	11.83%
	
	
	
	

	Class F
	
	
	
	
	
	
	

	Class TGM
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	Low delay B Main 10 

	
	Over 

	
	Y
	U
	V
	EncT
	DecT
	EncVmPeak
	DecVmPeak

	Class A1
	　
	　
	　
	　
	　
	　
	　

	Class A2
	　
	
	　
	
	
	
	

	Class B
	
	
	
	
	
	
	

	Class C
	
	
	
	
	
	
	

	Class E
	-0.36%
	21.83%
	21.13%
	
	
	
	

	Overall
	
	
	
	
	
	
	

	Class D
	-1.00%
	22.45%
	22.72%
	
	
	
	

	Class F
	
	
	
	
	
	
	

	Class TGM
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