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Abstract
This document contains draft text for several changes under consideration for future editions of the Coding-independent code points (CICP) Video specification (ISO/IEC 23091-2). The changes include support for the carriage and indication of depth and alpha map information in single-layer coded video bitstreams and extensions for the indication of chroma subsampling for formats beyond 4:2:0. 

[bookmark: _Hlk152255943]Changes that have been integrated:
The changes noted below correspond to aspects of JVET-AH0154 and JVET-AH0217. In particular, the following aspects are added:
· new values for the indication of depth and alpha map information in the colour primaries code point
· new values for the indication of monochromatic signals in the matrix coefficients code point.
· new code points and values for signalling chroma subsampling and sample location for formats beyond 4:2:0.
Changes to the specification text:
Additions to CICP subclause 8.1, Table 3 for supporting the direct indication of depth and alpha signals

8 Video code points
8.1	Colour primaries
Type: Unsigned integer, enumeration
Range: 0 to 255, inclusive
ColourPrimaries indicates whether the source picture has associated chromaticity coordinates, as represented by the HasChromaticityCoordinates variable, and if HasChromaticityCoordinates is equal to 1, ColourPrimaries indicates the chromaticity coordinates of the source colour primaries as specified in Table 3 in terms of the CIE 1931 definition of x and y, which shall be interpreted as specified by ISO/CIE 11664‑1. If HasChromaticityCoordinates is equal to 0, ColourPrimaries indicates the source picture type.  
NOTE 1	If ColourPrimaries is in the range of 128 to 130, additional information may be necessary to interpret the sample values. This additional information may be contained within the bitstream, within a systems layer, or provided via external means.
An 8-bit field should be adequate for representation of the ColourPrimaries code point.


Table 3 — Interpretation of colour primaries (ColourPrimaries) value
	Value
	Colour primaries
	HasChromaticityCoordinates
	Informative remarks

	0
	Reserved
	-
	For future use by ITU-T | ISO/IEC

	1
	primary
	x
	y
	1
	Rec. ITU-R BT.709-6
Rec. ITU-R BT.1361-0 conventional colour gamut system and extended colour gamut system
(historical)
IEC 61966-2-1 sRGB or sYCC
IEC 61966-2-4
SMPTE RP 177 (1993) Annex B

	
	green
	0.300
	0.600
	
	

	
	blue
	0.150
	0.060
	
	

	
	red
	0.640
	0.330
	
	

	
	white D65
	0.3127
	0.3290
	
	

	2
	Unspecified
	-
	Image characteristics are unknown or are
determined by the application.

	3
	Reserved
	-
	For future use by ITU-T | ISO/IEC

	4
	primary
	x
	y
	1
	Rec. ITU-R BT.470-6 System M (historical)
United States National Television System
Committee 1953 Recommendation for
transmission standards for colour television
United States Federal Communications
Commission Title 47 Code of Federal Regulations (2003) 73.682 (a) (20)

	
	green
	0.21
	0.71
	
	

	
	blue
	0.14
	0.08
	
	

	
	red
	0.67
	0.33
	
	

	
	white C
	0.310
	0.316
	
	

	5
	primary
	x
	y
	1
	Rec. ITU-R BT.470-6 System B, G (historical)
Rec. ITU-R BT.601-7 625
Rec. ITU-R BT.1358-0 625 (historical)
Rec. ITU-R BT.1700-0 625 PAL and 625 SECAM

	
	green
	0.29
	0.60
	
	

	
	blue
	0.15
	0.06
	
	

	
	red
	0.64
	0.33
	
	

	
	white D65
	0.3127
	0.3290
	
	

	6
	primary
	x
	y
	1
	Rec. ITU-R BT.601-7 525
Rec. ITU-R BT.1358-1 525 or 625 (historical)
Rec. ITU-R BT.1700-0 NTSC
SMPTE ST 170 (2004)
(functionally the same as the value 7)

	
	green
	0.310
	0.595
	
	

	
	blue
	0.155
	0.070
	
	

	
	red
	0.630
	0.340
	
	

	
	white D65
	0.3127
	0.3290
	
	

	7
	primary
	x
	y
	1
	SMPTE ST 240 (1999)
(functionally the same as the value 6)

	
	green
	0.310
	0.595
	
	

	
	blue
	0.155
	0.070
	
	

	
	red
	0.630
	0.340
	
	

	
	white D65
	0.3127
	0.3290
	
	

	8
	primary
	x
	y
	1
	Generic film (colour filters using Illuminant C)

	
	green
	0.243
	0.692 (Wratten 58)
	
	

	
	blue
	0.145
	0.049 (Wratten 47)
	
	

	
	red
	0.681
	0.319 (Wratten 25)
	
	

	
	white C
	0.310
	0.316
	
	

	9
	primary
	x
	y
	1
	Rec. ITU-R BT.2020-2
Rec. ITU-R BT.2100-2

	
	green
	0.170
	0.797
	
	

	
	blue
	0.131
	0.046
	
	

	
	red
	0.708
	0.292
	
	

	
	white D65
	0.3127
	0.3290
	
	

	10
	primary
	x
	y
	1
	SMPTE ST 428-1 (2019)
(CIE 1931 XYZ as in ISO/CIE 11664‑1)

	
	green (Y)
	0.0
	1.0
	
	

	
	blue (Z)
	0.0
	0.0
	
	

	
	red (X)
	1.0
	0.0
	
	

	
	centre white
	1 ÷ 3
	1 ÷ 3
	
	

	11
	primary
	x
	y
	1
	SMPTE RP 431-2 (2011)

	
	green
	0.265
	0.690
	
	

	
	blue
	0.150
	0.060
	
	

	
	red
	0.680
	0.320
	
	

	
	white
	0.314
	0.351
	
	

	12
	primary
	x
	y
	1
	SMPTE EG 432-1 (2010)

	
	green
	0.265
	0.690
	
	

	
	blue
	0.150
	0.060
	
	

	
	red
	0.680
	0.320
	
	

	
	white D65
	0.3127
	0.3290
	
	

	13 to 21
	Reserved
	-
	For future use by ITU-T | ISO/IEC

	22
	primary
	x
	y
	1
	No corresponding industry specification identified

	
	green
	0.295
	0.605
	
	

	
	blue
	0.155
	0.077
	
	

	
	red
	0.630
	0.340
	
	

	
	white D65
	0.3127
	0.3290
	
	

	23 to 127
	Reserved
	-
	For future use by ITU-T | ISO/IEC

	128
	Monochrome unspecified 
	0
	One colour component represents a purpose that is unknown or determined by the application.

	129
	Alpha channel
	0
	One colour component represents an alpha channel

	130
	Depth map
	0
	One colour component represents a depth map

	131 to 255
	Reserved
	-
	For future use by ITU-T | ISO/IEC



Modifications to CICP subclause 8.3, 

8.3 Matrix Coefficients

Type: Unsigned integer, enumeration
Range: 0 to 255, inclusive, plus associated flag
MatrixCoefficients describes the matrix coefficients used in deriving luma and chroma signals. If HasChromaticityCoordinates is equal to 1, the derivation is performed from the green, blue, and red, or X, Y, and Z primaries, as specified in Table 5 and the pseudocode logic expressions specified below. Otherwise (HasChromaticityCoordinates is equal to 0), the derivation is performed using a corresponding planar representation as specified in Table 5 and the pseudocode logic expressions specified below.
A flag, VideoFullRangeFlag, may be supplied with this code point (see below).
VideoFullRangeFlag specifies the scaling and offset values applied in association with the MatrixCoefficients. When not present or not specified, the value 0 for VideoFullRangeFlag would ordinarily be inferred as the default value for video imagery.
An 8-bit field should be adequate for representation of the MatrixCoefficients code point.
Certain values of MatrixCoefficients may be disallowed, depending on the application and the characteristics and format of the signal, e.g. with regard to combinations of the chroma format sampling structure and the values of BitDepthY, BitDepthC, and the value of HasChromaticityCoordinates.
The interpretation of MatrixCoefficients is specified by the following pseudocode logic. ER, EG, and EB are defined as "linear-domain" real-valued signals based on the indicated colour primaries (see 8.1) before applying the transfer characteristics (see 8.2).
When the source picture is associated with a ColourPrimaries value with HasChromaticityCoordinates equal to 0, then the values of ER, EG, and EB are set equal to P0, where P0 is the source plane associated with the source picture.
When the source picture is associated with a ColourPrimaries value with HasChromaticityCoordinates equal to 0,  values of MatrixCoefficients equal to 0, 1, 4 to 17, inclusive, and 21 to 23, inclusive, are not allowed.
For purposes of the YZX representation when MatrixCoefficients is equal to 0, the symbols R, G, and B are substituted for X, Y, and Z, respectively, in pseudocode operations (11) to (19), (27) to (29), and (33) to (35), and (48) to (50).
Nominal peak white is specified as having ER equal to 1, EG equal to 1, and EB equal to 1.
Nominal black is specified as having ER equal to 0, EG equal to 0, and EB equal to 0.s
The application of the transfer characteristics function is denoted by ( x )′ for an argument x.
–	If MatrixCoefficients is not equal to 14 or 15, the signals E′R, E′G and E′B are determined by application of the transfer characteristics function as in equations 11 to 13:

E′R = (ER)′								(11)
E′G = (EG)′								(12)
E′B = (EB)′								(13)
	 
	In this case, the range of E′R, E′G, and E′B is specified as follows:

	
	—
	If TransferCharacteristics is equal to 11 or 12, or TransferCharacteristics is equal to 13 and MatrixCoefficients is not equal to 0, E′R, E′G, and E′B are real numbers with values that have a larger range than the range of 0 to 1, inclusive, and their range is not specified in this document.

	
	—
	Otherwise, E′R, E′G, and E′B are real numbers in the range of 0 to 1, inclusive.

	—
	Otherwise (MatrixCoefficients is equal to 14 or 15), the signals E′L, E′M, and E′S are determined by the following ordered pseudocode steps:

	
	a)
	The "linear-domain" real-valued signals EL, EM, and ES are determined as follows:

	
	
	—
	If MatrixCoefficients is equal to 14, pseudocode operations (14) to (16) apply:


				EL = ( 1 688 * ER + 2 146 * EG + 262 * EB ) ÷ 4 096	(14)
				EM = ( 683 * ER + 2 951 * EG + 462 * EB ) ÷ 4 096	(15)
				ES = ( 99 * ER + 309 * EG + 3 688 * EB ) ÷ 4 096	(16)
	
	
	—
	Otherwise (MatrixCoefficients is equal to 15), pseudocode operations (17) to (19) apply:


								EL = ( 1 747 * ER + 2 169 * EG + 180 * EB ) ÷ 4 096	(17)
								EM = ( 673 * ER + 3 029 * EG + 394 * EB ) ÷ 4 096	(18)
								ES = ( 50 * ER + 207 * EG + 3 839 * EB ) ÷ 4 096	(19)
	
	b)
	The signals E′L, E′M, and E′S are determined by application of the transfer characteristics function as per pseudocode operations (20) to (22):


			E′L = (EL)′					(20)
			E′M = (EM)′					(21)
			E′S = (ES)′					(22)
When MatrixCoefficients is equal to 0, 8, 16, or 17, the variables BitDepthRGB and MaxValRGB are derived using the following ordered pseudocode steps:
	a)
	The variable BitDepthRGB is derived as follows:

	
	—
	If MatrixCoefficients is equal to 0 or 8, the following applies:


		BitDepthRGB = BitDepthY			(23)
	
	—
	Otherwise, if MatrixCoefficients is equal to 16, the following applies:


		BitDepthRGB = BitDepthY − 2		(24)
	
	—
	Otherwise (MatrixCoefficients is equal to 17), the following applies:


		BitDepthRGB = BitDepthY − 1		(25)
	b)
	The variable MaxValRGB is derived as follows:


MaxValRGB = ( 1 << BitDepthRGB ) − 1		(26)
The interpretation of MatrixCoefficients is specified as follows.
	—
	If VideoFullRangeFlag is equal to 0, the following applies:

	 
	—
	If MatrixCoefficients is equal to 0, 8, 16, or 17, pseudocode operations (25) to (27) apply:


R = Clip3( 0, MaxValRGB, ( 1 << ( BitDepthRGB − 8 ) ) * ( 219 * E′R + 16 ) )	(27)
G = Clip3( 0, MaxValRGB, ( 1 << ( BitDepthRGB − 8 ) ) * ( 219 * E′G + 16 ) )	(28)
B = Clip3( 0, MaxValRGB, ( 1 << ( BitDepthRGB − 8 ) ) * ( 219 * E′B + 16 ) )	(29)
NOTE 1	Pseudocode operations (27) to (29) are drafted under the assumption that BitDepthRGB is greater than or equal to 8.
	 
	—
	Otherwise, if MatrixCoefficients is equal to 1, 4, 5, 6, 7, 9, 10, 11, 12, 13, or 14, pseudocode operations (30) to (32) apply:


Y = Clip1Y ( Round( ( 1 << (BitDepthY − 8 ) ) * ( 219 * E′Y + 16 ) ) )	(30)
Cb = Clip1C ( Round( ( 1 << (BitDepthC − 8 ) ) * ( 224 * E′PB + 128 ) ) )	(31)
Cr = Clip1C ( Round( ( 1 << (BitDepthC − 8 ) ) * ( 224 * E′PR + 128 ) ) )	(32)
NOTE 2	Pseudocode operations (30) to (32) are drafted under the assumption that BitDepthY and BitDepthC are greater than or equal to 8.
	 
	—
	Otherwise, if MatrixCoefficients is equal to 2, the interpretation of the MatrixCoefficients code point is unknown or is determined by the application.

	 
	—
	Otherwise (MatrixCoefficients is not equal to 0, 1, 2, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 16, or 17), the interpretation of the MatrixCoefficients code point is reserved for future definition by ITU-T | ISO/IEC.

	—
	Otherwise (VideoFullRangeFlag is equal to 1), the following pseudocode logic applies:

	 
	—
	If MatrixCoefficients is equal to 0, 8, 16, or 17, pseudocode operations (33) to (35) apply:


R = Clip3( 0, MaxValRGB, MaxValRGB * E′R )	(33)
G = Clip3( 0, MaxValRGB, MaxValRGB * E′G )	(34)
B = Clip3( 0, MaxValRGB, MaxValRGB * E′B )	(35)
	 
	—
	Otherwise, if MatrixCoefficients is equal to 1, 4, 5, 6, 7, 9, 10, 11, 12, 13, or 14, pseudocode operations (36) to (38) apply:


Y = Clip1Y( Round( ( ( 1 << BitDepthY ) − 1 ) * E′Y ) )	(36)
Cb = Clip1C( Round( ( ( 1 << BitDepthC ) − 1 ) * E′PB + ( 1 << ( BitDepthC − 1 ) ) ) )	(37)
Cr = Clip1C( Round( ( ( 1 << BitDepthC ) − 1 ) * E′PR + ( 1 << ( BitDepthC − 1 ) ) ) )	(38)
	 
	—
	Otherwise, if MatrixCoefficients is equal to 2, the interpretation of the MatrixCoefficients code point is unknown or is determined by the application.

	 
	—
	Otherwise (MatrixCoefficients is not equal to 0, 1, 2, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, 16, or 17), the interpretation of the MatrixCoefficients code point is reserved for future definition by ITU-T | ISO/IEC.


When MatrixCoefficients is equal to 1, 4, 5, 6, 7, 9, 10, 11, 12, or 13, the constants KR and KB are specified as follows:
	—
	If MatrixCoefficients is not equal to 12 or 13, the constants KR and KB are specified in Table 5.

	—
	Otherwise (MatrixCoefficients is equal to 12 or 13), the constants KR and KB are computed as follows, using the chromaticity coordinates (xR, yR), (xG, yG), (xB, yB), and (xW, yW) specified by Table 3 for the ColourPrimaries code point for the red, green, blue, and white colour primaries, respectively:



	(39)

	(40)
	 
	where the values of zR, zG, zB, and zW, are given by pseudocode operations (41) to (44):


zR = 1 − ( xR + yR )						(41)
zG = 1 − ( xG + yG )						(42)
zB = 1 − ( xB + yB )						(43)
zW = 1 − ( xW + yW )						(44)
The variables E′Y, E′PB, and E′PR (for MatrixCoefficients not equal to 0, 8, 16, or 17) or Y, Cb, and Cr (for MatrixCoefficients equal to 0, 8, 16, or 17) are specified as follows.
	—
	If MatrixCoefficients is not equal to 0, 8, 10, 11, 13, 14, 15, 16, 17, or 23 pseudocode operations (45) to (47) apply:


E′Y = KR * E′R + ( 1− KR − KB ) * E′G + KB * E′B	(45)
E′PB = 0.5 * ( E′B − E′Y ) ÷ ( 1 − KB )		(46)
E′PR = 0.5 * ( E′R − E′Y ) ÷ ( 1 − KR )		(47)
	 
	E′Y is a real number with the value 0 associated with nominal black and the value 1 associated with nominal white. E′PB and E′PR are real numbers with the value 0 associated with both nominal black and nominal white. When TransferCharacteristics is not equal to 11 or 12, E′Y is a real number with values in the range of 0 to 1, inclusive. When TransferCharacteristics is not equal to 11 or 12, E′PB and E′PR are real numbers with values in the range of −0.5 to 0.5, inclusive. When TransferCharacteristics is equal to 11 (IEC 61966-2-4), or 12 (Rec. ITU R BT.1361-0 extended colour gamut system), E′Y, E′PB, and E′PR are real numbers with a larger range not specified in this document.

	—
	Otherwise, if MatrixCoefficients is equal to 0, pseudocode operations (48) to (50) apply:


Y = Round( G )							(48)
Cb = Round( B )							(49)
Cr = Round( R )							(50)
	—
	Otherwise, if MatrixCoefficients is equal to 8 and BitDepthC is equal to BitDepthY, pseudocode operations (51) to (53) apply:


Y = Round( 0.5 * G + 0.25 * ( R + B ) )		(51)
Cb = Round( 0.5 * G − 0.25 * ( R + B ) ) + (1 << ( BitDepthC − 1 ) )	(52)
Cr = Round( 0.5 * (R − B ) ) + (1 << ( BitDepthC − 1 ) )	(53)
NOTE 3	A problem has been reported with pseudocode operations (51) to (53), as it has been observed that the maximum value resulting from pseudocode operations (52) or (53) can be equal to ( 1 << BitDepthC ), which exceeds the intended range of values for Cb and Cr. A small modification of these pseudocode operations is likely to be introduced in a future version of this document to address the issue.
	 
	For purposes of the YCgCo nomenclature used in Table 5, Cb and Cr of pseudocode operations (52) and (53) may be referred to as Cg and Co, respectively. An appropriate inverse conversion for pseudocode operations (51) to (53) is given in pseudocode operations (54) to (57):


t = Y − ( Cb − ( 1 << ( BitDepthC − 1 ) ) )	(54)
G = Clip1Y( Y + ( Cb − ( 1 << ( BitDepthC − 1 ) ) ) )	(55)
B = Clip1Y( t − ( Cr − ( 1 << ( BitDepthC − 1 ) ) ) )	(56)
R = Clip1Y( t + ( Cr − ( 1 << ( BitDepthC − 1 ) ) ) )	(57)
	 
	—
	Otherwise, MatrixCoefficients is equal to 8, 16, or 17, pseudocode operations (58) to (61) apply:


Cr = Round( R ) − Round( B ) + (1 << ( BitDepthC − 1 ) )	(58)
t = Round( B ) + ( ( Cr − ( 1 << ( BitDepthC − 1 ) ) ) >> 1 )	(59)
Cb = Round( G ) − t + (1 << ( BitDepthC − 1 ) )	(60)
Y = t + ( ( Cb − ( 1 << ( BitDepthC − 1 ) ) ) >> 1 )	(61)
	 
	For purposes of the YCgCo nomenclature used in Table 5, Cb and Cr of pseudocode operations (60) and (58) may be referred to as Cg and Co, respectively. An appropriate inverse conversion for pseudocode operations (58) to (61) is given in pseudocode operations (62) to (65):


t = Y − ( ( Cb − ( 1 << ( BitDepthC − 1 ) ) ) >> 1 )	(62)
G = Clip3( 0, MaxValRGB, t + ( Cb − ( 1 << ( BitDepthC − 1 ) ) ) )	(63)
B = Clip3( 0, MaxValRGB, t − ( ( Cr − ( 1 << ( BitDepthC − 1 ) ) ) >> 1 ) )	(64)
R = Clip3( 0, MaxValRGB, B + ( Cr − ( 1 << ( BitDepthC − 1 ) ) ) )	(65)
	—
	Otherwise, if MatrixCoefficients is equal to 10 or 13, the signal E′Y is determined by application of the transfer characteristics function as given in pseudocode operations (66) and (67), and pseudocode operations (68) to (75) apply for specification of the signals E′PB and E′PR:


EY = KR * ER + ( 1 − KR − KB ) * EG + KB * EB	(66)
E′Y = ( EY )′								(67)
	 
	In this case, EY is defined from the "linear-domain" signals for ER, EG, and EB, prior to application of the transfer characteristics function, which is then applied to produce the signal E′Y. EY and E′Y are real values with the value 0 associated with nominal black and the value 1 associated with nominal white.


E′PB = ( E′B − E′Y ) ÷ ( 2 * NB ) for −NB <= E′B − E′Y <= 0	(68)
E′PB = ( E′B − E′Y ) ÷ ( 2 * PB ) for 0 < E′B − E′Y <= PB	(69)
E′PR = ( E′R − E′Y ) ÷ ( 2 * NR ) for −NR <= E′R − E′Y <= 0	(70)
E′PR = ( E′R − E′Y ) ÷ ( 2 * PR ) for 0 < E′R − E′Y <= PR	(71)
	 
	where the constants NB, PB, NR, and PR are determined by application of the transfer characteristics function to expressions involving the constants KB and KR as given in pseudocode operations (72) to (75):


NB = ( 1 − KB )′							(72)
PB = 1 − ( KB )′							(73)
NR = ( 1 − KR )′							(74)
PR = 1 − ( KR )′							(75)
	—
	Otherwise, if MatrixCoefficients is equal to 11, pseudocode operations (76) to (78) apply:


E′Y = E′G								(76)
E′PB = ( 0.986 566 * E′B − E′Y ) ÷ 2.0		(77)
E′PR = ( 0.991 902 * E′Y ) ÷ 2.0				(78)
	 
	In this case, for purposes of the Y′D′ZD′X nomenclature used in Table 5, E′PB may be referred to as D′Z and E′PR may be referred to as D′X.

	—
	Otherwise, if MatrixCoefficients is equal to 14 or 23, the following applies:

	 
	—
	If TransferCharacteristics is not equal to 18, pseudocode operations (79) to (81) apply:


E′Y = 0.5 * ( E′L + E′M )					(79)
E′PB = ( 6 610 * E′L − 13 613 * E′M + 7 003 * E′S ) ÷ 4 096	(80)
E′PR = ( 17 933 * E′L − 17 390 * E′M − 543 * E′S ) ÷ 4 096	(81)
	 
	—
	Otherwise, pseudocode operations (82) to (84) apply:


E′Y = 0.5 * ( E′L + E′M )					(82)
E′PB = ( 3 625 * E′L − 7 465 * E′M + 3 840 * E′S ) ÷ 4 096	(83)
E′PR = ( 9 500 * E′L − 9 212 * E′M − 288 * E′S ) ÷ 4 096	(84)
	
	In these cases, for purposes of the ICTCP nomenclature used in Table 5, E′Y, E′PB, and E′PR of pseudocode operations (79), (80), and (81) or pseudocode operations (82), (83), and (84) may be referred to as I, CT, and CP, respectively. pseudocode operations (79), (80), and (81) were designed specifically for use with TransferCharacteristics equal to 16 (PQ), and pseudocode operations (82), (83), and (84) were designed specifically for use with TransferCharacteristics equal to 18 (HLG).

	—
	Otherwise (MatrixCoefficients is equal to 15), pseudocode operations (85) to (87) apply:


E′Y = ( 1 638 * E′L + 1 638 * E′M + 820 * E′S ) ÷ 4 096	(85)
E′PB = ( 18 248 * E′L − 19 870 * E′M + 1 622 * E′S ) ÷ 4 096	(86)
E′PR = ( 3 300 * E′L + 1 463 * E′M − 4 763 * E′S ) ÷ 4 096	(87)
	 
	In this case, for purposes of the IPT nomenclature used in Table 5, E′Y, E′PB, and E′PR of pseudocode operations (85), (86), and (87) may be referred to as I, P, and T, respectively.


If MatrixCoefficients is in the range of 18 to 23, inclusive, equations 88 to 89 apply:
Cb = 1 << ( BitDepthC – 1)		(88)
Cr = 1 << ( BitDepthC – 1)		(89)
If MatrixCoefficients equal to 18, equation 90 applies:
Y = E′G			(90)
Otherwise if MatrixCoefficients equal to 19, equations 91 applies
Y = E′B			(91)
Otherwise if MatrixCoefficients equal to 20, equations 92 applies
Y = E′R			(92)

Additions to CICP subclause 8.3, Table 5 for supporting the direct indication of depth and alpha maps signals

Table 5 — Interpretation of the matrix coefficients (MatrixCoefficients) value
	Value
	Matrix coefficients
	Informative remarks

	0
	Identity
	The identity matrix.
Typically used for GBR (often referred to as RGB); however, may also be used for YZX (often referred to as XYZ);
IEC 61966-2-1 sRGB
SMPTE ST 428-1 (2019)
See equationsequations 48 to 50

	1
	KR = 0.2126; KB = 0.0722
	Rec. ITU-R BT.709-6
Rec. ITU-R BT.1361-0 conventional colour gamut system and extended colour gamut system (historical)
IEC 61966-2-4 xvYCC709
SMPTE RP 177 (1993) Annex B
See equations 45 to 47

	2
	Unspecified
	Image characteristics are unknown or are determined by the application

	3
	Reserved
	For future use by ITU-T | ISO/IEC

	4
	KR = 0.30; KB = 0.11
	United States Federal Communications Commission Title 47 Code of Federal Regulations (2003) 73.682 (a) (20)
See equations 45 to 47

	5
	KR = 0.299; KB = 0.114
	Rec. ITU-R BT.470-6 System B, G (historical)
Rec. ITU-R BT.601-7 625
Rec. ITU-R BT.1358-0 625 (historical)
Rec. ITU-R BT.1700-0 625 PAL and 625 SECAM
IEC 61966-2-1 sYCC
IEC 61966-2-4 xvYCC601
(functionally the same as the value 6)
See equations 45 to 47

	6
	KR = 0.299; KB = 0.114
	Rec. ITU-R BT.601-7 525
Rec. ITU-R BT.1358-1 525 or 625 (historical)
Rec. ITU-R BT.1700-0 NTSC
SMPTE ST 170 (2004)
(functionally the same as the value 5)
See equations 45 to 47

	7
	KR = 0.212; KB = 0.087
	SMPTE ST 240 (1999)
See equations 45 to 47

	8
	YCgCo or YCgCo-R
	See equations 51 to 57 for YCgCo (when BitDepthC is equal to BitDepthY)
See equations 58 to 65 for YCgCo-R (when BitDepthC is equal to BitDepthY + 1)

	9
	KR = 0.2627; KB = 0.0593
	Rec. ITU-R BT.2020-2 (non-constant luminance)
Rec. ITU-R BT.2100-2 Y′CbCr
See equations 45 to 47

	10
	KR = 0.2627; KB = 0.0593
	Rec. ITU-R BT.2020-2 (constant luminance)
See equations 66 to 75

	11
	Y′D′ZD′X
	SMPTE ST 2085 (2015)
See equations 76 to 78

	12
	See equations 39 to 44
	Chromaticity-derived non-constant luminance system
See equations 45 to 47

	13
	See equations 39 to 44
	Chromaticity-derived constant luminance system
See equations 66 to 75

	14
	ICTCP
	Rec. ITU-R BT.2100-2 ICTCP
See equations 79 to 81 for TransferCharacteristics value 16 (PQ)
See equations 82 to 84 for TransferCharacteristics value 18 (HLG)

	15
	IPT-C2
	SMPTE ST 2128 (2023)
See equations 85 to 87

	16
	YCgCo-Re
	See equations 58 to 65

	17
	YCgCo-Ro
	See equations 58 to 65

	[bookmark: _Hlk200545678]18
	1st colour component
	A monochromatic representation with only the first colour component in the original representation present in the coded image. Typically used for Green only; however, may also be used for the Y tristimulus value (luminance), when the colour primaries are set to XYΖ, or to indicate that the representation contains only the first component of an image not representing texture. See equations 88 to 90.

	[bookmark: _Hlk200545650]19
	2nd  colour component
	A monochromatic representation with only the second colour component in the original representation present in the coded image. Typically used for Blue only; however, may also be used for the Z tristimulus value, when the colour primaries are set to XYΖ, or to indicate that the representation contains only the second component of an image not representing texture. See equations 88, 89, and 91.

	20
	3rd  colour component
	A monochromatic representation with only the third colour component in the original representation present in the coded image. Typically used for Red only; however, may also be used for the X tristimulus value, when the colour primaries are set to XYΖ, or to indicate that the representation contains only the third component of an image not representing texture. See equations 88, 89, and 92.

	21
	Luma only
KR = 0.2126; KB = 0.0722
	A monochromatic representation of the luma component of the Rec. ITU‑R BT.709-6 representation. See equations 45 to 47, 88, and 89. 

	22
	Luma only
KR = 0.2627; KB = 0.0593
	A monochromatic representation of the luma component of the Rec. ITU‑R BT.2020-2 non-constant luminance representation. See equations 45 to 47, 88, and 89.

	23
	I only - ICTCP
	A monochromatic representation of the I component of ICTCP representation. See equation 75.

	24 to 255
	Reserved
	For future use by ITU-T | ISO/IEC



NOTE	In a previous edition of this document, the IEC 61966-2-1 sYCC representation was identified as corresponding to MatrixCoefficients equal to 1. Closer study later determined that this representation should correspond to MatrixCoefficients equal to 5 instead (which is functionally the same as the value 6). This document was therefore revised to correct the error.
Addition of new subclause 8.8 to CICP for signalling chroma subsampling and sample location beyond 4:2:0 formats.

8.8	Generic subsampling and sample location
8.8.1 	Generic subsampling type
Type: Unsigned integer, enumeration
Range: 0 to 15, inclusive
GenericSubsamplingType indicates the subsampling of a channel compared to a channel that has not been subsampled. It is specified explicitly or implicitly per channel in a frame. At least one channel in a frame shall have a GenericSubsamplingType value of 0.
Table 9 — Interpretation of generic subsampling type indicator (GenericSubsamplingType)

	Value
	Interpretation of GenericSubsamplingType

	0
	No subsampling

	1
	2x horizontal subsampling (4:2:2)

	2
	2x horizontal and vertical subsampling (4:2:0)

	3
	4x vertical subsampling (4:1:1)

	4
	2x vertical subsampling (4:4:0)

	5-14
	Reserved

	15
	Undefined



Table 9 describes the meaning of the GenericSubsamplingType values. As an example, 4:4:4 subsampled content would be described with GenericSubsamplingType as [0,0,0], 4:2:0 as [0,2,2] and 4:2:2 as [0,1,1].

8.8.2 	Generic subsampling sample location
Type: Unsigned integer, enumeration
Range: 0 to 15, inclusive
GenericSubsamplingSampleLocType indicates the sample alignment of a channel compared to a channel that has not been subsampled. It is specified per channel in a frame. It is assumed that at least one channel in a frame is not subsampled.
The meaning of GenericSubsamplingSampleLocType depends on the value of GenericSubsamplingType for the same channel. The relative spatial positioning of the sample compared to a channel that is not subsampled, can be expressed by defining two variables HorizontalOffset and VerticalOffset as a function of GenericSubsamplingSampleLocType as given by Table 10. HorizontalOffset is the horizontal (x) position of the centre of the top-left sample of the current channel relative to the centre of the top-left sample of a channel that is not subsampled in units of non-subsampled samples. VerticalOffset is the vertical (y) position of the centre of the top-left sample of the current channel relative to the centre of the top-left sample of a channel that is not subsampled in units of non-subsampled samples.
Table 10 — Interpretation of the value of GenericSubsamplingSampleLocType for 
different GenericSamplingType values in terms of [HorizontalOffset,VerticalOffset]
	
	GenericSubsamplingType

	Value
	0
	1
	2
	3
	4

	0
	(0.0, 0.0)
	(0.0, 0.0)
	(0.0, 0.5)
	(0.0, 0.0)
	(0.0, 0.5)

	1
	(0.0, 0.0)
	(0.5, 0.0)
	(0.5, 0.5)
	(0.25, 0.0)
	(0.0, 0.5)

	2
	(0.0, 0.0)
	(0.0, 0.0)
	(0.0, 0.0)
	(0.0, 0.0)
	(0.0, 0.0)

	3
	(0.0, 0.0)
	(0.5, 0.0)
	(0.5, 0.0)
	(0.25, 0.0)
	(0.0, 0.0)

	4
	(0.0, 0.0)
	(0.0, 0.0)
	(0.0, 1.0)
	(0.0, 0.0)
	(0.0, 1.0)

	5
	(0.0, 0.0)
	(0.5, 0.0)
	(0.5, 1.0)
	(0.25, 0.0)
	(0.0, 1.0)

	6-14
	Reserved
	Reserved
	Reserved
	Reserved
	Reserved

	15
	Undefined
	Undefined
	Undefined
	Undefined
	Undefined


Table 10 describes the meaning of the GenericSubsamplingSampleLocType values given the GenericSubsamplingType for the current channel. For the case of GenericSubsamplingType equal to 
2 (4:2:0), the values of GenericSubsamplingSampleLocType have the same meaning as Chroma420SampleLocType. The meaning for the other cases of GenericSubsamplingSampleLocType have the corresponding HorizontalOffset and VerticalOffset as for GenericSubsamplingType 2, where applicable.
If a channel has a GenericSubsamplingType of 0, the value of GenericSubsamplingSampleLocType for that channel is ignored.
Examples:
· GenericSubsamplingType [0,2,2] and GenericSubsamplingSampleLocType [2,1,1] corresponds to 4:2:0 subsampling with centre-centre chroma location (i.e. Chroma420SampleLocType 1).
· GenericSubsamplingType [0,3,3] and GenericSubsamplingSampleLocType [2,1,1] corresponds to 4:1:1 subsampling with centre chroma location.
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