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Abstract

This contribution reports the cross-checking results for JVET-F0036. The simulation results reportedly match those provided by the proponents.
1 Introduction

JVET-F0036 [1] proposed Rotated Sphere Projection (RSP) projection format. RSP partitions the sphere into two parts and packs them in the same way as CMP 3x2.
2 Experimental Results
The simulation was performed using HM-16.15-360Lib-2.1 with those changes proposed in JVET-F0036 [1] according to 360 video common test conditions [2]. The anchor is equirectangular projection coded with Main10 random access configuration using HM-16.15-360Lib-2.1 [3]. The results are summarized as follows, which match those provided by the proponents Error! Reference source not found.. More details can be found in the spreadsheet in the contribution. 
Table 1. F003636 vs HM ERP anchor 
	RSP
	SPSNR-NN-E2E
	SPSNR-I-E2E
	CPP-PSNR-E2E
	WS-PSNR-E2E

	
	Y
	U
	V
	Y
	U
	V
	Y
	U
	V
	Y
	U
	V

	Trolley
	-8.4%
	3.0%
	-1.9%
	-8.5%
	2.9%
	-2.0%
	-8.7%
	2.8%
	-2.2%
	-8.6%
	2.9%
	-2.1%

	GasLamp
	-4.0%
	3.4%
	8.0%
	-4.0%
	3.2%
	7.7%
	-4.3%
	3.0%
	7.6%
	-4.2%
	3.2%
	7.8%

	Skateboarding_in_lot
	-17.4%
	-15.3%
	-16.4%
	-17.5%
	-15.6%
	-16.6%
	-17.5%
	-15.6%
	-16.7%
	-17.4%
	-15.4%
	-16.5%

	Chairlift
	-23.5%
	-16.3%
	-16.7%
	-23.5%
	-16.4%
	-16.8%
	-23.7%
	-16.4%
	-16.9%
	-23.6%
	-16.4%
	-16.8%

	KiteFlite
	-9.5%
	-2.8%
	-3.7%
	-9.7%
	-2.9%
	-3.8%
	-9.6%
	-3.1%
	-3.9%
	-9.5%
	-3.0%
	-3.8%

	Harbor
	-8.4%
	-1.2%
	-1.0%
	-8.6%
	-1.4%
	-1.1%
	-9.1%
	-1.5%
	-1.2%
	-8.9%
	-1.4%
	-1.1%

	PoleVault
	-8.9%
	-9.4%
	-9.2%
	-8.4%
	-9.4%
	-9.2%
	-8.5%
	-9.4%
	-9.4%
	-8.9%
	-9.4%
	-9.2%

	AerialCity
	-1.8%
	1.9%
	0.9%
	-2.0%
	1.1%
	0.5%
	-1.9%
	1.0%
	0.3%
	-1.8%
	1.9%
	0.9%

	DrivingInCity
	-2.6%
	9.0%
	6.6%
	-1.9%
	8.2%
	6.1%
	-1.9%
	8.0%
	6.0%
	-2.6%
	9.1%
	6.6%

	DrivingInCountry
	-19.9%
	-16.7%
	-17.4%
	-19.2%
	-17.0%
	-17.5%
	-19.2%
	-17.1%
	-17.6%
	-19.9%
	-16.7%
	-17.3%

	Overall
	-10.5%
	-4.4%
	-5.1%
	-10.3%
	-4.7%
	-5.3%
	-10.4%
	-4.8%
	-5.4%
	-10.5%
	-4.5%
	-5.2%
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