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Abstract
This contribution reports the cross-checking results of the contribution JVET-L0194. It is reported that the results obtained during this cross-checking match the results described in JVET-L0194.
Introduction
In JVET-L0194 “CE4-related: On Merge Index coding”, the Merge index is coded as in VTM-1.0, i.e. only one CABAC context is used for the first bit, then the other bits are coded in CABAC bypass mode.

Simulation results
The cross-check test is performed on top of VTM-2.0.1. The results are shown in the following tables and match the results shown in JVET-L0194.

	
	Random Access Main 10

	
	Over VTM-2.0.1

	
	Y
	U
	V
	EncT
	DecT

	Class A1
	#VALUE!
	#VALUE!
	#VALUE!
	#NUM!
	#NUM!

	Class A2
	#VALUE!
	#VALUE!
	#VALUE!
	#NUM!
	#NUM!

	Class B
	0.03%
	-0.01%
	-0.09%
	99%
	96%

	Class C
	0.02%
	0.09%
	-0.03%
	99%
	93%

	Overall
	#VALUE!
	#VALUE!
	#VALUE!
	#NUM!
	#NUM!

	Class D
	0.02%
	0.06%
	-0.04%
	99%
	85%



	
	Low delay B Main10 

	
	Over VTM-2.0.1

	
	Y
	U
	V
	EncT
	DecT

	Class B
	0.01%
	-0.01%
	0.09%
	98%
	92%

	Class C
	0.02%
	-0.04%
	-0.06%
	99%
	95%

	Class E
	-0.21%
	0.37%
	0.03%
	99%
	94%

	Overall
	-0.04%
	0.08%
	0.03%
	99%
	94%

	Class D
	-0.04%
	0.17%
	0.08%
	100%
	92%
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