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Abstract
The contribution reports a crosscheck of JVET-M0421 (Non-CE1: Split-first signalling for partitioning). The crosscheck was carried out under the JVET common test condition. Experimental results match with those provided by the proponent.
In v2, results are updated.
1 Experimental result
The software on top of VTM-3.0 was provided by the proponents [1]. Crosscheck experiments were performed under JVET common test conditions.

Following tables show the results of the cross-check experiments under VTM-3.0 configuration.
Experimental results for Test #1
	
	All Intra Main10 

	
	Over VTM30-SHARP

	
	Y
	U
	V
	EncT
	DecT

	Class A1
	-0.04%
	-0.38%
	-0.24%
	108%
	97%

	Class A2
	-0.04%
	-0.13%
	-0.10%
	105%
	99%

	Class B
	-0.04%
	-0.28%
	-0.30%
	103%
	99%

	Class C
	-0.01%
	-0.36%
	-0.43%
	100%
	102%

	Class E
	-0.05%
	-0.69%
	-0.67%
	99%
	100%

	Overall 
	-0.03%
	-0.36%
	-0.35%
	103%
	100%

	SClass D
	0.02%
	-0.19%
	-0.36%
	100%
	104%

	Class F
	0.04%
	-0.22%
	-0.16%
	100%
	103%


	
	Random access Main10 

	
	Over VTM30-SHARP

	
	Y
	U
	V
	EncT
	DecT

	Class A1
	-0.03%
	-0.16%
	-0.22%
	103%
	100%

	Class A2
	-0.12%
	-0.11%
	-0.13%
	102%
	100%

	Class B
	-0.08%
	-0.17%
	-0.34%
	101%
	100%

	Class C
	-0.04%
	-0.38%
	-0.24%
	100%
	101%

	Class E
	　
	
	　
	　
	　

	Overall
	-0.07%
	-0.21%
	-0.25%
	101%
	100%

	Class D
	0.00%
	-0.62%
	-0.51%
	101%
	101%

	Class F
	-0.02%
	-0.09%
	-0.26%
	101%
	101%


	
	Low delay B Main10 

	
	Over VTM30-SHARP

	
	Y
	U
	V
	EncT
	DecT

	Class A1
	　
	　
	　
	　
	　

	Class A2
	　
	
	　
	　
	　

	Class B
	-0.08%
	-0.33%
	-0.52%
	102%
	101%

	Class C
	-0.04%
	0.06%
	0.00%
	101%
	101%

	Class E
	-0.05%
	0.43%
	-0.96%
	101%
	101%

	Overall
	-0.06%
	-0.01%
	-0.46%
	102%
	101%

	Class D
	0.00%
	-0.23%
	-0.21%
	101%
	102%

	Class F
	0.10%
	-0.43%
	-0.88%
	102%
	100%


2 Conclusion

It was confirmed that the simulation results of bitrate and PSNR match with those provided by the proponent.
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