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Abstract
This document reports the cross check results of “CE7-related: Context modeling of pred_mode_flag (JVET-M0513)”. The simulation was carried out under CTC. The partial results provided by the proponent were verified.
Cross Check Results
The simulation was carried out under the JVET common test condition [1]. The software was compiled with GCC version 7.3 and the AVX2 SIMD instructions. Huawei provided the source code of their proposal based on the VTM-3.0 software and results. The partial results are the same with those provided by the proponents.

Table 1. Test 1 results (LDP)
	
	Low delay P Main10 

	
	Over VTM-3.0

	
	Y
	U
	V
	EncT
	DecT

	Class A1
	　
	　
	　
	　
	　

	Class A2
	　
	
	　
	　
	　

	Class B
	#VALUE!
	#VALUE!
	#VALUE!
	#NUM!
	#NUM!

	Class C
	#VALUE!
	#VALUE!
	#VALUE!
	#NUM!
	#NUM!

	Class E
	#VALUE!
	#VALUE!
	#VALUE!
	#NUM!
	#NUM!

	Overall
	#VALUE!
	#VALUE!
	#VALUE!
	#NUM!
	#NUM!

	Class D
	#VALUE!
	#VALUE!
	#VALUE!
	#NUM!
	#NUM!

	Class F (optional)
	#VALUE!
	#VALUE!
	#VALUE!
	#NUM!
	#NUM!



Table 2. Test 2 results (RA, LDB and LDP)
	
	Random Access Main 10

	
	Over VTM-3.0

	
	Y
	U
	V
	EncT
	DecT

	Class A1
	#VALUE!
	#VALUE!
	#VALUE!
	#NUM!
	#NUM!

	Class A2
	#VALUE!
	#VALUE!
	#VALUE!
	#NUM!
	#NUM!

	Class B
	#VALUE!
	#VALUE!
	#VALUE!
	#NUM!
	#NUM!

	Class C
	-0.08%
	-0.01%
	0.12%
	99%
	100%

	Class E
	　
	
	　
	　
	　

	Overall
	#VALUE!
	#VALUE!
	#VALUE!
	#NUM!
	#NUM!

	Class D
	-0.02%
	-0.02%
	0.04%
	96%
	100%

	Class F (optional)
	#VALUE!
	#VALUE!
	#VALUE!
	#NUM!
	#NUM!

	
	
	
	
	
	

	
	Low delay B Main10 

	
	Over VTM-3.0

	
	Y
	U
	V
	EncT
	DecT

	Class A1
	　
	　
	　
	　
	　

	Class A2
	　
	
	　
	　
	　

	Class B
	#VALUE!
	#VALUE!
	#VALUE!
	#NUM!
	#NUM!

	Class C
	#VALUE!
	#VALUE!
	#VALUE!
	#NUM!
	#NUM!

	Class E
	#VALUE!
	#VALUE!
	#VALUE!
	#NUM!
	#NUM!

	Overall
	#VALUE!
	#VALUE!
	#VALUE!
	#NUM!
	#NUM!

	Class D
	#VALUE!
	#VALUE!
	#VALUE!
	#NUM!
	#NUM!

	Class F (optional)
	#VALUE!
	#VALUE!
	#VALUE!
	#NUM!
	#NUM!

	
	
	
	
	
	

	
	Low delay P Main10 

	
	Over VTM-3.0

	
	Y
	U
	V
	EncT
	DecT

	Class A1
	　
	　
	　
	　
	　

	Class A2
	　
	
	　
	　
	　

	Class B
	#VALUE!
	#VALUE!
	#VALUE!
	#NUM!
	#NUM!

	Class C
	#VALUE!
	#VALUE!
	#VALUE!
	#NUM!
	#NUM!

	Class E
	#VALUE!
	#VALUE!
	#VALUE!
	#NUM!
	#NUM!

	Overall
	#VALUE!
	#VALUE!
	#VALUE!
	#NUM!
	#NUM!

	Class D
	-0.01%
	-0.08%
	0.12%
	94%
	91%

	Class F (optional)
	#VALUE!
	#VALUE!
	#VALUE!
	#NUM!
	#NUM!



Table 3. Test 3 results (RA, LDB and LDP)
	
	Random Access Main 10

	
	Over VTM-3.0

	
	Y
	U
	V
	EncT
	DecT

	Class A1
	#VALUE!
	#VALUE!
	#VALUE!
	#NUM!
	#NUM!

	Class A2
	#VALUE!
	#VALUE!
	#VALUE!
	#NUM!
	#NUM!

	Class B
	#VALUE!
	#VALUE!
	#VALUE!
	#NUM!
	#NUM!

	Class C
	-0.04%
	0.15%
	0.12%
	97%
	97%

	Class E
	　
	
	　
	　
	　

	Overall
	#VALUE!
	#VALUE!
	#VALUE!
	#NUM!
	#NUM!

	Class D
	-0.06%
	-0.11%
	-0.01%
	98%
	99%

	Class F (optional)
	#VALUE!
	#VALUE!
	#VALUE!
	#NUM!
	#NUM!

	
	
	
	
	
	

	
	Low delay B Main10 

	
	Over VTM-3.0

	
	Y
	U
	V
	EncT
	DecT

	Class A1
	　
	　
	　
	　
	　

	Class A2
	　
	
	　
	　
	　

	Class B
	#VALUE!
	#VALUE!
	#VALUE!
	#NUM!
	#NUM!

	Class C
	#VALUE!
	#VALUE!
	#VALUE!
	#NUM!
	#NUM!

	Class E
	#VALUE!
	#VALUE!
	#VALUE!
	#NUM!
	#NUM!

	Overall
	#VALUE!
	#VALUE!
	#VALUE!
	#NUM!
	#NUM!

	Class D
	#VALUE!
	#VALUE!
	#VALUE!
	#NUM!
	#NUM!

	Class F (optional)
	#VALUE!
	#VALUE!
	#VALUE!
	#NUM!
	#NUM!

	
	
	
	
	
	

	
	Low delay P Main10 

	
	Over VTM-3.0

	
	Y
	U
	V
	EncT
	DecT

	Class A1
	　
	　
	　
	　
	　

	Class A2
	　
	
	　
	　
	　

	Class B
	#VALUE!
	#VALUE!
	#VALUE!
	#NUM!
	#NUM!

	Class C
	#VALUE!
	#VALUE!
	#VALUE!
	#NUM!
	#NUM!

	Class E
	#VALUE!
	#VALUE!
	#VALUE!
	#NUM!
	#NUM!

	Overall
	#VALUE!
	#VALUE!
	#VALUE!
	#NUM!
	#NUM!

	Class D
	0.02%
	-0.13%
	0.21%
	94%
	93%

	Class F (optional)
	#VALUE!
	#VALUE!
	#VALUE!
	#NUM!
	#NUM!



It should be noted that encoding and decoding times of the cross check results might be different from those provided by the proponent because the simulation was conducted in a different computing environment.
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