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Abstract
The cross checker reports that the source code provided by Technicolor who proposes JVET-N0304 has been carefully analysed and has been found to be consistent with the description in JVET-N0304. In JVET-N0304, are proposed. The cross checker could reproduce the results reported in JVET-N0304. The difference from measured encoder and decoder run time ratios to those reported in JVET-N0304 is acceptable.

Simulation Results
JVET-N0304 [1] has been implemented on VTM-4.0. The simulation was based on VTM configuration JVET-M1010 [2]. The PC cluster was used for the simulation, but since the same CPUs are allocated to the same parameters of the same sequences, the execution time is almost accurate. In order to measure more accurate decoding times, the decoder was re-run all the bitstreams on single CPU.
The results were consistent with the results of JVET-N0304. The difference from measured encoder and decoder run time ratios to those reported in JVET-N0304 is acceptable.

Table 1 Summary of experimental results (Combination LIC (CE1-5.4b) and bilateral filter)
	
	Random Access Main 10
	Low delay B Main10 

	
	Over VTM-4.0
	Over VTM-4.0

	
	Y
	U
	V
	EncT
	DecT
	Y
	U
	V
	EncT
	DecT

	Class A1
	-0.96%
	-0.51%
	-0.51%
	129%
	101%
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	Class A2
	-0.72%
	-0.47%
	-0.41%
	117%
	102%
	
	
	
	
	

	Class B
	-0.93%
	-0.47%
	-0.36%
	121%
	103%
	-1.14%
	-0.05%
	-0.02%
	128%
	104%

	Class C
	-0.68%
	-0.28%
	-0.40%
	126%
	103%
	-1.03%
	0.17%
	-0.18%
	134%
	106%

	Class E
	
	
	
	
	
	-0.34%
	0.57%
	0.34%
	103%
	103%

	Overall
	-0.82%
	-0.43%
	-0.41%
	123%
	102%
	-0.90%
	0.18%
	0.01%
	123%
	104%

	Class D
	-0.51%
	-0.04%
	-0.05%
	123%
	103%
	-0.71%
	0.84%
	0.32%
	129%
	106%

	Class F
	-1.09%
	-0.54%
	-0.65%
	114%
	102%
	-3.22%
	-2.70%
	-2.48%
	122%
	103%



Conclusion
In this contribution, the result of JVET-N0304 (combination LIC (CE1-5.4b) and bilateral filter) has been confirmed.
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