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Abstract
[bookmark: _GoBack]This document reports the crosscheck results of JVET-P0290 entitled “CE5-related: Clipping of intermediate value in CC-ALF”. The simulation was carried out under CTC. The results provided by the software author match the partial results obtained in this crosscheck.
Cross Check Results
The simulation was carried out under the JVET common test condition [1]. The software was compiled with GCC version 7.3 and the AVX2 SIMD instructions. Proponent provided the source code of their proposal based on the VTM-6.0 software and results. The results match with those provided by the proponent.

	
	 
	 
	All Intra Main10 
	 
	 

	
	 
	 
	Over VTM-6.0
	 
	 

	
	Y
	U
	V
	EncT
	DecT

	Class A1
	0.13%
	-3.49%
	-4.16%
	105%
	103%

	Class A2
	0.13%
	-8.65%
	-8.91%
	105%
	104%

	Class B
	0.10%
	-10.56%
	-8.57%
	102%
	106%

	Class C
	0.13%
	-4.17%
	-3.90%
	103%
	107%

	Class E
	0.19%
	-10.17%
	-3.44%
	104%
	109%

	Overall 
	0.13%
	-7.58%
	-6.00%
	103%
	106%

	Class D
	0.11%
	-2.74%
	-3.27%
	101%
	101%

	Class F
	0.18%
	-6.56%
	-6.63%
	102%
	106%

	
	
	
	
	
	

	
	 
	 
	Random access Main10 
	 
	 

	
	 
	 
	Over VTM-6.0
	 
	 

	
	Y
	U
	V
	EncT
	DecT

	Class A1
	#VALUE!
	#VALUE!
	#VALUE!
	#NUM!
	#NUM!

	Class A2
	#VALUE!
	#VALUE!
	#VALUE!
	#NUM!
	#NUM!

	Class B
	0.21%
	-17.64%
	-14.05%
	104%
	104%

	Class C
	0.09%
	-5.03%
	-4.29%
	104%
	108%

	Class E
	 
	
	 
	 
	 

	Overall
	#VALUE!
	#VALUE!
	#VALUE!
	#NUM!
	#NUM!

	Class D
	0.10%
	-4.46%
	-4.47%
	102%
	103%

	Class F
	0.19%
	-4.74%
	-4.61%
	103%
	105%

	
	
	
	
	
	

	
	 
	 
	Low delay B Main10 
	 
	 

	
	 
	 
	Over VTM-6.0
	 
	 

	
	Y
	U
	V
	EncT
	DecT

	Class A1
	 
	 
	 
	 
	 

	Class A2
	 
	
	 
	 
	 

	Class B
	#VALUE!
	#VALUE!
	#VALUE!
	#NUM!
	#NUM!

	Class C
	0.11%
	-8.25%
	-6.74%
	105%
	106%

	Class E
	0.22%
	-15.75%
	-6.29%
	107%
	108%

	Overall
	#VALUE!
	#VALUE!
	#VALUE!
	#NUM!
	#NUM!

	Class D
	0.19%
	-8.17%
	-6.00%
	102%
	100%

	Class F
	#VALUE!
	#VALUE!
	#VALUE!
	#NUM!
	#NUM!



The proponent also mentioned that GCC compilation might have an issue due to CE5-2.1 code under Linux such that the compiler produces an error message for array-bounds. GCC error checks were disabled with removing GCC's -Werror option in this crosscheck. This does not affect the results.
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