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Abstract
[bookmark: _GoBack]In this document, a crosscheck result of JVET- P0565 [1] is provided. The simulation results are provided when their proposed algirhthm, cross-component prediction in residual domain, is enabled.
It is reported that BD-rate changes of the crosschecked method are -0.88% / -1.03% / -0.93% for AI/RA/LDB in single tree case and -0.51% / -0.74% for RA/LDB in chroma separate tree case.
It is confirmed that the reported result of the proponent and the result from the cross-checker matches from each other.
Experiment result
	
	All Intra

	
	　Over VTM-6.0 DualITree=0 YUV444　
	Over VTM-6.0 DualITree=1 YUV444　

	
	Y
	U
	V
	EncT
	DecT
	Y
	U
	V
	EncT
	DecT

	TGM 1080p
	-1.69%
	-2.36%
	-2.09%
	101%
	101%
	
	
	
	
	

	TGM 720p
	-0.67%
	-1.41%
	-1.13%
	101%
	98%
	
	
	
	
	

	A
	-0.24%
	-2.20%
	-1.23%
	101%
	99%
	
	
	
	
	

	M
	-1.34%
	-3.33%
	-2.86%
	101%
	100%
	
	
	
	
	

	CC
	0.09%
	-1.49%
	-1.39%
	101%
	98%
	
	
	
	
	

	Overall 
	-0.88%
	-2.17%
	-1.74%
	101%
	99%
	
	
	
	
	

	
	　Random access　

	
	Over VTM-6.0 DualITree=0 YUV444　
	Over VTM-6.0 DualITree=1 YUV444　

	
	Y
	U
	V
	EncT
	DecT
	Y
	U
	V
	EncT
	DecT

	TGM 1080p
	-2.02%
	-3.19%
	-2.74%
	100%
	98%
	-1.25%
	-2.23%
	-2.06%
	100%
	102%

	TGM 720p
	-0.98%
	-1.97%
	-1.74%
	101%
	98%
	-0.55%
	-1.01%
	-0.99%
	100%
	100%

	A
	-0.65%
	-4.49%
	-2.48%
	100%
	100%
	-0.53%
	-3.33%
	-1.83%
	100%
	100%

	M
	-1.22%
	-3.66%
	-3.31%
	100%
	100%
	-0.17%
	-0.83%
	-0.76%
	100%
	101%

	CC
	0.59%
	-5.29%
	-4.56%
	99%
	100%
	0.57%
	-4.31%
	-3.60%
	99%
	101%

	Overall 
	-1.03%
	-3.48%
	-2.78%
	100%
	99%
	-0.51%
	-2.13%
	-1.70%
	100%
	101%

	
	　Low Delay B

	
	Over VTM-6.0 DualITree=0 YUV444
	Over VTM-6.0 DualITree=1 YUV444

	
	Y
	U
	V
	EncT
	DecT
	Y
	U
	V
	EncT
	DecT

	TGM 1080p
	-1.88%
	-3.00%
	-2.69%
	100%
	100%
	-1.89%
	-2.88%
	-2.70%
	98%
	95%

	TGM 720p
	-0.88%
	-2.60%
	-1.77%
	100%
	99%
	-0.50%
	-2.36%
	-1.65%
	99%
	101%

	A
	-0.74%
	-5.25%
	-2.17%
	101%
	98%
	-0.50%
	-4.71%
	-2.44%
	98%
	94%

	M
	-0.71%
	-3.80%
	-3.11%
	100%
	100%
	-0.43%
	-2.54%
	-1.57%
	99%
	98%

	CC
	0.29%
	-4.38%
	-10.44%
	100%
	99%
	0.31%
	-4.35%
	-10.31%
	98%
	96%

	Overall 
	-0.93%
	-3.64%
	-3.41%
	100%
	99%
	-0.74%
	-3.21%
	-3.13%
	98%
	97%
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