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Abstract
In this document, a crosscheck result of JVET- P0345 [1] is provided. The simulation results are provided when their proposed method, setting GOP as 8 for low delay B, is enabled.
It is reported that BD-rate changes of the crosschecked method are shown like below :
· Overall (Y/U/V) : -4.87% / -5.87% /-5.56%	
Also, we observe that there is 7% of complexity reduction at the encoder.
[bookmark: _GoBack]It is confirmed that the reported result of the proponent and the result from the cross-checker matches from each other.

Experiment result
	
	　
	　
	Low delay B Main10 
	　
	　

	
	　
	　
	Over VTM-6.0
	　
	　

	
	Y
	U
	V
	EncT
	DecT

	Class A1
	　
	　
	　
	　
	　

	Class A2
	　
	
	　
	　
	　

	Class B
	-3.61%
	-4.21%
	-4.44%
	93%
	97%

	Class C
	-5.58%
	-6.15%
	-5.49%
	94%
	101%

	Class E
	-6.04%
	-8.26%
	-7.54%
	91%
	102%

	Overall
	-4.87%
	-5.87%
	-5.56%
	93%
	100%

	Class D
	-3.10%
	-4.26%
	-4.03%
	95%
	100%

	Class F
	-4.61%
	-4.49%
	-3.66%
	95%
	100%
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