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Abstract
This contribution presents a crosscheck report of JVET-Q0526 (GEO support for 4xN and Nx4 CU) method 2. In method 2, allows 64 partition modes and limits GEO to CU smaller than 128. The experimental result of tester match with those provided by proponents.
Simulation Results
The software on top of VTM-7.0 was provided by the proponents.

	
	Random access

	
	Over CE4 common base (sharp)

	
	Y
	U
	V
	EncT
	DecT

	Class A1
	0.00%
	-0.06%
	-0.04%
	100%
	102%

	Class A2
	0.01%
	0.02%
	-0.08%
	100%
	101%

	Class B
	0.00%
	-0.03%
	0.00%
	101%
	101%

	Class C
	-0.08%
	-0.11%
	-0.20%
	101%
	101%

	Class E
	　
	
	　
	　
	　

	Overall 
	-0.02%
	-0.05%
	-0.08%
	101%
	101%

	Class D
	-0.10%
	-0.30%
	-0.17%
	101%
	101%

	Class F
	0.00%
	-0.12%
	-0.08%
	101%
	107%

	
	0.00%
	-0.06%
	-0.04%
	100%
	102%

	
	Random access 

	
	Over VTM-7.0 (sharp)

	
	Y
	U
	V
	EncT
	DecT

	Class A1
	-0.14%
	-0.16%
	-0.22%
	103%
	102%

	Class A2
	-0.20%
	-0.17%
	-0.10%
	103%
	101%

	Class B
	-0.15%
	-0.13%
	-0.18%
	103%
	101%

	Class C
	-0.67%
	-1.10%
	-1.10%
	103%
	100%

	Class E
	　
	
	　
	　
	　

	Overall
	-0.29%
	-0.40%
	-0.42%
	103%
	101%

	Class D
	-0.52%
	-0.97%
	-0.79%
	103%
	100%

	Class F
	-0.31%
	-0.50%
	-0.41%
	102%
	107%




	
	Low delay B

	
	Over CE4 common base (sharp)

	
	Y
	U
	V
	EncT
	DecT

	Class A1
	
	
	
	
	

	Class A2
	
	
	
	
	

	Class B
	0.08%
	0.07%
	0.30%
	100%
	101%

	Class C
	-0.09%
	-0.12%
	-0.30%
	100%
	101%

	Class E
	0.15%
	0.22%
	0.26%
	100%
	101%

	Overall 
	0.04%
	0.04%
	0.09%
	100%
	101%

	Class D
	-0.15%
	-0.38%
	0.01%
	100%
	100%

	Class F
	
	
	
	
	

	
	
	
	
	
	

	
	Low delay B

	
	Over VTM-7.0 (sharp)

	
	Y
	U
	V
	EncT
	DecT

	Class A1
	
	
	
	
	

	Class A2
	
	
	
	
	

	Class B
	-0.28%
	-0.43%
	-0.29%
	104%
	100%

	Class C
	-0.89%
	-1.37%
	-1.19%
	104%
	99%

	Class E
	-1.02%
	0.03%
	-0.63%
	101%
	100%

	Overall
	-0.67%
	-0.63%
	-0.68%
	103%
	100%

	Class D
	-0.83%
	-0.83%
	-1.03%
	103%
	99%

	Class F
	
	
	
	
	


Conclusion
In this contribution, the result of JVET-Q0526 method 2 has been confirmed.
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