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Abstract
Section A.4.3 of the VVC specification is informative and provides examples of the relationship between level, picture size, and maximum picture rate. Values for level 6.3 are provided in this document to support the disposition of a related ballot comment.
Introduction
Maximum pictures rates for level 6.3 are provided in the tables below. Moving values for levels 6.0, 6.1, and 6.2 into these new tables may be considered.
[bookmark: _Ref45178674]Table X – Maximum picture rates (pictures per second) at the Main tier, level 6.3 for some example picture sizes when MinCbSizeY is equal to 64
	Level:
	 
	 
	 
	6.3

	Max luma picture size (samples):
	 
	 
	 
	80 216 064

	Max luma sample rate (samples/sec)
	 
	 
	 
	4 812 963 840

	Format nickname
	Luma width
	Luma height
	Luma picture size
	 

	1080 HD
	1 920
	1 080
	2 088 960
	300.0

	2K×1K
	2 048
	1 024
	2 097 152
	300.0

	2K×1080
	2 048
	1 080
	2 228 224
	300.0

	4XGA
	2 048
	1 536
	3 145 728
	300.0

	16VGA
	2 560
	1 920
	4 915 200
	300.0

	3616×1536 (2.35:1)
	3 616
	1 536
	5 603 328
	300.0

	3672×1536 (2.39:1)
	3 680
	1 536
	5 701 632
	300.0

	3840×2160 (4*HD)
	3 840
	2 160
	8 355 840
	300.0

	4K×2K
	4 096
	2 048
	8 388 608
	300.0

	4096×2160
	4 096
	2 160
	8 912 896
	300.0

	4096×2304 (16:9)
	4 096
	2 304
	9 437 184
	300.0

	4096×3072
	4 096
	3 072
	12 582 912
	300.0

	7680×4320
	7 680
	4 320
	33 423 360
	144.0

	8192×4096
	8 192
	4 096
	33 554 432
	143.4

	8192×4320
	8 192
	4 320
	35 651 584
	135.0

	11520×6480
	11 520
	6 480
	74 649 600
	64.0

	12288×6144
	12 288
	6 144
	75 497 472
	63.7

	12288×6480
	12 288
	6 480
	79 626 240
	60.0



Table X – Maximum picture rates (pictures per second) at the High tier, level 6.3 for some example picture sizes when MinCbSizeY is equal to 64
	Level:
	 
	 
	 
	6.3

	Max luma picture size (samples):
	 
	 
	 
	80 216 064

	Max luma sample rate (samples/sec)
	 
	 
	 
	4 812 963 840

	Format nickname
	Luma width
	Luma height
	Luma picture size
	 

	1080 HD
	1 920
	1 080
	2 088 960
	960.0

	2K×1K
	2 048
	1 024
	2 097 152
	960.0

	2K×1080
	2 048
	1 080
	2 228 224
	960.0

	4XGA
	2 048
	1 536
	3 145 728
	960.0

	16VGA
	2 560
	1 920
	4 915 200
	960.0

	3616×1536 (2.35:1)
	3 616
	1 536
	5 603 328
	858.9

	3672×1536 (2.39:1)
	3 680
	1 536
	5 701 632
	844.1

	3840×2160 (4*HD)
	3 840
	2 160
	8 355 840
	576.0

	4K×2K
	4 096
	2 048
	8 388 608
	573.5

	4096×2160
	4 096
	2 160
	8 912 896
	540.0

	4096×2304 (16:9)
	4 096
	2 304
	9 437 184
	510.0

	4096×3072
	4 096
	3 072
	12 582 912
	382.5

	7680×4320
	7 680
	4 320
	33 423 360
	144.0

	8192×4096
	8 192
	4 096
	33 554 432
	143.4

	8192×4320
	8 192
	4 320
	35 651 584
	135.0

	11520×6480
	11 520
	6 480
	74 649 600
	64.0

	12288×6144
	12 288
	6 144
	75 497 472
	63.7

	12288×6480
	12 288
	6 480
	79 626 240
	60.0
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