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Abstract
This document reports on experiment EE2-1.11b on Combination of EE2 tests Test 1.8, Test 1.9 and Test 1.10.
Introduction
In test EE2-1.11b [1], combination of tests Test 1.8 [2], Test 1.9 [3] and Test 1.10 [4] is tested. These tests propose modifications to Decoder Side Intra mode Derivation (DIMD) and Template-based Intra Mode Derivation (TIMD).
Experimental results
The tables below summarize the coding efficiency and runtime impact of the proposed tests in ECM 7.0 using the JVET common test conditions. 


	
	All Intra Main10 

	
	Over ECM-7.0

	
	Y
	U
	V
	EncT
	DecT

	Class A1
	-0.22%
	-0.28%
	-0.27%
	109%
	105%

	Class A2
	-0.19%
	-0.10%
	-0.22%
	108%
	105%

	Class B
	-0.20%
	-0.16%
	-0.18%
	109%
	108%

	Class C
	-0.24%
	-0.19%
	-0.16%
	111%
	111%

	Class E
	-0.30%
	-0.28%
	-0.26%
	110%
	108%

	Overall 
	-0.23%
	-0.20%
	-0.21%
	110%
	107%

	Class D
	-0.23%
	-0.24%
	-0.17%
	110%
	110%

	Class F
	-0.16%
	0.20%
	0.05%
	109%
	105%

	
	
	
	
	
	

	
	Random Access Main 10

	
	Over ECM-7.0

	
	Y
	U
	V
	EncT
	DecT

	Class A1
	-0,15%
	-0,38%
	-0,12%
	102%
	102%

	Class A2
	-0,07%
	0,15%
	-0,11%
	101%
	102%

	Class B
	-0,11%
	-0,18%
	-0,33%
	102%
	102%

	Class C
	-0.11%
	-0.09%
	-0.12%
	103%
	103%

	Class E
	 
	
	 
	 
	 

	Overall
	-0,11%
	-0,13%
	-0,19%
	102%
	102%

	Class D
	-0.09%
	-0.26%
	0.12%
	102%
	104%

	Class F
	-0,16%
	-0,14%
	0,05%
	102%
	102%
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