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Abstract
This contribution reports the crosscheck results of JVET-AH0075 [1], which proposes a TIMD merge mode inheriting the TIMD modes from the previously TIMD coded blocks. Test 2.1a includes TIMD merge mode with one candidate, while Test 2.1b proposes TIMD merge mode with two candidates. The simulation results match with those provided in JVET-AH0075.
Experimental results
JVET-AH0075 was implemented on top of ECM-12.0. The simulations were conducted under the common test conditions of EE2 [2]. The crosscheck results for Test 2.1a and Test 2.1b are shown in Table 1 and Table 2 respectively.
[bookmark: _Ref457078802]Table 1. Results of Test #1
	
	All Intra Main 10

	
	Over ECM-12.0

	
	Y
	U
	V
	EncT
	DecT
	EncVmPeak
	DecVmPeak

	Class A1
	-0.07%
	-0.06%
	0.11%
	103.8%
	101.4%
	100.3%
	100.4%

	Class A2
	-0.10%
	-0.01%
	-0.04%
	101.5%
	102.1%
	100.0%
	100.5%

	Class B
	-0.09%
	0.02%
	-0.01%
	103.5%
	101.5%
	102.2%
	100.4%

	Class C
	-0.06%
	-0.02%
	0.09%
	102.7%
	101.9%
	102.3%
	100.2%

	Class E
	-0.04%
	0.06%
	0.12%
	103.5%
	100.8%
	100.3%
	100.1%

	Overall
	-0.07%
	0.00%
	0.05%
	103.0%
	101.5%
	101.2%
	100.3%

	Class D
	-0.08%
	0.03%
	0.14%
	103.6%
	101.0%
	100.4%
	100.1%

	Class F
	-0.04%
	0.16%
	-0.01%
	109.2%
	100.4%
	99.9%
	100.3%

	Class TGM
	0.00%
	0.02%
	-0.14%
	107.4%
	102.0%
	102.8%
	100.5%

	
	Random Access Main 10

	
	Over ECM-12.0

	
	Y
	U
	V
	EncT
	DecT
	EncVmPeak
	DecVmPeak

	Class A1
	
	
	
	
	
	
	

	Class A2
	
	
	
	
	
	
	

	Class B
	-0.05%
	0.10%
	-0.04%
	100.7%
	99.6%
	100.2%
	100.3%

	Class C
	-0.02%
	0.01%
	-0.03%
	100.2%
	100.3%
	100.3%
	100.2%

	Class E
	
	
	
	
	
	
	

	Overall
	
	
	
	
	
	
	

	Class D
	0.01%
	-0.44%
	0.36%
	100.9%
	100.2%
	100.8%
	100.1%

	Class F
	0.03%
	0.08%
	-0.06%
	103.2%
	100.9%
	100.1%
	100.6%

	Class TGM
	0.11%
	0.13%
	0.08%
	102.1%
	99.3%
	100.1%
	100.1%


[bookmark: _Ref164070870]Table 2. Results of Test #2
	
	All Intra Main 10

	
	Over ECM-12.0

	
	Y
	U
	V
	EncT
	DecT
	EncVmPeak
	DecVmPeak

	Class A1
	-0.10%
	-0.06%
	0.15%
	102.8%
	102.1%
	100.7%
	100.5%

	Class A2
	-0.13%
	0.06%
	0.00%
	103.1%
	103.1%
	100.2%
	100.5%

	Class B
	-0.12%
	0.05%
	-0.02%
	104.0%
	102.8%
	104.5%
	100.3%

	Class C
	-0.09%
	0.02%
	0.03%
	103.4%
	104.4%
	102.3%
	100.2%

	Class E
	-0.07%
	0.00%
	-0.06%
	103.9%
	102.5%
	100.3%
	100.2%

	Overall
	-0.10%
	0.02%
	0.02%
	103.5%
	103.0%
	101.9%
	100.3%

	Class D
	-0.11%
	0.06%
	0.03%
	103.7%
	103.3%
	100.4%
	100.1%

	Class F
	-0.03%
	0.09%
	0.07%
	101.5%
	101.8%
	99.4%
	100.2%

	Class TGM
	0.00%
	0.06%
	-0.10%
	102.2%
	102.3%
	100.3%
	100.4%

	
	Random Access Main 10

	
	Over ECM-12.0

	
	Y
	U
	V
	EncT
	DecT
	EncVmPeak
	DecVmPeak

	Class A1
	
	
	
	
	
	
	

	Class A2
	
	
	
	
	
	
	

	Class B
	-0.06%
	-0.13%
	-0.18%
	100.2%
	98.8%
	100.2%
	100.3%

	Class C
	-0.03%
	0.01%
	0.11%
	100.5%
	99.5%
	100.3%
	100.2%

	Class E
	
	
	
	
	
	
	

	Overall
	
	
	
	
	
	
	

	Class D
	0.00%
	-0.01%
	0.27%
	101.0%
	99.3%
	100.4%
	100.1%

	Class F
	0.01%
	0.00%
	-0.01%
	100.8%
	100.6%
	100.3%
	100.4%

	Class TGM
	-0.03%
	0.00%
	0.03%
	101.0%
	99.0%
	100.3%
	100.3%
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