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Abstract
This document reports the outcome of the informal viewing of JVET-AM0078 [1]. The viewing was made as an A-B test on the two lowest bitrate points of AHG 17 test content classes that use random access configuration. The viewing indicates a clear preference for JVET-AM0045 [2] rather than JVET-AM0078 which also include JVET-AM0045.
Test setup
The viewing was performed by 7 participants in the viewing room 211. The viewing follows an A-B test procedure where the viewers are not informed about the origin of A and B and just vote which version looks better.
[bookmark: _Hlk202365234]The viewing was split into 2 sessions, one UHD and a HD session, by running the two lowest bitrate points of each sequence in a sequential order. Both sessions where build with JVET-AM0045 as A, and JVET-AM0078 as B.
[bookmark: _Hlk202363775][bookmark: _Hlk202365110][bookmark: _Hlk202365140]The test content was compressed video by VTM-23.9 [3] using JVET-AM0045 or JVET-AM0078 following the random access categories of JVET-AL2026 [4].
Results
[bookmark: _Hlk202365897][bookmark: _Hlk202365742]The following raw results were obtained (no outlier rejection or other processing was performed):
[bookmark: _Hlk202365782]Session 1 UHD:
Votes A = AM0045:	104
Votes B = AM0078:	55
Session 2 HD:
Votes A = AM0045:	90
Votes B = AM0078:	44
[bookmark: _Hlk202365689][bookmark: _Hlk202365597]Summarized Votes for AM0045:	194
Summarized Votes for AM0078:	99
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Annex A: Table with votes per volunteer 
	
	C2
	A1
	A2
	A3
	D1
	D2
	D3
	
	

	UHD
	V1
	V2
	V3
	V4
	V5
	V6
	V7
	#VOTES A
	#VOTES B

	HRC1
	A
	B
	A
	B
	A
	A
	A
	5
	2

	HRC1
	A
	A
	B
	B
	A
	A
	B
	4
	3

	HRC2
	A
	A
	A
	A
	A
	A
	A
	7
	0

	HRC2
	A
	A
	A
	-
	B
	A
	A
	5
	1

	HRC3
	A
	A
	B
	B
	A
	A
	A
	5
	2

	HRC3
	B
	A
	B
	-
	A
	B
	A
	3
	3

	HRC4
	A
	A
	A
	-
	A
	A
	B
	5
	1

	HRC4
	A
	A
	A
	-
	B
	B
	B
	3
	3

	HRU1
	A
	A
	A
	-
	A
	A
	A
	6
	0

	HRU1
	A
	B
	B
	B
	A
	A
	A
	4
	3

	HRU2
	A
	B
	A
	A
	A
	A
	A
	6
	1

	HRU2
	A
	A
	B
	A
	A
	A
	B
	5
	2

	HRU3
	A
	B
	B
	A
	B
	B
	A
	3
	4

	HRU3
	A
	A
	A
	B
	B
	B
	B
	3
	4

	HRU4
	A
	B
	A
	A
	A
	A
	B
	5
	2

	HRU4
	A
	B
	B
	-
	A
	A
	A
	4
	2

	SRU1
	A
	A
	A
	B
	A
	A
	B
	5
	2

	SRU1
	A
	B
	B
	B
	B
	B
	B
	1
	6

	SRU2
	A
	A
	A
	-
	A
	A
	A
	6
	0

	SRU2
	A
	B
	B
	A
	B
	B
	A
	3
	4

	SRU3
	A
	A
	A
	-
	A
	A
	A
	6
	0

	SRU3
	B
	A
	B
	-
	B
	B
	A
	2
	4

	SRU4
	A
	B
	A
	A
	A
	A
	A
	6
	1

	SRU4
	B
	A
	A
	B
	B
	B
	B
	2
	5

	
	
	
	
	
	
	
	UHD 
	104
	55

	HD
	V1
	V2
	V3
	V4
	V5
	V6
	V7
	#VOTES A #VOTES B

	SRH1
	B
	A
	A
	A
	A
	A
	B
	5
	2

	SRH1
	A
	A
	A
	-
	A
	B
	B
	4
	2

	SRH2
	A
	A
	A
	B
	A
	A
	A
	6
	1

	SRH2
	B
	B
	A
	-
	A
	B
	A
	3
	3

	SRH3
	A
	B
	A
	-
	A
	B
	A
	4
	2

	SRH3
	B
	A
	B
	B
	B
	A
	A
	3
	4

	SRH4
	A
	A
	A
	A
	B
	A
	A
	6
	1

	SRH4
	A
	A
	A
	-
	B
	B
	B
	3
	3

	URH1
	A
	B
	A
	A
	B
	A
	B
	4
	3

	URH1
	A
	A
	B
	A
	B
	B
	A
	4
	3

	URH2
	A
	A
	A
	A
	A
	A
	A
	7
	0

	URH2
	A
	A
	B
	B
	B
	A
	B
	3
	4

	URH3
	A
	A
	A
	-
	A
	A
	A
	6
	0

	URH3
	A
	B
	B
	B
	A
	A
	A
	4
	3

	URH4
	A
	A
	A
	B
	A
	A
	A
	6
	1

	URH4
	B
	A
	B
	A
	A
	A
	B
	4
	3

	URH5
	A
	B
	A
	A
	B
	A
	B
	4
	3

	URH5
	A
	A
	B
	A
	B
	B
	B
	3
	4

	URH5
	A
	B
	A
	A
	A
	A
	A
	6
	1

	URH6
	A
	B
	A
	 -
	A
	A
	A
	5
	1

	
	
	
	
	
	
	
	HD
	90
	44

	
	
	
	
	
	
	
	Total
	194
	99
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