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Abstract
This proposal JVET-Q0380 proposed two methods on block size restriction. The BD-rate performance of the proposed two methods matches with crosscheck result in all point.  
Introduction
The first method proposes to apply LFNST only for blocks where either height or width are greater than or equal to 16 or (maximum (height, width) greater than or equal to 32 && minimum(height, width) greater than or equal to 4). The second method proposes to apply LFNST only for blocks where either height or width both are greater than or equal to 16 or (H>=4 && W>=64) and vice-versa or (H>=8 && W>=32) and vice versa.
Simulation results
Method 1:
	
	Over VTM-7 AI

	
	Y
	U
	V
	EncT
	DecT

	Class A1
	-0.01%
	-0.14%
	0.11%
	100%
	101%

	Class A2
	0.01%
	0.00%
	-0.07%
	101%
	101%

	Class B
	0.01%
	-0.01%
	-0.05%
	102%
	103%

	Class C
	0.00%
	-0.03%
	0.01%
	101%
	103%

	Class E
	0.00%
	-0.01%
	0.10%
	101%
	101%

	Overall 
	0.00%
	-0.03%
	0.01%
	101%
	102%

	Class D
	0.00%
	-0.05%
	0.17%
	101%
	104%

	Class F
	-0.02%
	0.03%
	0.10%
	101%
	103%



	
	Over VTM-7 RA

	
	Y
	U
	V
	EncT
	DecT

	Class A1
	0.00%
	-0.05%
	0.09%
	101%
	99%

	Class A2
	-0.03%
	-0.10%
	0.00%
	101%
	99%

	Class B
	-0.01%
	-0.01%
	0.05%
	101%
	102%

	Class C
	0.01%
	-0.18%
	-0.10%
	101%
	101%

	Class E
	 
	
	 
	 
	

	Overall
	0.00%
	-0.08%
	0.01%
	101%
	101%

	Class D
	-0.01%
	-0.19%
	-0.16%
	101%
	102%

	Class F
	0.02%
	0.00%
	-0.02%
	101%
	101%


Method 2:
	
	Over VTM-7 AI

	
	Y
	U
	V
	EncT
	DecT

	Class A1
	-0.01%
	-0.11%
	0.09%
	102%
	101%

	Class A2
	-0.01%
	0.03%
	-0.06%
	101%
	101%

	Class B
	0.00%
	-0.03%
	-0.10%
	101%
	102%

	Class C
	0.00%
	0.00%
	-0.07%
	101%
	102%

	Class E
	0.01%
	-0.08%
	0.09%
	101%
	102%

	Overall 
	0.00%
	-0.03%
	-0.02%
	101%
	101%

	Class D
	0.01%
	-0.03%
	0.07%
	101%
	106%

	Class F
	-0.01%
	-0.01%
	0.03%
	101%
	102%



	
	[bookmark: _GoBack]Over VTM-7 RA

	
	Y
	U
	V
	EncT
	DecT

	Class A1
	0.00%
	-0.01%
	-0.07%
	101%
	99%

	Class A2
	-0.02%
	0.07%
	0.00%
	101%
	99%

	Class B
	0.01%
	0.06%
	0.11%
	101%
	102%

	Class C
	0.03%
	-0.08%
	0.05%
	101%
	102%

	Class E
	 
	
	 
	 
	

	Overall
	0.01%
	0.01%
	0.03%
	101%
	101%

	Class D
	-0.01%
	-0.05%
	-0.09%
	101%
	102%

	Class F
	0.00%
	-0.04%
	-0.03%
	101%
	102%




Conclusion
The BD-rate performance of the proposed two methods matches with crosscheck result in all point. 
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