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Abstract
This contribution reports the cross-check results of the JVET-Q0110 (On Intra Prediction Mode and Chroma BDPCM) [1], which proposes two bug fixes: 
- aspect1: follow JVET-O0315’s intra mode derivation for BDPCM (align SW to WD).
- aspect2: align BDPCM context assignments in SW to WD.
The source code provided by the proponent was carefully analyzed and found to be consistent with the description in JVET-Q0110. 
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